{"text_format":"2","workbook":"xlsx","n_sheets":2,"sheets":["Orçamento","Planilha1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":6,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Orçamento","index":0,"n_rows":520,"n_cols":13,"rows_kept":520,"cut":false,"hidden":false,"merged":[[1,4,1,11],[2,4,2,11],[3,4,3,11],[6,1,6,11],[4,2,4,7],[5,2,5,7]]}
[]
[{"$nulls":4},"Ministério da Integração e do Desenvolvimento Regional"]
[{"$nulls":4},"Companhia de Desenvolvimento dos Vales do São Francisco e do Parnaíba"]
[{"$nulls":4},"Área de Desenvolvimento e Infraestrutura"]
[null,"OBRA:","OBRAS E SERVIÇOS REMANESCENTES PARA CONSTRUÇÃO DE CENTRO COMERCIAL",{"$nulls":5},"PRAZO:",10,"BDI-SERVIÇO %:",21.9]
[null,"LOCAL:","MUNICÍPIO DE SANTANA, NO ESTADO DO AMAPÁ",{"$nulls":5},"DATA BASE:","SETEMBRO/2024","BDI-FORN. %:",14.41]
[null,"PLANILHA DE ORÇAMENTAÇÃO"]
[null,"ITEM","CÓDIGO","FONTE","DISCRIMINAÇÃO","TIPO","UNID.","QUANT.","VR.UNIT.S/BDI","PR. UNIT.C/BDI","C. TOT.S/BDI","P. TOT.C/BDI"]
[null,1,null,null,"ADMINISTRAÇÃO DA OBRA",{"$nulls":4},{"$f":"IF(F9<>\"\",\nTRUNC(IF(F9=\"SERV\",I9*(1+$L$5/100),I9*(1+$L$6/100)),2),\n\"\" )","v":""},{"$f":"IF( $G9 <> \"\",\nTRUNC( $H9 * $I9, 2 ),\nSUMIFS( $K10:$K$520,\n          $B10:$B$520, $B9 & \".*\",\n          $B10:$B$520, \"<>\" & $B9 & \".*.*\"\n) )","v":0},{"$f":"IF( $G9 <> \"\",\n     TRUNC( $H9 * $J9, 2 ),\n     SUMIFS( $L10:$L$520,\n              $B10:$B$520, $B9 & \".*\",\n              $B10:$B$520, \"<>\" & $B9 & \".*.*\"\n     ) )","v":0},{"$f":"IF( $G38 <> \"\",\nTRUNC( $H38 * $J38, 2 ),\nSUMIFS( $L39:$L$520, $B39:$B$520, $B38 & \".*\", $F39:$F$520, \"<>\", $B39:$B$520, \"=\" & COUNT($B39:$B$520, \".\") & 1 )\n)","v":0}]
[null,"1.1",null,null,"ADMINISTRAÇÃO LOCAL","SERV","UNID.",null,null,0,{"$f":"IF( $G10 <> \"\",\nTRUNC( $H10 * $I10, 2 ),\nSUMIFS( $K11:$K$520,\n          $B11:$B$520, $B10 & \".*\",\n          $B11:$B$520, \"<>\" & $B10 & \".*.*\"\n) )","v":0},{"$f":"IF( $G10 <> \"\",\n     TRUNC( $H10 * $J10, 2 ),\n     SUMIFS( $L11:$L$520,\n              $B11:$B$520, $B10 & \".*\",\n              $B11:$B$520, \"<>\" & $B10 & \".*.*\"\n     ) )","v":0}]
[null,2,null,null,"SERVIÇOS PRELIMINARES",{"$nulls":4},"",{"$f":"IF( $G11 <> \"\",\nTRUNC( $H11 * $I11, 2 ),\nSUMIFS( $K12:$K$520,\n          $B12:$B$520, $B11 & \".*\",\n          $B12:$B$520, \"<>\" & $B11 & \".*.*\"\n) )","v":0},{"$f":"IF( $G11 <> \"\",\n     TRUNC( $H11 * $J11, 2 ),\n     SUMIFS( $L12:$L$520,\n              $B12:$B$520, $B11 & \".*\",\n              $B12:$B$520, \"<>\" & $B11 & \".*.*\"\n     ) )","v":0}]
[null,"2.1",null,null,"FORNECIMENTO E INSTALAÇÃO DE PLACA DE OBRA COM CHAPA GALVANIZADA E ESTRUTURA DE MADEIRA. AF_03/2022_PS","SERV","M²",null,null,0,{"$f":"IF( $G12 <> \"\",\nTRUNC( $H12 * $I12, 2 ),\nSUMIFS( $K13:$K$520,\n          $B13:$B$520, $B12 & \".*\",\n          $B13:$B$520, \"<>\" & $B12 & \".*.*\"\n) )","v":0},{"$f":"IF( $G12 <> \"\",\n     TRUNC( $H12 * $J12, 2 ),\n     SUMIFS( $L13:$L$520,\n              $B13:$B$520, $B12 & \".*\",\n              $B13:$B$520, \"<>\" & $B12 & \".*.*\"\n     ) )","v":0}]
[null,"2.2",null,null,"TAPUME COM COMPENSADO DE MADEIRA. AF_03/2024","SERV","M²",null,null,0,{"$f":"IF( $G13 <> \"\",\nTRUNC( $H13 * $I13, 2 ),\nSUMIFS( $K14:$K$520,\n          $B14:$B$520, $B13 & \".*\",\n          $B14:$B$520, \"<>\" & $B13 & \".*.*\"\n) )","v":0},{"$f":"IF( $G13 <> \"\",\n     TRUNC( $H13 * $J13, 2 ),\n     SUMIFS( $L14:$L$520,\n              $B14:$B$520, $B13 & \".*\",\n              $B14:$B$520, \"<>\" & $B13 & \".*.*\"\n     ) )","v":0}]
[null,"2.3",null,null,"CÂMERA HDCVI SPEED DOME VHD 3020 SD, DA INTELBRÁS OU SIMILAR","SERV","UNID.",null,null,0,{"$f":"IF( $G14 <> \"\",\nTRUNC( $H14 * $I14, 2 ),\nSUMIFS( $K15:$K$520,\n          $B15:$B$520, $B14 & \".*\",\n          $B15:$B$520, \"<>\" & $B14 & \".*.*\"\n) )","v":0},{"$f":"IF( $G14 <> \"\",\n     TRUNC( $H14 * $J14, 2 ),\n     SUMIFS( $L15:$L$520,\n              $B15:$B$520, $B14 & \".*\",\n              $B15:$B$520, \"<>\" & $B14 & \".*.*\"\n     ) )","v":0}]
[null,"2.4",null,null,"POSTE GALVANIZADO COM 5M PARA INSTALAÇÃO DE CÂMERA DE SEGURANÇA P/PENITENCIÁRIA","SERV","UNID.",null,null,0,{"$f":"IF( $G15 <> \"\",\nTRUNC( $H15 * $I15, 2 ),\nSUMIFS( $K16:$K$520,\n          $B16:$B$520, $B15 & \".*\",\n          $B16:$B$520, \"<>\" & $B15 & \".*.*\"\n) )","v":0},{"$f":"IF( $G15 <> \"\",\n     TRUNC( $H15 * $J15, 2 ),\n     SUMIFS( $L16:$L$520,\n              $B16:$B$520, $B15 & \".*\",\n              $B16:$B$520, \"<>\" & $B15 & \".*.*\"\n     ) )","v":0}]
[null,"2.5",null,null,"KIT CAVALETE PARA MEDIÇÃO DE ÁGUA - ENTRADA PRINCIPAL, EM AÇO GALVANIZADO DN 25 MM (1\") - FORNECIMENTO E INSTALAÇÃO (EXCLUSIVE HIDRÔMETRO). AF_03/2024","SERV","UNID.",null,null,0,{"$f":"IF( $G16 <> \"\",\nTRUNC( $H16 * $I16, 2 ),\nSUMIFS( $K17:$K$520,\n          $B17:$B$520, $B16 & \".*\",\n          $B17:$B$520, \"<>\" & $B16 & \".*.*\"\n) )","v":0},{"$f":"IF( $G16 <> \"\",\n     TRUNC( $H16 * $J16, 2 ),\n     SUMIFS( $L17:$L$520,\n              $B17:$B$520, $B16 & \".*\",\n              $B17:$B$520, \"<>\" & $B16 & \".*.*\"\n     ) )","v":0}]
[null,3,null,null,"PAREDES E PAINÉIS",{"$nulls":4},"",{"$f":"IF( $G17 <> \"\",\nTRUNC( $H17 * $I17, 2 ),\nSUMIFS( $K18:$K$520,\n          $B18:$B$520, $B17 & \".*\",\n          $B18:$B$520, \"<>\" & $B17 & \".*.*\"\n) )","v":0},{"$f":"IF( $G17 <> \"\",\n     TRUNC( $H17 * $J17, 2 ),\n     SUMIFS( $L18:$L$520,\n              $B18:$B$520, $B17 & \".*\",\n              $B18:$B$520, \"<>\" & $B17 & \".*.*\"\n     ) )","v":0}]
[null,"3.1",null,null,"ALVENARIA DE VEDAÇÃO DE BLOCOS CERÂMICOS FURADOS NA VERTICAL DE 14X19X39 CM (ESPESSURA 14 CM) E ARGAMASSA DE ASSENTAMENTO COM PREPARO EM BETONEIRA. AF_12/2021","SERV","M²",null,null,0,{"$f":"IF( $G18 <> \"\",\nTRUNC( $H18 * $I18, 2 ),\nSUMIFS( $K19:$K$520,\n          $B19:$B$520, $B18 & \".*\",\n          $B19:$B$520, \"<>\" & $B18 & \".*.*\"\n) )","v":0},{"$f":"IF( $G18 <> \"\",\n     TRUNC( $H18 * $J18, 2 ),\n     SUMIFS( $L19:$L$520,\n              $B19:$B$520, $B18 & \".*\",\n              $B19:$B$520, \"<>\" & $B18 & \".*.*\"\n     ) )","v":0}]
[null,"3.2",null,null,"DIVISÓRIA EM GRANITO CINZA ANDORINHA PARA MICTÓRIOS, POLIDO, E=2CM, INCLUSIVEFIXAÇÃO - REV 02","SERV","M²",null,null,0,{"$f":"IF( $G19 <> \"\",\nTRUNC( $H19 * $I19, 2 ),\nSUMIFS( $K20:$K$520,\n          $B20:$B$520, $B19 & \".*\",\n          $B20:$B$520, \"<>\" & $B19 & \".*.*\"\n) )","v":0},{"$f":"IF( $G19 <> \"\",\n     TRUNC( $H19 * $J19, 2 ),\n     SUMIFS( $L20:$L$520,\n              $B20:$B$520, $B19 & \".*\",\n              $B20:$B$520, \"<>\" & $B19 & \".*.*\"\n     ) )","v":0}]
[null,4,null,null,"ESQUADRIAS",{"$nulls":4},"",{"$f":"IF( $G20 <> \"\",\nTRUNC( $H20 * $I20, 2 ),\nSUMIFS( $K21:$K$520,\n          $B21:$B$520, $B20 & \".*\",\n          $B21:$B$520, \"<>\" & $B20 & \".*.*\"\n) )","v":0},{"$f":"IF( $G20 <> \"\",\n     TRUNC( $H20 * $J20, 2 ),\n     SUMIFS( $L21:$L$520,\n              $B21:$B$520, $B20 & \".*\",\n              $B21:$B$520, \"<>\" & $B20 & \".*.*\"\n     ) )","v":0}]
[null,"4.1",null,null,"PORTA EM ALUMÍNIO DE ABRIR TIPO VENEZIANA COM GUARNIÇÃO, FIXAÇÃO COM PARAFUSOS - FORNECIMENTO E INSTALAÇÃO. AF_12/2019","SERV","M²",null,null,0,{"$f":"IF( $G21 <> \"\",\nTRUNC( $H21 * $I21, 2 ),\nSUMIFS( $K22:$K$520,\n          $B22:$B$520, $B21 & \".*\",\n          $B22:$B$520, \"<>\" & $B21 & \".*.*\"\n) )","v":0},{"$f":"IF( $G21 <> \"\",\n     TRUNC( $H21 * $J21, 2 ),\n     SUMIFS( $L22:$L$520,\n              $B22:$B$520, $B21 & \".*\",\n              $B22:$B$520, \"<>\" & $B21 & \".*.*\"\n     ) )","v":0}]
[null,"4.2",null,null,"PORTA DE ALUMÍNIO DE ABRIR PARA VIDRO SEM GUARNIÇÃO, 87X210CM, FIXAÇÃO COM PARAFUSOS, INCLUSIVE VIDROS - FORNECIMENTO E INSTALAÇÃO. AF_12/2019","SERV","UNID.",null,null,0,{"$f":"IF( $G22 <> \"\",\nTRUNC( $H22 * $I22, 2 ),\nSUMIFS( $K23:$K$520,\n          $B23:$B$520, $B22 & \".*\",\n          $B23:$B$520, \"<>\" & $B22 & \".*.*\"\n) )","v":0},{"$f":"IF( $G22 <> \"\",\n     TRUNC( $H22 * $J22, 2 ),\n     SUMIFS( $L23:$L$520,\n              $B23:$B$520, $B22 & \".*\",\n              $B23:$B$520, \"<>\" & $B22 & \".*.*\"\n     ) )","v":0}]
[null,"4.3",null,null,"FORNECIMENTO E MONTAGEM DE PORTA DE ENROLAR AUTOMÁTICA, EM CHAPA 20 TRANSVISION, COM GUIAS LATERAIS, SOLEIRA T, MOTOR PARA 1000KG , PVC AUTO LUBRIFICANTE NAS GUIAS, BORRACHA DE VEDAÇÃO DE SOLEIRA, CENTRAL COM 02 CONTROLES E PINTURAELETROSTÁTICA","SERV","M²",null,null,0,{"$f":"IF( $G23 <> \"\",\nTRUNC( $H23 * $I23, 2 ),\nSUMIFS( $K24:$K$520,\n          $B24:$B$520, $B23 & \".*\",\n          $B24:$B$520, \"<>\" & $B23 & \".*.*\"\n) )","v":0},{"$f":"IF( $G23 <> \"\",\n     TRUNC( $H23 * $J23, 2 ),\n     SUMIFS( $L24:$L$520,\n              $B24:$B$520, $B23 & \".*\",\n              $B24:$B$520, \"<>\" & $B23 & \".*.*\"\n     ) )","v":0}]
[null,"4.4",null,null,"FORNECIMENTO E INSTALAÇÃO DE BRISE METÁLICO DE ALUMÍNIO, REF. B57, BRANCO NIEVE 7000, DA HUNTER DOUGLAS OU SIMILAR","SERV","M²",null,null,0,{"$f":"IF( $G24 <> \"\",\nTRUNC( $H24 * $I24, 2 ),\nSUMIFS( $K25:$K$520,\n          $B25:$B$520, $B24 & \".*\",\n          $B25:$B$520, \"<>\" & $B24 & \".*.*\"\n) )","v":0},{"$f":"IF( $G24 <> \"\",\n     TRUNC( $H24 * $J24, 2 ),\n     SUMIFS( $L25:$L$520,\n              $B25:$B$520, $B24 & \".*\",\n              $B25:$B$520, \"<>\" & $B24 & \".*.*\"\n     ) )","v":0}]
[null,"4.5",null,null,"ALÇAPÃO DE ALUMÍNIO, TIPO ESCAMA, COR FOSCA","SERV","M²",null,null,0,{"$f":"IF( $G25 <> \"\",\nTRUNC( $H25 * $I25, 2 ),\nSUMIFS( $K26:$K$520,\n          $B26:$B$520, $B25 & \".*\",\n          $B26:$B$520, \"<>\" & $B25 & \".*.*\"\n) )","v":0},{"$f":"IF( $G25 <> \"\",\n     TRUNC( $H25 * $J25, 2 ),\n     SUMIFS( $L26:$L$520,\n              $B26:$B$520, $B25 & \".*\",\n              $B26:$B$520, \"<>\" & $B25 & \".*.*\"\n     ) )","v":0}]
[null,"4.6",null,null,"GUARDA-CORPO PANORÂMICO COM PERFIS DE ALUMÍNIO E VIDRO LAMINADO 8 MM, FIXADO COM CHUMBADOR MECÂNICO. AF_04/2019_PS","SERV","M",null,null,0,{"$f":"IF( $G26 <> \"\",\nTRUNC( $H26 * $I26, 2 ),\nSUMIFS( $K27:$K$520,\n          $B27:$B$520, $B26 & \".*\",\n          $B27:$B$520, \"<>\" & $B26 & \".*.*\"\n) )","v":0},{"$f":"IF( $G26 <> \"\",\n     TRUNC( $H26 * $J26, 2 ),\n     SUMIFS( $L27:$L$520,\n              $B27:$B$520, $B26 & \".*\",\n              $B27:$B$520, \"<>\" & $B26 & \".*.*\"\n     ) )","v":0}]
[null,"4.7",null,null,"PORTA DE ALUMÍNIO DE ABRIR COM LAMBRI, COM GUARNIÇÃO, FIXAÇÃO COM PARAFUSOS - FORNECIMENTO E INSTALAÇÃO. AF_12/2019","SERV","M²",null,null,0,{"$f":"IF( $G27 <> \"\",\nTRUNC( $H27 * $I27, 2 ),\nSUMIFS( $K28:$K$520,\n          $B28:$B$520, $B27 & \".*\",\n          $B28:$B$520, \"<>\" & $B27 & \".*.*\"\n) )","v":0},{"$f":"IF( $G27 <> \"\",\n     TRUNC( $H27 * $J27, 2 ),\n     SUMIFS( $L28:$L$520,\n              $B28:$B$520, $B27 & \".*\",\n              $B28:$B$520, \"<>\" & $B27 & \".*.*\"\n     ) )","v":0}]
[null,"4.8",null,null,"VIGA METÁLICA EM PERFIL LAMINADO OU SOLDADO EM AÇO ESTRUTURAL, COM CONEXÕES PARAFUSADAS, INCLUSOS MÃO DE OBRA, TRANSPORTE E IÇAMENTO UTILIZANDO GUINDASTE - FORNECIMENTO E INSTALAÇÃO. AF_01/2020_PSA","SERV","KG",null,null,0,{"$f":"IF( $G28 <> \"\",\nTRUNC( $H28 * $I28, 2 ),\nSUMIFS( $K29:$K$520,\n          $B29:$B$520, $B28 & \".*\",\n          $B29:$B$520, \"<>\" & $B28 & \".*.*\"\n) )","v":0},{"$f":"IF( $G28 <> \"\",\n     TRUNC( $H28 * $J28, 2 ),\n     SUMIFS( $L29:$L$520,\n              $B29:$B$520, $B28 & \".*\",\n              $B29:$B$520, \"<>\" & $B28 & \".*.*\"\n     ) )","v":0}]
[null,"4.9",null,null,"INSTALAÇÃO DE VIDRO LISO INCOLOR, E = 8 MM, EM ESQUADRIA DE ALUMÍNIO OU PVC, FIXADO COM BAGUETE. AF_01/2021_PS","SERV","M²",null,null,0,{"$f":"IF( $G29 <> \"\",\nTRUNC( $H29 * $I29, 2 ),\nSUMIFS( $K30:$K$520,\n          $B30:$B$520, $B29 & \".*\",\n          $B30:$B$520, \"<>\" & $B29 & \".*.*\"\n) )","v":0},{"$f":"IF( $G29 <> \"\",\n     TRUNC( $H29 * $J29, 2 ),\n     SUMIFS( $L30:$L$520,\n              $B30:$B$520, $B29 & \".*\",\n              $B30:$B$520, \"<>\" & $B29 & \".*.*\"\n     ) )","v":0}]
[null,"4.10",null,null,"CORRIMÃO SIMPLES, DIÂMETRO EXTERNO = 1 1/2\", EM AÇO GALVANIZADO. AF_04/2019_PS","SERV","M",null,null,0,{"$f":"IF( $G30 <> \"\",\nTRUNC( $H30 * $I30, 2 ),\nSUMIFS( $K31:$K$520,\n          $B31:$B$520, $B30 & \".*\",\n          $B31:$B$520, \"<>\" & $B30 & \".*.*\"\n) )","v":0},{"$f":"IF( $G30 <> \"\",\n     TRUNC( $H30 * $J30, 2 ),\n     SUMIFS( $L31:$L$520,\n              $B31:$B$520, $B30 & \".*\",\n              $B31:$B$520, \"<>\" & $B30 & \".*.*\"\n     ) )","v":0}]
[null,5,null,null,"COBERTURA",{"$nulls":4},"",{"$f":"IF( $G31 <> \"\",\nTRUNC( $H31 * $I31, 2 ),\nSUMIFS( $K32:$K$520,\n          $B32:$B$520, $B31 & \".*\",\n          $B32:$B$520, \"<>\" & $B31 & \".*.*\"\n) )","v":0},{"$f":"IF( $G31 <> \"\",\n     TRUNC( $H31 * $J31, 2 ),\n     SUMIFS( $L32:$L$520,\n              $B32:$B$520, $B31 & \".*\",\n              $B32:$B$520, \"<>\" & $B31 & \".*.*\"\n     ) )","v":0}]
[null,"5.1",null,null,"ESTRUTURA TRELIÇADA DE COBERTURA, TIPO FINK, COM LIGAÇÕES PARAFUSADAS, INCLUSOS PERFIS METÁLICOS, CHAPAS METÁLICAS, MÃO DE OBRA E TRANSPORTE COM GUINDASTE - FORNECIMENTO E INSTALAÇÃO. AF_01/2020_PSA","SERV","KG",null,null,0,{"$f":"IF( $G32 <> \"\",\nTRUNC( $H32 * $I32, 2 ),\nSUMIFS( $K33:$K$520,\n          $B33:$B$520, $B32 & \".*\",\n          $B33:$B$520, \"<>\" & $B32 & \".*.*\"\n) )","v":0},{"$f":"IF( $G32 <> \"\",\n     TRUNC( $H32 * $J32, 2 ),\n     SUMIFS( $L33:$L$520,\n              $B33:$B$520, $B32 & \".*\",\n              $B33:$B$520, \"<>\" & $B32 & \".*.*\"\n     ) )","v":0}]
[null,"5.2",null,null,"CALHA EM CHAPA DE AÇO GALVANIZADO NÚMERO 24, DESENVOLVIMENTO DE 33 CM, INCLUSO TRANSPORTE VERTICAL. AF_07/2019","SERV","M",null,null,0,{"$f":"IF( $G33 <> \"\",\nTRUNC( $H33 * $I33, 2 ),\nSUMIFS( $K34:$K$520,\n          $B34:$B$520, $B33 & \".*\",\n          $B34:$B$520, \"<>\" & $B33 & \".*.*\"\n) )","v":0},{"$f":"IF( $G33 <> \"\",\n     TRUNC( $H33 * $J33, 2 ),\n     SUMIFS( $L34:$L$520,\n              $B34:$B$520, $B33 & \".*\",\n              $B34:$B$520, \"<>\" & $B33 & \".*.*\"\n     ) )","v":0}]
[null,"5.3",null,null,"RUFO EM CHAPA DE AÇO GALVANIZADO NÚMERO 24, CORTE DE 25 CM, INCLUSO TRANSPORTE VERTICAL. AF_07/2019","SERV","M",null,null,0,{"$f":"IF( $G34 <> \"\",\nTRUNC( $H34 * $I34, 2 ),\nSUMIFS( $K35:$K$520,\n          $B35:$B$520, $B34 & \".*\",\n          $B35:$B$520, \"<>\" & $B34 & \".*.*\"\n) )","v":0},{"$f":"IF( $G34 <> \"\",\n     TRUNC( $H34 * $J34, 2 ),\n     SUMIFS( $L35:$L$520,\n              $B35:$B$520, $B34 & \".*\",\n              $B35:$B$520, \"<>\" & $B34 & \".*.*\"\n     ) )","v":0}]
[null,"5.4",null,null,"CUMEEIRA EM GALVALUME PARA TELHA TRAPEZOIDAL GALVALUME STANDARD, COM 40 CM DECADA LADO, E = 0,43MM, COR NATURAL","SERV","M",null,null,0,{"$f":"IF( $G35 <> \"\",\nTRUNC( $H35 * $I35, 2 ),\nSUMIFS( $K36:$K$520,\n          $B36:$B$520, $B35 & \".*\",\n          $B36:$B$520, \"<>\" & $B35 & \".*.*\"\n) )","v":0},{"$f":"IF( $G35 <> \"\",\n     TRUNC( $H35 * $J35, 2 ),\n     SUMIFS( $L36:$L$520,\n              $B36:$B$520, $B35 & \".*\",\n              $B36:$B$520, \"<>\" & $B35 & \".*.*\"\n     ) )","v":0}]
[null,"5.5",null,null,"TELHA TERMOISOLANTE REVESTIDA EM ACO GALVANIZADO, FACES SUPERIOR E INFERIOR EM TELHA TRAPEZOIDAL (SEM ACESSORIOS DE FIXACAO), REVESTIMENTO COM ESPESSURA DE 0,50 MM COM PRE-PINTURA NAS DUAS FACES, NUCLEO EM POLIESTIRENO (EPS) DE 50 MM","FORN","M²",null,null,0,{"$f":"IF( $G36 <> \"\",\nTRUNC( $H36 * $I36, 2 ),\nSUMIFS( $K37:$K$520,\n          $B37:$B$520, $B36 & \".*\",\n          $B37:$B$520, \"<>\" & $B36 & \".*.*\"\n) )","v":0},{"$f":"IF( $G36 <> \"\",\n     TRUNC( $H36 * $J36, 2 ),\n     SUMIFS( $L37:$L$520,\n              $B37:$B$520, $B36 & \".*\",\n              $B37:$B$520, \"<>\" & $B36 & \".*.*\"\n     ) )","v":0}]
[null,"5.6",null,null,"TELHAMENTO COM TELHA EM AÇO GALVALUME, DUPLA, TRAPEZOIDAL, COM PREENCHIMENTO PIR 50MM, PRÉ-PINTADA, TP40 - 2 X 0,43MM, KINGSPAN- ISOESTE OU SIMILAR","SERV","M²",null,null,0,{"$f":"IF( $G37 <> \"\",\nTRUNC( $H37 * $I37, 2 ),\nSUMIFS( $K38:$K$520,\n          $B38:$B$520, $B37 & \".*\",\n          $B38:$B$520, \"<>\" & $B37 & \".*.*\"\n) )","v":0},{"$f":"IF( $G37 <> \"\",\n     TRUNC( $H37 * $J37, 2 ),\n     SUMIFS( $L38:$L$520,\n              $B38:$B$520, $B37 & \".*\",\n              $B38:$B$520, \"<>\" & $B37 & \".*.*\"\n     ) )","v":0}]
[null,6,null,null,"INSTALAÇÕES ELÉTRICAS",{"$nulls":4},"",{"$f":"IF( $G38 <> \"\",\nTRUNC( $H38 * $I38, 2 ),\nSUMIFS( $K39:$K$520,\n          $B39:$B$520, $B38 & \".*\",\n          $B39:$B$520, \"<>\" & $B38 & \".*.*\"\n) )","v":0},{"$f":"IF( $G38 <> \"\",\n     TRUNC( $H38 * $J38, 2 ),\n     SUMIFS( $L39:$L$520,\n              $B39:$B$520, $B38 & \".*\",\n              $B39:$B$520, \"<>\" & $B38 & \".*.*\"\n     ) )","v":0}]
[null,"6.1",null,null,"SPDA",{"$nulls":4},"",{"$f":"IF( $G39 <> \"\",\nTRUNC( $H39 * $I39, 2 ),\nSUMIFS( $K40:$K$520,\n          $B40:$B$520, $B39 & \".*\",\n          $B40:$B$520, \"<>\" & $B39 & \".*.*\"\n) )","v":0},{"$f":"IF( $G39 <> \"\",\n     TRUNC( $H39 * $J39, 2 ),\n     SUMIFS( $L40:$L$520,\n              $B40:$B$520, $B39 & \".*\",\n              $B40:$B$520, \"<>\" & $B39 & \".*.*\"\n     ) )","v":0}]
[null,"6.1.1",null,null,"FORNECIMENTO E ASSENTAMENTO DE BARRA CHATA DE ALUMÍNIO DE 7/8\" X 1/8\"","SERV","M",null,null,0,{"$f":"IF( $G40 <> \"\",\nTRUNC( $H40 * $I40, 2 ),\nSUMIFS( $K41:$K$520,\n          $B41:$B$520, $B40 & \".*\",\n          $B41:$B$520, \"<>\" & $B40 & \".*.*\"\n) )","v":0},{"$f":"IF( $G40 <> \"\",\n     TRUNC( $H40 * $J40, 2 ),\n     SUMIFS( $L41:$L$520,\n              $B41:$B$520, $B40 & \".*\",\n              $B41:$B$520, \"<>\" & $B40 & \".*.*\"\n     ) )","v":0}]
[null,"6.1.2",null,null,"MINI CAPTOR PARA SPDA - FORNECIMENTO E INSTALAÇÃO. AF_08/2023","SERV","UNID.",null,null,0,{"$f":"IF( $G41 <> \"\",\nTRUNC( $H41 * $I41, 2 ),\nSUMIFS( $K42:$K$520,\n          $B42:$B$520, $B41 & \".*\",\n          $B42:$B$520, \"<>\" & $B41 & \".*.*\"\n) )","v":0},{"$f":"IF( $G41 <> \"\",\n     TRUNC( $H41 * $J41, 2 ),\n     SUMIFS( $L42:$L$520,\n              $B42:$B$520, $B41 & \".*\",\n              $B42:$B$520, \"<>\" & $B41 & \".*.*\"\n     ) )","v":0}]
[null,"6.1.3",null,null,"CAIXA DE INSPEÇÃO PARA ATERRAMENTO, CIRCULAR, EM POLIETILENO, DIÂMETRO INTERNO = 0,3 M. AF_12/2020","SERV","UNID.",null,null,0,{"$f":"IF( $G42 <> \"\",\nTRUNC( $H42 * $I42, 2 ),\nSUMIFS( $K43:$K$520,\n          $B43:$B$520, $B42 & \".*\",\n          $B43:$B$520, \"<>\" & $B42 & \".*.*\"\n) )","v":0},{"$f":"IF( $G42 <> \"\",\n     TRUNC( $H42 * $J42, 2 ),\n     SUMIFS( $L43:$L$520,\n              $B43:$B$520, $B42 & \".*\",\n              $B43:$B$520, \"<>\" & $B42 & \".*.*\"\n     ) )","v":0}]
[null,"6.1.4",null,null,"HASTE DE ATERRAMENTO, DIÂMETRO 5/8\", COM 3 METROS - FORNECIMENTO E INSTALAÇÃO. AF_08/2023","SERV","UNID.",null,null,0,{"$f":"IF( $G43 <> \"\",\nTRUNC( $H43 * $I43, 2 ),\nSUMIFS( $K44:$K$520,\n          $B44:$B$520, $B43 & \".*\",\n          $B44:$B$520, \"<>\" & $B43 & \".*.*\"\n) )","v":0},{"$f":"IF( $G43 <> \"\",\n     TRUNC( $H43 * $J43, 2 ),\n     SUMIFS( $L44:$L$520,\n              $B44:$B$520, $B43 & \".*\",\n              $B44:$B$520, \"<>\" & $B43 & \".*.*\"\n     ) )","v":0}]
[null,"6.1.5",null,null,"ESCAVAÇÃO MANUAL DE VALA. AF_09/2024","SERV","M³",null,null,0,{"$f":"IF( $G44 <> \"\",\nTRUNC( $H44 * $I44, 2 ),\nSUMIFS( $K45:$K$520,\n          $B45:$B$520, $B44 & \".*\",\n          $B45:$B$520, \"<>\" & $B44 & \".*.*\"\n) )","v":0},{"$f":"IF( $G44 <> \"\",\n     TRUNC( $H44 * $J44, 2 ),\n     SUMIFS( $L45:$L$520,\n              $B45:$B$520, $B44 & \".*\",\n              $B45:$B$520, \"<>\" & $B44 & \".*.*\"\n     ) )","v":0}]
[null,"6.1.6",null,null,"BUCHA DE NYLON SEM ABA S6, COM PARAFUSO DE 4,20 X 40 MM EM ACO ZINCADO COM ROSCA SOBERBA, CABECA CHATA E FENDA PHILLIPS","FORN","UNID.",null,null,0,{"$f":"IF( $G45 <> \"\",\nTRUNC( $H45 * $I45, 2 ),\nSUMIFS( $K46:$K$520,\n          $B46:$B$520, $B45 & \".*\",\n          $B46:$B$520, \"<>\" & $B45 & \".*.*\"\n) )","v":0},{"$f":"IF( $G45 <> \"\",\n     TRUNC( $H45 * $J45, 2 ),\n     SUMIFS( $L46:$L$520,\n              $B46:$B$520, $B45 & \".*\",\n              $B46:$B$520, \"<>\" & $B45 & \".*.*\"\n     ) )","v":0}]
[null,"6.1.7",null,null,"TERMINAL A COMPRESSAO EM COBRE ESTANHADO PARA CABO 35 MM2, 1 FURO E 1 COMPRESSAO, PARA PARAFUSO DE FIXACAO M8","FORN","UNID.",null,null,0,{"$f":"IF( $G46 <> \"\",\nTRUNC( $H46 * $I46, 2 ),\nSUMIFS( $K47:$K$520,\n          $B47:$B$520, $B46 & \".*\",\n          $B47:$B$520, \"<>\" & $B46 & \".*.*\"\n) )","v":0},{"$f":"IF( $G46 <> \"\",\n     TRUNC( $H46 * $J46, 2 ),\n     SUMIFS( $L47:$L$520,\n              $B47:$B$520, $B46 & \".*\",\n              $B47:$B$520, \"<>\" & $B46 & \".*.*\"\n     ) )","v":0}]
[null,"6.1.8",null,null,"CABO DE COBRE NÚ 35 MM2 - FORNECIMENTO E ASSENTAMENTO (3,16M/KG)","SERV","KG",null,null,0,{"$f":"IF( $G47 <> \"\",\nTRUNC( $H47 * $I47, 2 ),\nSUMIFS( $K48:$K$520,\n          $B48:$B$520, $B47 & \".*\",\n          $B48:$B$520, \"<>\" & $B47 & \".*.*\"\n) )","v":0},{"$f":"IF( $G47 <> \"\",\n     TRUNC( $H47 * $J47, 2 ),\n     SUMIFS( $L48:$L$520,\n              $B48:$B$520, $B47 & \".*\",\n              $B48:$B$520, \"<>\" & $B47 & \".*.*\"\n     ) )","v":0}]
[null,"6.1.9",null,null,"CABO DE COBRE NÚ 50 MM2 - FORNECIMENTO E ASSENTAMENTO (2,27M/KG)","SERV","KG",null,null,0,{"$f":"IF( $G48 <> \"\",\nTRUNC( $H48 * $I48, 2 ),\nSUMIFS( $K49:$K$520,\n          $B49:$B$520, $B48 & \".*\",\n          $B49:$B$520, \"<>\" & $B48 & \".*.*\"\n) )","v":0},{"$f":"IF( $G48 <> \"\",\n     TRUNC( $H48 * $J48, 2 ),\n     SUMIFS( $L49:$L$520,\n              $B49:$B$520, $B48 & \".*\",\n              $B49:$B$520, \"<>\" & $B48 & \".*.*\"\n     ) )","v":0}]
[null,"6.1.10",null,null,"SOLDA EXOTÉRMICA PARA CABO DE 35MM²","SERV","UNID.",null,null,0,{"$f":"IF( $G49 <> \"\",\nTRUNC( $H49 * $I49, 2 ),\nSUMIFS( $K50:$K$520,\n          $B50:$B$520, $B49 & \".*\",\n          $B50:$B$520, \"<>\" & $B49 & \".*.*\"\n) )","v":0},{"$f":"IF( $G49 <> \"\",\n     TRUNC( $H49 * $J49, 2 ),\n     SUMIFS( $L50:$L$520,\n              $B50:$B$520, $B49 & \".*\",\n              $B50:$B$520, \"<>\" & $B49 & \".*.*\"\n     ) )","v":0}]
[null,"6.1.11",null,null,"SOLDA EXOTÉRMICA PARA CABO DE 50MM²","SERV","UNID.",null,null,0,{"$f":"IF( $G50 <> \"\",\nTRUNC( $H50 * $I50, 2 ),\nSUMIFS( $K51:$K$520,\n          $B51:$B$520, $B50 & \".*\",\n          $B51:$B$520, \"<>\" & $B50 & \".*.*\"\n) )","v":0},{"$f":"IF( $G50 <> \"\",\n     TRUNC( $H50 * $J50, 2 ),\n     SUMIFS( $L51:$L$520,\n              $B51:$B$520, $B50 & \".*\",\n              $B51:$B$520, \"<>\" & $B50 & \".*.*\"\n     ) )","v":0}]
[null,"6.2",null,null,"PREVENTIVO ELÉTRICO",{"$nulls":4},"",{"$f":"IF( $G51 <> \"\",\nTRUNC( $H51 * $I51, 2 ),\nSUMIFS( $K52:$K$520,\n          $B52:$B$520, $B51 & \".*\",\n          $B52:$B$520, \"<>\" & $B51 & \".*.*\"\n) )","v":0},{"$f":"IF( $G51 <> \"\",\n     TRUNC( $H51 * $J51, 2 ),\n     SUMIFS( $L52:$L$520,\n              $B52:$B$520, $B51 & \".*\",\n              $B52:$B$520, \"<>\" & $B51 & \".*.*\"\n     ) )","v":0}]
[null,"6.2.1",null,null,"BUCHA DE NYLON SEM ABA S6, COM PARAFUSO DE 4,20 X 40 MM EM ACO ZINCADO COM ROSCA SOBERBA, CABECA CHATA E FENDA PHILLIPS","FORN","UNID.",null,null,0,{"$f":"IF( $G52 <> \"\",\nTRUNC( $H52 * $I52, 2 ),\nSUMIFS( $K53:$K$520,\n          $B53:$B$520, $B52 & \".*\",\n          $B53:$B$520, \"<>\" & $B52 & \".*.*\"\n) )","v":0},{"$f":"IF( $G52 <> \"\",\n     TRUNC( $H52 * $J52, 2 ),\n     SUMIFS( $L53:$L$520,\n              $B53:$B$520, $B52 & \".*\",\n              $B53:$B$520, \"<>\" & $B52 & \".*.*\"\n     ) )","v":0}]
[null,"6.2.2",null,null,"ACIONADOR MANUAL (BOTOEIRA) TIPO QUEBRA-VIDRO, P/INSTAL. INCENDIO","SERV","UNID.",null,null,0,{"$f":"IF( $G53 <> \"\",\nTRUNC( $H53 * $I53, 2 ),\nSUMIFS( $K54:$K$520,\n          $B54:$B$520, $B53 & \".*\",\n          $B54:$B$520, \"<>\" & $B53 & \".*.*\"\n) )","v":0},{"$f":"IF( $G53 <> \"\",\n     TRUNC( $H53 * $J53, 2 ),\n     SUMIFS( $L54:$L$520,\n              $B54:$B$520, $B53 & \".*\",\n              $B54:$B$520, \"<>\" & $B53 & \".*.*\"\n     ) )","v":0}]
[null,"6.2.3",null,null,"SIRENE AÚDIOVISUAL ENDEREÇAVEL, 120DB, PARA ALARME DE INCÊNDIO","SERV","UNID.",null,null,0,{"$f":"IF( $G54 <> \"\",\nTRUNC( $H54 * $I54, 2 ),\nSUMIFS( $K55:$K$520,\n          $B55:$B$520, $B54 & \".*\",\n          $B55:$B$520, \"<>\" & $B54 & \".*.*\"\n) )","v":0},{"$f":"IF( $G54 <> \"\",\n     TRUNC( $H54 * $J54, 2 ),\n     SUMIFS( $L55:$L$520,\n              $B55:$B$520, $B54 & \".*\",\n              $B55:$B$520, \"<>\" & $B54 & \".*.*\"\n     ) )","v":0}]
[null,"6.2.4",null,null,"CENTRAL DE ALARME ENDEREÇÁVEL DE INCENDIO COM SISTEMA P/ ATÉ 250 DISPOSITIVOS, MARCAL VERIN OU SIMILAR, MODELO VRE-250 C/ BATERIA DE 12V E 7AMPERES","SERV","UNID.",null,null,0,{"$f":"IF( $G55 <> \"\",\nTRUNC( $H55 * $I55, 2 ),\nSUMIFS( $K56:$K$520,\n          $B56:$B$520, $B55 & \".*\",\n          $B56:$B$520, \"<>\" & $B55 & \".*.*\"\n) )","v":0},{"$f":"IF( $G55 <> \"\",\n     TRUNC( $H55 * $J55, 2 ),\n     SUMIFS( $L56:$L$520,\n              $B56:$B$520, $B55 & \".*\",\n              $B56:$B$520, \"<>\" & $B55 & \".*.*\"\n     ) )","v":0}]
[null,"6.2.5",null,null,"FONTE DE ALIMENTAÇÃO 15W (24V)","FORN","UNID.",null,null,0,{"$f":"IF( $G56 <> \"\",\nTRUNC( $H56 * $I56, 2 ),\nSUMIFS( $K57:$K$520,\n          $B57:$B$520, $B56 & \".*\",\n          $B57:$B$520, \"<>\" & $B56 & \".*.*\"\n) )","v":0},{"$f":"IF( $G56 <> \"\",\n     TRUNC( $H56 * $J56, 2 ),\n     SUMIFS( $L57:$L$520,\n              $B57:$B$520, $B56 & \".*\",\n              $B57:$B$520, \"<>\" & $B56 & \".*.*\"\n     ) )","v":0}]
[null,"6.2.6",null,null,"LUMINÁRIA DE EMERGÊNCIA C/ DOIS PROJETORS LED ALIMENTAÇÃO 127/220 DE 12V/55 AUTONOMIA DE 3HORAS","FORN","UNID.",null,null,0,{"$f":"IF( $G57 <> \"\",\nTRUNC( $H57 * $I57, 2 ),\nSUMIFS( $K58:$K$520,\n          $B58:$B$520, $B57 & \".*\",\n          $B58:$B$520, \"<>\" & $B57 & \".*.*\"\n) )","v":0},{"$f":"IF( $G57 <> \"\",\n     TRUNC( $H57 * $J57, 2 ),\n     SUMIFS( $L58:$L$520,\n              $B58:$B$520, $B57 & \".*\",\n              $B58:$B$520, \"<>\" & $B57 & \".*.*\"\n     ) )","v":0}]
[null,"6.2.7",null,null,"CAIXA RETANGULAR 4\" X 2\" MÉDIA (1,30 M DO PISO), PVC, INSTALADA EM PAREDE - FORNECIMENTO E INSTALAÇÃO. AF_03/2023","SERV","UNID.",null,null,0,{"$f":"IF( $G58 <> \"\",\nTRUNC( $H58 * $I58, 2 ),\nSUMIFS( $K59:$K$520,\n          $B59:$B$520, $B58 & \".*\",\n          $B59:$B$520, \"<>\" & $B58 & \".*.*\"\n) )","v":0},{"$f":"IF( $G58 <> \"\",\n     TRUNC( $H58 * $J58, 2 ),\n     SUMIFS( $L59:$L$520,\n              $B59:$B$520, $B58 & \".*\",\n              $B59:$B$520, \"<>\" & $B58 & \".*.*\"\n     ) )","v":0}]
[null,"6.2.8",null,null,"CURVA 90 GRAUS PARA ELETRODUTO, PVC, ROSCÁVEL, DN 25 MM (3/4\"), PARA CIRCUITOS TERMINAIS, INSTALADA EM PAREDE - FORNECIMENTO E INSTALAÇÃO. AF_03/2023","SERV","UNID.",null,null,0,{"$f":"IF( $G59 <> \"\",\nTRUNC( $H59 * $I59, 2 ),\nSUMIFS( $K60:$K$520,\n          $B60:$B$520, $B59 & \".*\",\n          $B60:$B$520, \"<>\" & $B59 & \".*.*\"\n) )","v":0},{"$f":"IF( $G59 <> \"\",\n     TRUNC( $H59 * $J59, 2 ),\n     SUMIFS( $L60:$L$520,\n              $B60:$B$520, $B59 & \".*\",\n              $B60:$B$520, \"<>\" & $B59 & \".*.*\"\n     ) )","v":0}]
[null,"6.2.9",null,null,"CABO BLINDADO PARA ALARME E DETECÇÃO DE INCÊNCIO 4 X 1,5MM2","SERV","M",null,null,0,{"$f":"IF( $G60 <> \"\",\nTRUNC( $H60 * $I60, 2 ),\nSUMIFS( $K61:$K$520,\n          $B61:$B$520, $B60 & \".*\",\n          $B61:$B$520, \"<>\" & $B60 & \".*.*\"\n) )","v":0},{"$f":"IF( $G60 <> \"\",\n     TRUNC( $H60 * $J60, 2 ),\n     SUMIFS( $L61:$L$520,\n              $B61:$B$520, $B60 & \".*\",\n              $B61:$B$520, \"<>\" & $B60 & \".*.*\"\n     ) )","v":0}]
[null,"6.2.10",null,null,"PLACA DE SINALIZACAO, FOTOLUMINESCENTE, 38X19 CM, EM PVC , COM SETA INDICATIVA DE SENTIDO (ESQUERDA OU DIREITA) DE SAÍDA DE EMERGÊNCIA- PLACA S2","SERV","UNID.",null,null,0,{"$f":"IF( $G61 <> \"\",\nTRUNC( $H61 * $I61, 2 ),\nSUMIFS( $K62:$K$520,\n          $B62:$B$520, $B61 & \".*\",\n          $B62:$B$520, \"<>\" & $B61 & \".*.*\"\n) )","v":0},{"$f":"IF( $G61 <> \"\",\n     TRUNC( $H61 * $J61, 2 ),\n     SUMIFS( $L62:$L$520,\n              $B62:$B$520, $B61 & \".*\",\n              $B62:$B$520, \"<>\" & $B61 & \".*.*\"\n     ) )","v":0}]
[null,"6.2.11",null,null,"PLACA DE SINALIZACAO DE SEGURANCA CONTRA INCENDIO, FOTOLUMINESCENTE, RETANGULAR, *20 X 40* CM, EM PVC *2* MM ANTI-CHAMAS (SIMBOLOS, CORES E PICTOGRAMAS CONFORME NBR 16820)","FORN","UNID.",null,null,0,{"$f":"IF( $G62 <> \"\",\nTRUNC( $H62 * $I62, 2 ),\nSUMIFS( $K63:$K$520,\n          $B63:$B$520, $B62 & \".*\",\n          $B63:$B$520, \"<>\" & $B62 & \".*.*\"\n) )","v":0},{"$f":"IF( $G62 <> \"\",\n     TRUNC( $H62 * $J62, 2 ),\n     SUMIFS( $L63:$L$520,\n              $B63:$B$520, $B62 & \".*\",\n              $B63:$B$520, \"<>\" & $B62 & \".*.*\"\n     ) )","v":0}]
[null,"6.2.12",null,null,"PLACA DE SINALIZACAO, FOTOLUMINESCENTE, 38X19 CM, EM PVC , COM LOGOTIPO \"COMANDO MANUAL DE ALARME DE INCÊNDIO\"- PLACA E2","SERV","UNID.",null,null,0,{"$f":"IF( $G63 <> \"\",\nTRUNC( $H63 * $I63, 2 ),\nSUMIFS( $K64:$K$520,\n          $B64:$B$520, $B63 & \".*\",\n          $B64:$B$520, \"<>\" & $B63 & \".*.*\"\n) )","v":0},{"$f":"IF( $G63 <> \"\",\n     TRUNC( $H63 * $J63, 2 ),\n     SUMIFS( $L64:$L$520,\n              $B64:$B$520, $B63 & \".*\",\n              $B64:$B$520, \"<>\" & $B63 & \".*.*\"\n     ) )","v":0}]
[null,"6.2.13",null,null,"PINTURA DE SÍMBOLOS E TEXTOS COM TINTA ACRÍLICA, DEMARCAÇÃO COM FITA ADESIVA E APLICAÇÃO COM ROLO. AF_05/2021","SERV","M²",null,null,0,{"$f":"IF( $G64 <> \"\",\nTRUNC( $H64 * $I64, 2 ),\nSUMIFS( $K65:$K$520,\n          $B65:$B$520, $B64 & \".*\",\n          $B65:$B$520, \"<>\" & $B64 & \".*.*\"\n) )","v":0},{"$f":"IF( $G64 <> \"\",\n     TRUNC( $H64 * $J64, 2 ),\n     SUMIFS( $L65:$L$520,\n              $B65:$B$520, $B64 & \".*\",\n              $B65:$B$520, \"<>\" & $B64 & \".*.*\"\n     ) )","v":0}]
[null,"6.2.14",null,null,"EXTINTOR DE INCÊNDIO PORTÁTIL COM CARGA DE PQS DE 6 KG, CLASSE BC - FORNECIMENTO E INSTALAÇÃO. AF_10/2020_PE","SERV","UNID.",null,null,0,{"$f":"IF( $G65 <> \"\",\nTRUNC( $H65 * $I65, 2 ),\nSUMIFS( $K66:$K$520,\n          $B66:$B$520, $B65 & \".*\",\n          $B66:$B$520, \"<>\" & $B65 & \".*.*\"\n) )","v":0},{"$f":"IF( $G65 <> \"\",\n     TRUNC( $H65 * $J65, 2 ),\n     SUMIFS( $L66:$L$520,\n              $B66:$B$520, $B65 & \".*\",\n              $B66:$B$520, \"<>\" & $B65 & \".*.*\"\n     ) )","v":0}]
[null,"6.2.15",null,null,"SUPORTE DECORATIVO PARA EXTINTORES - REV 01/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G66 <> \"\",\nTRUNC( $H66 * $I66, 2 ),\nSUMIFS( $K67:$K$520,\n          $B67:$B$520, $B66 & \".*\",\n          $B67:$B$520, \"<>\" & $B66 & \".*.*\"\n) )","v":0},{"$f":"IF( $G66 <> \"\",\n     TRUNC( $H66 * $J66, 2 ),\n     SUMIFS( $L67:$L$520,\n              $B67:$B$520, $B66 & \".*\",\n              $B67:$B$520, \"<>\" & $B66 & \".*.*\"\n     ) )","v":0}]
[null,"6.2.16",null,null,"ELETRODUTO RÍGIDO ROSCÁVEL, PVC, DN 25 MM (3/4\"), PARA CIRCUITOS TERMINAIS, INSTALADO EM PAREDE - FORNECIMENTO E INSTALAÇÃO. AF_03/2023","SERV","M",null,null,0,{"$f":"IF( $G67 <> \"\",\nTRUNC( $H67 * $I67, 2 ),\nSUMIFS( $K68:$K$520,\n          $B68:$B$520, $B67 & \".*\",\n          $B68:$B$520, \"<>\" & $B67 & \".*.*\"\n) )","v":0},{"$f":"IF( $G67 <> \"\",\n     TRUNC( $H67 * $J67, 2 ),\n     SUMIFS( $L68:$L$520,\n              $B68:$B$520, $B67 & \".*\",\n              $B68:$B$520, \"<>\" & $B67 & \".*.*\"\n     ) )","v":0}]
[null,"6.2.17",null,null,"ABRACADEIRA EM ACO PARA AMARRACAO DE ELETRODUTOS, TIPO D, COM 3/4\" E CUNHA DE FIXACAO","FORN","UNID.",null,null,0,{"$f":"IF( $G68 <> \"\",\nTRUNC( $H68 * $I68, 2 ),\nSUMIFS( $K69:$K$520,\n          $B69:$B$520, $B68 & \".*\",\n          $B69:$B$520, \"<>\" & $B68 & \".*.*\"\n) )","v":0},{"$f":"IF( $G68 <> \"\",\n     TRUNC( $H68 * $J68, 2 ),\n     SUMIFS( $L69:$L$520,\n              $B69:$B$520, $B68 & \".*\",\n              $B69:$B$520, \"<>\" & $B68 & \".*.*\"\n     ) )","v":0}]
[null,"6.3",null,null,"INFRAESTRUTURA GERAL PARA ALIMENTAÇÃO DOS BOXES E CONDOMÍNIO",{"$nulls":4},"",{"$f":"IF( $G69 <> \"\",\nTRUNC( $H69 * $I69, 2 ),\nSUMIFS( $K70:$K$520,\n          $B70:$B$520, $B69 & \".*\",\n          $B70:$B$520, \"<>\" & $B69 & \".*.*\"\n) )","v":0},{"$f":"IF( $G69 <> \"\",\n     TRUNC( $H69 * $J69, 2 ),\n     SUMIFS( $L70:$L$520,\n              $B70:$B$520, $B69 & \".*\",\n              $B70:$B$520, \"<>\" & $B69 & \".*.*\"\n     ) )","v":0}]
[null,"6.3.1",null,null,"ELETRODUTO FLEXÍVEL CORRUGADO, PVC, DN 32 MM (1\"), PARA CIRCUITOS TERMINAIS, INSTALADO EM FORRO - FORNECIMENTO E INSTALAÇÃO. AF_03/2023_PA","SERV","M",null,null,0,{"$f":"IF( $G70 <> \"\",\nTRUNC( $H70 * $I70, 2 ),\nSUMIFS( $K71:$K$520,\n          $B71:$B$520, $B70 & \".*\",\n          $B71:$B$520, \"<>\" & $B70 & \".*.*\"\n) )","v":0},{"$f":"IF( $G70 <> \"\",\n     TRUNC( $H70 * $J70, 2 ),\n     SUMIFS( $L71:$L$520,\n              $B71:$B$520, $B70 & \".*\",\n              $B71:$B$520, \"<>\" & $B70 & \".*.*\"\n     ) )","v":0}]
[null,"6.3.2",null,null,"ELETRODUTO RÍGIDO ROSCÁVEL, PVC, DN 32 MM (1\"), PARA CIRCUITOS TERMINAIS, INSTALADO EM FORRO - FORNECIMENTO E INSTALAÇÃO. AF_03/2023","SERV","M",null,null,0,{"$f":"IF( $G71 <> \"\",\nTRUNC( $H71 * $I71, 2 ),\nSUMIFS( $K72:$K$520,\n          $B72:$B$520, $B71 & \".*\",\n          $B72:$B$520, \"<>\" & $B71 & \".*.*\"\n) )","v":0},{"$f":"IF( $G71 <> \"\",\n     TRUNC( $H71 * $J71, 2 ),\n     SUMIFS( $L72:$L$520,\n              $B72:$B$520, $B71 & \".*\",\n              $B72:$B$520, \"<>\" & $B71 & \".*.*\"\n     ) )","v":0}]
[null,"6.3.3",null,null,"CURVA 90 GRAUS PARA ELETRODUTO, PVC, ROSCÁVEL, DN 32 MM (1\"), PARA CIRCUITOS TERMINAIS, INSTALADA EM FORRO - FORNECIMENTO E INSTALAÇÃO. AF_03/2023","SERV","UNID.",null,null,0,{"$f":"IF( $G72 <> \"\",\nTRUNC( $H72 * $I72, 2 ),\nSUMIFS( $K73:$K$520,\n          $B73:$B$520, $B72 & \".*\",\n          $B73:$B$520, \"<>\" & $B72 & \".*.*\"\n) )","v":0},{"$f":"IF( $G72 <> \"\",\n     TRUNC( $H72 * $J72, 2 ),\n     SUMIFS( $L73:$L$520,\n              $B73:$B$520, $B72 & \".*\",\n              $B73:$B$520, \"<>\" & $B72 & \".*.*\"\n     ) )","v":0}]
[null,"6.3.4",null,null,"LUVA PARA ELETRODUTO, PVC, ROSCÁVEL, DN 32 MM (1\"), PARA CIRCUITOS TERMINAIS, INSTALADA EM FORRO - FORNECIMENTO E INSTALAÇÃO. AF_03/2023","SERV","UNID.",null,null,{"$f":"IF(F73<>\"\",\nTRUNC(IF(F73=\"SERV\",I73*(1+$L$5/100),I73*(1+$L$6/100)),2),\n\"\" )","v":0},{"$f":"IF( $G73 <> \"\",\nTRUNC( $H73 * $I73, 2 ),\nSUMIFS( $K74:$K$520,\n          $B74:$B$520, $B73 & \".*\",\n          $B74:$B$520, \"<>\" & $B73 & \".*.*\"\n) )","v":0},{"$f":"IF( $G73 <> \"\",\n     TRUNC( $H73 * $J73, 2 ),\n     SUMIFS( $L74:$L$520,\n              $B74:$B$520, $B73 & \".*\",\n              $B74:$B$520, \"<>\" & $B73 & \".*.*\"\n     ) )","v":0}]
[null,"6.3.5",null,null,"ABRACADEIRA EM ACO PARA AMARRACAO DE ELETRODUTOS, TIPO D, COM 3/4\" E CUNHA DE FIXACAO","FORN","UNID.",null,null,0,{"$f":"IF( $G74 <> \"\",\nTRUNC( $H74 * $I74, 2 ),\nSUMIFS( $K75:$K$520,\n          $B75:$B$520, $B74 & \".*\",\n          $B75:$B$520, \"<>\" & $B74 & \".*.*\"\n) )","v":0},{"$f":"IF( $G74 <> \"\",\n     TRUNC( $H74 * $J74, 2 ),\n     SUMIFS( $L75:$L$520,\n              $B75:$B$520, $B74 & \".*\",\n              $B75:$B$520, \"<>\" & $B74 & \".*.*\"\n     ) )","v":0}]
[null,"6.3.6",null,null,"FORNECIMENTO E INSTALAÇÃO DE ELETROCALHA PERFURADA 100 X   100 X 3000 MM (REF. MOPA OU SIMILAR)","SERV","UNID.",null,null,0,{"$f":"IF( $G75 <> \"\",\nTRUNC( $H75 * $I75, 2 ),\nSUMIFS( $K76:$K$520,\n          $B76:$B$520, $B75 & \".*\",\n          $B76:$B$520, \"<>\" & $B75 & \".*.*\"\n) )","v":0},{"$f":"IF( $G75 <> \"\",\n     TRUNC( $H75 * $J75, 2 ),\n     SUMIFS( $L76:$L$520,\n              $B76:$B$520, $B75 & \".*\",\n              $B76:$B$520, \"<>\" & $B75 & \".*.*\"\n     ) )","v":0}]
[null,"6.3.7",null,null,"TAMPA DE ENCAIXE 100 X 3000 MM, ZINCADA, PARA ELETROCALHA METÁLICA (REF.: MOPA OU SIMILAR)","SERV","M",null,null,0,{"$f":"IF( $G76 <> \"\",\nTRUNC( $H76 * $I76, 2 ),\nSUMIFS( $K77:$K$520,\n          $B77:$B$520, $B76 & \".*\",\n          $B77:$B$520, \"<>\" & $B76 & \".*.*\"\n) )","v":0},{"$f":"IF( $G76 <> \"\",\n     TRUNC( $H76 * $J76, 2 ),\n     SUMIFS( $L77:$L$520,\n              $B77:$B$520, $B76 & \".*\",\n              $B77:$B$520, \"<>\" & $B76 & \".*.*\"\n     ) )","v":0}]
[null,"6.3.8",null,null,"TERMINAL 100 X 100 MM, GALVANIZADO À FOGO, PARA ELETROCALHA METALICA (REF. MOPA OU SIMILAR)","SERV","UNID.",null,null,0,{"$f":"IF( $G77 <> \"\",\nTRUNC( $H77 * $I77, 2 ),\nSUMIFS( $K78:$K$520,\n          $B78:$B$520, $B77 & \".*\",\n          $B78:$B$520, \"<>\" & $B77 & \".*.*\"\n) )","v":0},{"$f":"IF( $G77 <> \"\",\n     TRUNC( $H77 * $J77, 2 ),\n     SUMIFS( $L78:$L$520,\n              $B78:$B$520, $B77 & \".*\",\n              $B78:$B$520, \"<>\" & $B77 & \".*.*\"\n     ) )","v":0}]
[null,"6.3.9",null,null,"CURVA VERTICAL 200 X 100 MM PARA ELETROCALHA METÁLICA, COM ÂNGULO 90° (REF.: MOPA OU SIMILAR)","SERV","UNID.",null,null,0,{"$f":"IF( $G78 <> \"\",\nTRUNC( $H78 * $I78, 2 ),\nSUMIFS( $K79:$K$520,\n          $B79:$B$520, $B78 & \".*\",\n          $B79:$B$520, \"<>\" & $B78 & \".*.*\"\n) )","v":0},{"$f":"IF( $G78 <> \"\",\n     TRUNC( $H78 * $J78, 2 ),\n     SUMIFS( $L79:$L$520,\n              $B79:$B$520, $B78 & \".*\",\n              $B79:$B$520, \"<>\" & $B78 & \".*.*\"\n     ) )","v":0}]
[null,"6.3.10",null,null,"SUPORTE VERTICAL  100 X 100 MM  PARA FIXAÇÃO DE ELETROCALHA METÁLICA ( REF.: MOPA OU SIMILAR)","FORN","UNID.",null,null,0,{"$f":"IF( $G79 <> \"\",\nTRUNC( $H79 * $I79, 2 ),\nSUMIFS( $K80:$K$520,\n          $B80:$B$520, $B79 & \".*\",\n          $B80:$B$520, \"<>\" & $B79 & \".*.*\"\n) )","v":0},{"$f":"IF( $G79 <> \"\",\n     TRUNC( $H79 * $J79, 2 ),\n     SUMIFS( $L80:$L$520,\n              $B80:$B$520, $B79 & \".*\",\n              $B80:$B$520, \"<>\" & $B79 & \".*.*\"\n     ) )","v":0}]
[null,"6.3.11",null,null,"EMENDA INTERNA 100 X 100 MM COM BASE LISA PERFURADA PARA ELETROCALHA METÁLICA(REF. MOPA OU SIMILAR)","SERV","UNID.",null,null,0,{"$f":"IF( $G80 <> \"\",\nTRUNC( $H80 * $I80, 2 ),\nSUMIFS( $K81:$K$520,\n          $B81:$B$520, $B80 & \".*\",\n          $B81:$B$520, \"<>\" & $B80 & \".*.*\"\n) )","v":0},{"$f":"IF( $G80 <> \"\",\n     TRUNC( $H80 * $J80, 2 ),\n     SUMIFS( $L81:$L$520,\n              $B81:$B$520, $B80 & \".*\",\n              $B81:$B$520, \"<>\" & $B80 & \".*.*\"\n     ) )","v":0}]
[null,"6.3.12",null,null,"TALA PLANA PERFURADA 100MM PARA ELETROCALHA METÁLICA (REF.: MOPA OU SIMILAR) - REV 01","SERV","UNID.",null,null,0,{"$f":"IF( $G81 <> \"\",\nTRUNC( $H81 * $I81, 2 ),\nSUMIFS( $K82:$K$520,\n          $B82:$B$520, $B81 & \".*\",\n          $B82:$B$520, \"<>\" & $B81 & \".*.*\"\n) )","v":0},{"$f":"IF( $G81 <> \"\",\n     TRUNC( $H81 * $J81, 2 ),\n     SUMIFS( $L82:$L$520,\n              $B82:$B$520, $B81 & \".*\",\n              $B82:$B$520, \"<>\" & $B81 & \".*.*\"\n     ) )","v":0}]
[null,"6.3.13",null,null,"TAMPA DE ENCAIXE 100MM PARA TÊ HORIZONTAL, ZINCADA, PARA ELETROCALHA METÁLICA(REF.: MOPA OU SIMILAR)","SERV","UNID.",null,null,0,{"$f":"IF( $G82 <> \"\",\nTRUNC( $H82 * $I82, 2 ),\nSUMIFS( $K83:$K$520,\n          $B83:$B$520, $B82 & \".*\",\n          $B83:$B$520, \"<>\" & $B82 & \".*.*\"\n) )","v":0},{"$f":"IF( $G82 <> \"\",\n     TRUNC( $H82 * $J82, 2 ),\n     SUMIFS( $L83:$L$520,\n              $B83:$B$520, $B82 & \".*\",\n              $B83:$B$520, \"<>\" & $B82 & \".*.*\"\n     ) )","v":0}]
[null,"6.3.14",null,null,"TÊ HORIZONTAL 100 X 100MM PARA ELETROCALHA METÁLICA (REF. MOPA OU SIMILAR)","FORN","UNID.",null,null,0,{"$f":"IF( $G83 <> \"\",\nTRUNC( $H83 * $I83, 2 ),\nSUMIFS( $K84:$K$520,\n          $B84:$B$520, $B83 & \".*\",\n          $B84:$B$520, \"<>\" & $B83 & \".*.*\"\n) )","v":0},{"$f":"IF( $G83 <> \"\",\n     TRUNC( $H83 * $J83, 2 ),\n     SUMIFS( $L84:$L$520,\n              $B84:$B$520, $B83 & \".*\",\n              $B84:$B$520, \"<>\" & $B83 & \".*.*\"\n     ) )","v":0}]
[null,"6.3.15",null,null,"TAMPA DE ENCAIXE PARA CURVA 90º, VERTICAL, 100MM, ZINCADA, PARA ELETROCALHA METÁLICA","SERV","UNID.",null,null,0,{"$f":"IF( $G84 <> \"\",\nTRUNC( $H84 * $I84, 2 ),\nSUMIFS( $K85:$K$520,\n          $B85:$B$520, $B84 & \".*\",\n          $B85:$B$520, \"<>\" & $B84 & \".*.*\"\n) )","v":0},{"$f":"IF( $G84 <> \"\",\n     TRUNC( $H84 * $J84, 2 ),\n     SUMIFS( $L85:$L$520,\n              $B85:$B$520, $B84 & \".*\",\n              $B85:$B$520, \"<>\" & $B84 & \".*.*\"\n     ) )","v":0}]
[null,"6.3.16",null,null,"BUCHA COM ARRUELA EM LIGA ESPECIAL ZAMAK P/ELETRODUTO 25MM, D=1\"","SERV","UNID.",null,null,0,{"$f":"IF( $G85 <> \"\",\nTRUNC( $H85 * $I85, 2 ),\nSUMIFS( $K86:$K$520,\n          $B86:$B$520, $B85 & \".*\",\n          $B86:$B$520, \"<>\" & $B85 & \".*.*\"\n) )","v":0},{"$f":"IF( $G85 <> \"\",\n     TRUNC( $H85 * $J85, 2 ),\n     SUMIFS( $L86:$L$520,\n              $B86:$B$520, $B85 & \".*\",\n              $B86:$B$520, \"<>\" & $B85 & \".*.*\"\n     ) )","v":0}]
[null,"6.3.17",null,null,"FORNECIMENTO E INSTALAÇÃO DE SAÍDA HORIZONTAL PARA ELETRODUTO 1\" (REF. VL 33 VALEMAM OU SIMILAR)","SERV","UNID.",null,null,0,{"$f":"IF( $G86 <> \"\",\nTRUNC( $H86 * $I86, 2 ),\nSUMIFS( $K87:$K$520,\n          $B87:$B$520, $B86 & \".*\",\n          $B87:$B$520, \"<>\" & $B86 & \".*.*\"\n) )","v":0},{"$f":"IF( $G86 <> \"\",\n     TRUNC( $H86 * $J86, 2 ),\n     SUMIFS( $L87:$L$520,\n              $B87:$B$520, $B86 & \".*\",\n              $B87:$B$520, \"<>\" & $B86 & \".*.*\"\n     ) )","v":0}]
[null,"6.3.18",null,null,"FORNECIMENTO E INSTALAÇÃO DE SAÍDA HORIZONTAL PARA ELETRODUTO 3/4\" (REF. VL 33 VALEMAM OU SIMILAR)","SERV","UNID.",null,null,0,{"$f":"IF( $G87 <> \"\",\nTRUNC( $H87 * $I87, 2 ),\nSUMIFS( $K88:$K$520,\n          $B88:$B$520, $B87 & \".*\",\n          $B88:$B$520, \"<>\" & $B87 & \".*.*\"\n) )","v":0},{"$f":"IF( $G87 <> \"\",\n     TRUNC( $H87 * $J87, 2 ),\n     SUMIFS( $L88:$L$520,\n              $B88:$B$520, $B87 & \".*\",\n              $B88:$B$520, \"<>\" & $B87 & \".*.*\"\n     ) )","v":0}]
[null,"6.3.19",null,null,"FORNECIMENTO E INSTALAÇÃO DE MÃO FRANCESA SIMPLES 200 MM","SERV","UNID.",null,null,0,{"$f":"IF( $G88 <> \"\",\nTRUNC( $H88 * $I88, 2 ),\nSUMIFS( $K89:$K$520,\n          $B89:$B$520, $B88 & \".*\",\n          $B89:$B$520, \"<>\" & $B88 & \".*.*\"\n) )","v":0},{"$f":"IF( $G88 <> \"\",\n     TRUNC( $H88 * $J88, 2 ),\n     SUMIFS( $L89:$L$520,\n              $B89:$B$520, $B88 & \".*\",\n              $B89:$B$520, \"<>\" & $B88 & \".*.*\"\n     ) )","v":0}]
[null,"6.3.20",null,null,"BUCHA DE NYLON SEM ABA S8","FORN","UNID.",null,null,0,{"$f":"IF( $G89 <> \"\",\nTRUNC( $H89 * $I89, 2 ),\nSUMIFS( $K90:$K$520,\n          $B90:$B$520, $B89 & \".*\",\n          $B90:$B$520, \"<>\" & $B89 & \".*.*\"\n) )","v":0},{"$f":"IF( $G89 <> \"\",\n     TRUNC( $H89 * $J89, 2 ),\n     SUMIFS( $L90:$L$520,\n              $B90:$B$520, $B89 & \".*\",\n              $B90:$B$520, \"<>\" & $B89 & \".*.*\"\n     ) )","v":0}]
[null,"6.3.21",null,null,"BUCHA DE NYLON SEM ABA S4","FORN","UNID.",null,null,0,{"$f":"IF( $G90 <> \"\",\nTRUNC( $H90 * $I90, 2 ),\nSUMIFS( $K91:$K$520,\n          $B91:$B$520, $B90 & \".*\",\n          $B91:$B$520, \"<>\" & $B90 & \".*.*\"\n) )","v":0},{"$f":"IF( $G90 <> \"\",\n     TRUNC( $H90 * $J90, 2 ),\n     SUMIFS( $L91:$L$520,\n              $B91:$B$520, $B90 & \".*\",\n              $B91:$B$520, \"<>\" & $B90 & \".*.*\"\n     ) )","v":0}]
[null,"6.3.22",null,null,"FORNECIMENTO E INSTALAÇÃO DE PARAFUSO CABEÇA CHATA ROSCA SOBERBAL 6,10 X 65MM, COM BUCHA DE NYLON S10 SEM ABAS","SERV","UNID.",null,null,0,{"$f":"IF( $G91 <> \"\",\nTRUNC( $H91 * $I91, 2 ),\nSUMIFS( $K92:$K$520,\n          $B92:$B$520, $B91 & \".*\",\n          $B92:$B$520, \"<>\" & $B91 & \".*.*\"\n) )","v":0},{"$f":"IF( $G91 <> \"\",\n     TRUNC( $H91 * $J91, 2 ),\n     SUMIFS( $L92:$L$520,\n              $B92:$B$520, $B91 & \".*\",\n              $B92:$B$520, \"<>\" & $B91 & \".*.*\"\n     ) )","v":0}]
[null,"6.3.23",null,null,"BUCHA DE NYLON SEM ABA S10, COM PARAFUSO DE 6,10 X 65 MM EM ACO ZINCADO COM ROSCA SOBERBA, CABECA CHATA E FENDA PHILLIPS","FORN","UNID.",null,null,0,{"$f":"IF( $G92 <> \"\",\nTRUNC( $H92 * $I92, 2 ),\nSUMIFS( $K93:$K$520,\n          $B93:$B$520, $B92 & \".*\",\n          $B93:$B$520, \"<>\" & $B92 & \".*.*\"\n) )","v":0},{"$f":"IF( $G92 <> \"\",\n     TRUNC( $H92 * $J92, 2 ),\n     SUMIFS( $L93:$L$520,\n              $B93:$B$520, $B92 & \".*\",\n              $B93:$B$520, \"<>\" & $B92 & \".*.*\"\n     ) )","v":0}]
[null,"6.3.24",null,null,"PORCA ZINCADA, SEXTAVADA, DIAMETRO 1/4\"","FORN","UNID.",null,null,0,{"$f":"IF( $G93 <> \"\",\nTRUNC( $H93 * $I93, 2 ),\nSUMIFS( $K94:$K$520,\n          $B94:$B$520, $B93 & \".*\",\n          $B94:$B$520, \"<>\" & $B93 & \".*.*\"\n) )","v":0},{"$f":"IF( $G93 <> \"\",\n     TRUNC( $H93 * $J93, 2 ),\n     SUMIFS( $L94:$L$520,\n              $B94:$B$520, $B93 & \".*\",\n              $B94:$B$520, \"<>\" & $B93 & \".*.*\"\n     ) )","v":0}]
[null,"6.3.25",null,null,"PARAFUSO FENDA EM AÇO INOX AUTO-ATARRACHANTE D=4,2 X 32MM, REF:TEL-5333","FORN","UNID.",null,null,0,{"$f":"IF( $G94 <> \"\",\nTRUNC( $H94 * $I94, 2 ),\nSUMIFS( $K95:$K$520,\n          $B95:$B$520, $B94 & \".*\",\n          $B95:$B$520, \"<>\" & $B94 & \".*.*\"\n) )","v":0},{"$f":"IF( $G94 <> \"\",\n     TRUNC( $H94 * $J94, 2 ),\n     SUMIFS( $L95:$L$520,\n              $B95:$B$520, $B94 & \".*\",\n              $B95:$B$520, \"<>\" & $B94 & \".*.*\"\n     ) )","v":0}]
[null,"6.3.26",null,null,"ARRUELA DE PRESSÃO 1/4\"","SERV","UNID.",null,null,0,{"$f":"IF( $G95 <> \"\",\nTRUNC( $H95 * $I95, 2 ),\nSUMIFS( $K96:$K$520,\n          $B96:$B$520, $B95 & \".*\",\n          $B96:$B$520, \"<>\" & $B95 & \".*.*\"\n) )","v":0},{"$f":"IF( $G95 <> \"\",\n     TRUNC( $H95 * $J95, 2 ),\n     SUMIFS( $L96:$L$520,\n              $B96:$B$520, $B95 & \".*\",\n              $B96:$B$520, \"<>\" & $B95 & \".*.*\"\n     ) )","v":0}]
[null,"6.3.27",null,null,"ARRUELA LISA ZINCADA D=1/4\"","SERV","UNID.",null,null,0,{"$f":"IF( $G96 <> \"\",\nTRUNC( $H96 * $I96, 2 ),\nSUMIFS( $K97:$K$520,\n          $B97:$B$520, $B96 & \".*\",\n          $B97:$B$520, \"<>\" & $B96 & \".*.*\"\n) )","v":0},{"$f":"IF( $G96 <> \"\",\n     TRUNC( $H96 * $J96, 2 ),\n     SUMIFS( $L97:$L$520,\n              $B97:$B$520, $B96 & \".*\",\n              $B97:$B$520, \"<>\" & $B96 & \".*.*\"\n     ) )","v":0}]
[null,"6.3.28",null,null,"CABO DE COBRE ISOLADO, 10 MM², ANTI-CHAMA 450/750 V, INSTALADO EM ELETROCALHA OU PERFILADO - FORNECIMENTO E INSTALAÇÃO. AF_10/2020","SERV","M",null,null,0,{"$f":"IF( $G97 <> \"\",\nTRUNC( $H97 * $I97, 2 ),\nSUMIFS( $K98:$K$520,\n          $B98:$B$520, $B97 & \".*\",\n          $B98:$B$520, \"<>\" & $B97 & \".*.*\"\n) )","v":0},{"$f":"IF( $G97 <> \"\",\n     TRUNC( $H97 * $J97, 2 ),\n     SUMIFS( $L98:$L$520,\n              $B98:$B$520, $B97 & \".*\",\n              $B98:$B$520, \"<>\" & $B97 & \".*.*\"\n     ) )","v":0}]
[null,"6.3.29",null,null,"CABO DE COBRE ISOLADO, 16 MM², ANTI-CHAMA 450/750 V, INSTALADO EM ELETROCALHA OU PERFILADO - FORNECIMENTO E INSTALAÇÃO. AF_10/2020","SERV","M",null,null,0,{"$f":"IF( $G98 <> \"\",\nTRUNC( $H98 * $I98, 2 ),\nSUMIFS( $K99:$K$520,\n          $B99:$B$520, $B98 & \".*\",\n          $B99:$B$520, \"<>\" & $B98 & \".*.*\"\n) )","v":0},{"$f":"IF( $G98 <> \"\",\n     TRUNC( $H98 * $J98, 2 ),\n     SUMIFS( $L99:$L$520,\n              $B99:$B$520, $B98 & \".*\",\n              $B99:$B$520, \"<>\" & $B98 & \".*.*\"\n     ) )","v":0}]
[null,"6.3.30",null,null,"CABO DE COBRE FLEXÍVEL ISOLADO, 35 MM², ANTI-CHAMA 0,6/1,0 KV, PARA REDE ENTERRADA DE DISTRIBUIÇÃO DE ENERGIA ELÉTRICA - FORNECIMENTO E INSTALAÇÃO. AF_12/2021","SERV","M",null,null,0,{"$f":"IF( $G99 <> \"\",\nTRUNC( $H99 * $I99, 2 ),\nSUMIFS( $K100:$K$520,\n          $B100:$B$520, $B99 & \".*\",\n          $B100:$B$520, \"<>\" & $B99 & \".*.*\"\n) )","v":0},{"$f":"IF( $G99 <> \"\",\n     TRUNC( $H99 * $J99, 2 ),\n     SUMIFS( $L100:$L$520,\n              $B100:$B$520, $B99 & \".*\",\n              $B100:$B$520, \"<>\" & $B99 & \".*.*\"\n     ) )","v":0}]
[null,"6.4",null,null,"PROJETO ELÉTRICO BOX 01 A 100",{"$nulls":4},"",{"$f":"IF( $G100 <> \"\",\nTRUNC( $H100 * $I100, 2 ),\nSUMIFS( $K101:$K$520,\n          $B101:$B$520, $B100 & \".*\",\n          $B101:$B$520, \"<>\" & $B100 & \".*.*\"\n) )","v":0},{"$f":"IF( $G100 <> \"\",\n     TRUNC( $H100 * $J100, 2 ),\n     SUMIFS( $L101:$L$520,\n              $B101:$B$520, $B100 & \".*\",\n              $B101:$B$520, \"<>\" & $B100 & \".*.*\"\n     ) )","v":0}]
[null,"6.4.1",null,null,"PERFILADO, PRÉ-ZINCADO  A FOGO, PERFURADO 38 X 38 X 6000MM","SERV","UNID.",null,null,0,{"$f":"IF( $G101 <> \"\",\nTRUNC( $H101 * $I101, 2 ),\nSUMIFS( $K102:$K$520,\n          $B102:$B$520, $B101 & \".*\",\n          $B102:$B$520, \"<>\" & $B101 & \".*.*\"\n) )","v":0},{"$f":"IF( $G101 <> \"\",\n     TRUNC( $H101 * $J101, 2 ),\n     SUMIFS( $L102:$L$520,\n              $B102:$B$520, $B101 & \".*\",\n              $B102:$B$520, \"<>\" & $B101 & \".*.*\"\n     ) )","v":0}]
[null,"6.4.2",null,null,"GANCHO CURTO PARA PERFILADO, ( REF.: MOPA OU SIMILAR)","SERV","UNID.",null,null,0,{"$f":"IF( $G102 <> \"\",\nTRUNC( $H102 * $I102, 2 ),\nSUMIFS( $K103:$K$520,\n          $B103:$B$520, $B102 & \".*\",\n          $B103:$B$520, \"<>\" & $B102 & \".*.*\"\n) )","v":0},{"$f":"IF( $G102 <> \"\",\n     TRUNC( $H102 * $J102, 2 ),\n     SUMIFS( $L103:$L$520,\n              $B103:$B$520, $B102 & \".*\",\n              $B103:$B$520, \"<>\" & $B102 & \".*.*\"\n     ) )","v":0}]
[null,"6.4.3",null,null,"FORNECIMENTO E INSTALAÇÃO DE SAÍDA HORIZONTAL PARA ELETRODUTO 3/4\" (REF. VL 33 VALEMAM OU SIMILAR)","SERV","UNID.",null,null,0,{"$f":"IF( $G103 <> \"\",\nTRUNC( $H103 * $I103, 2 ),\nSUMIFS( $K104:$K$520,\n          $B104:$B$520, $B103 & \".*\",\n          $B104:$B$520, \"<>\" & $B103 & \".*.*\"\n) )","v":0},{"$f":"IF( $G103 <> \"\",\n     TRUNC( $H103 * $J103, 2 ),\n     SUMIFS( $L104:$L$520,\n              $B104:$B$520, $B103 & \".*\",\n              $B104:$B$520, \"<>\" & $B103 & \".*.*\"\n     ) )","v":0}]
[null,"6.4.4",null,null,"FORNECIMENTO E INSTALAÇÃO DE SAÍDA HORIZONTAL PARA ELETRODUTO 1\" (REF. VL 33 VALEMAM OU SIMILAR)","SERV","UNID.",null,null,0,{"$f":"IF( $G104 <> \"\",\nTRUNC( $H104 * $I104, 2 ),\nSUMIFS( $K105:$K$520,\n          $B105:$B$520, $B104 & \".*\",\n          $B105:$B$520, \"<>\" & $B104 & \".*.*\"\n) )","v":0},{"$f":"IF( $G104 <> \"\",\n     TRUNC( $H104 * $J104, 2 ),\n     SUMIFS( $L105:$L$520,\n              $B105:$B$520, $B104 & \".*\",\n              $B105:$B$520, \"<>\" & $B104 & \".*.*\"\n     ) )","v":0}]
[null,"6.4.5",null,null,"EMENDA EXTERNA, PARA PERFILADO TIPO \"I\", 38 X 38 MM, REF. CKP 116 OU SIMILAR","SERV","UNID.",null,null,0,{"$f":"IF( $G105 <> \"\",\nTRUNC( $H105 * $I105, 2 ),\nSUMIFS( $K106:$K$520,\n          $B106:$B$520, $B105 & \".*\",\n          $B106:$B$520, \"<>\" & $B105 & \".*.*\"\n) )","v":0},{"$f":"IF( $G105 <> \"\",\n     TRUNC( $H105 * $J105, 2 ),\n     SUMIFS( $L106:$L$520,\n              $B106:$B$520, $B105 & \".*\",\n              $B106:$B$520, \"<>\" & $B105 & \".*.*\"\n     ) )","v":0}]
[null,"6.4.6",null,null,"JUNÇÃO INTERNA TIPO \"L\" PARA PERFILADO, REF. MOPA OU SIMILAR","FORN","UNID.",null,null,0,{"$f":"IF( $G106 <> \"\",\nTRUNC( $H106 * $I106, 2 ),\nSUMIFS( $K107:$K$520,\n          $B107:$B$520, $B106 & \".*\",\n          $B107:$B$520, \"<>\" & $B106 & \".*.*\"\n) )","v":0},{"$f":"IF( $G106 <> \"\",\n     TRUNC( $H106 * $J106, 2 ),\n     SUMIFS( $L107:$L$520,\n              $B107:$B$520, $B106 & \".*\",\n              $B107:$B$520, \"<>\" & $B106 & \".*.*\"\n     ) )","v":0}]
[null,"6.4.7",null,null,"CANTONEIRA \"ZZ\" PARA FIXAÇÃO DE  PERFILADO, REF. MOPA OU SIMILAR","SERV","UNID.",null,null,0,{"$f":"IF( $G107 <> \"\",\nTRUNC( $H107 * $I107, 2 ),\nSUMIFS( $K108:$K$520,\n          $B108:$B$520, $B107 & \".*\",\n          $B108:$B$520, \"<>\" & $B107 & \".*.*\"\n) )","v":0},{"$f":"IF( $G107 <> \"\",\n     TRUNC( $H107 * $J107, 2 ),\n     SUMIFS( $L108:$L$520,\n              $B108:$B$520, $B107 & \".*\",\n              $B108:$B$520, \"<>\" & $B107 & \".*.*\"\n     ) )","v":0}]
[null,"6.4.8",null,null,"EMENDA EXTERNA, PARA PERFILADO TIPO \"X\", 38 X 38 MM, REF. CKP 119 OU SIMILAR","SERV","UNID.",null,null,0,{"$f":"IF( $G108 <> \"\",\nTRUNC( $H108 * $I108, 2 ),\nSUMIFS( $K109:$K$520,\n          $B109:$B$520, $B108 & \".*\",\n          $B109:$B$520, \"<>\" & $B108 & \".*.*\"\n) )","v":0},{"$f":"IF( $G108 <> \"\",\n     TRUNC( $H108 * $J108, 2 ),\n     SUMIFS( $L109:$L$520,\n              $B109:$B$520, $B108 & \".*\",\n              $B109:$B$520, \"<>\" & $B108 & \".*.*\"\n     ) )","v":0}]
[null,"6.4.9",null,null,"INTERRUPTOR SIMPLES (1 MÓDULO), 10A/250V, INCLUINDO SUPORTE E PLACA - FORNECIMENTO E INSTALAÇÃO. AF_03/2023","SERV","UNID.",null,null,0,{"$f":"IF( $G109 <> \"\",\nTRUNC( $H109 * $I109, 2 ),\nSUMIFS( $K110:$K$520,\n          $B110:$B$520, $B109 & \".*\",\n          $B110:$B$520, \"<>\" & $B109 & \".*.*\"\n) )","v":0},{"$f":"IF( $G109 <> \"\",\n     TRUNC( $H109 * $J109, 2 ),\n     SUMIFS( $L110:$L$520,\n              $B110:$B$520, $B109 & \".*\",\n              $B110:$B$520, \"<>\" & $B109 & \".*.*\"\n     ) )","v":0}]
[null,"6.4.10",null,null,"TOMADA MÉDIA DE EMBUTIR (1 MÓDULO), 2P+T 10 A, INCLUINDO SUPORTE E PLACA - FORNECIMENTO E INSTALAÇÃO. AF_03/2023","SERV","UNID.",null,null,0,{"$f":"IF( $G110 <> \"\",\nTRUNC( $H110 * $I110, 2 ),\nSUMIFS( $K111:$K$520,\n          $B111:$B$520, $B110 & \".*\",\n          $B111:$B$520, \"<>\" & $B110 & \".*.*\"\n) )","v":0},{"$f":"IF( $G110 <> \"\",\n     TRUNC( $H110 * $J110, 2 ),\n     SUMIFS( $L111:$L$520,\n              $B111:$B$520, $B110 & \".*\",\n              $B111:$B$520, \"<>\" & $B110 & \".*.*\"\n     ) )","v":0}]
[null,"6.4.11",null,null,"TOMADA MÉDIA DE EMBUTIR (1 MÓDULO), 2P+T 20 A, INCLUINDO SUPORTE E PLACA - FORNECIMENTO E INSTALAÇÃO. AF_03/2023","SERV","UNID.",null,null,0,{"$f":"IF( $G111 <> \"\",\nTRUNC( $H111 * $I111, 2 ),\nSUMIFS( $K112:$K$520,\n          $B112:$B$520, $B111 & \".*\",\n          $B112:$B$520, \"<>\" & $B111 & \".*.*\"\n) )","v":0},{"$f":"IF( $G111 <> \"\",\n     TRUNC( $H111 * $J111, 2 ),\n     SUMIFS( $L112:$L$520,\n              $B112:$B$520, $B111 & \".*\",\n              $B112:$B$520, \"<>\" & $B111 & \".*.*\"\n     ) )","v":0}]
[null,"6.4.12",null,null,"CAIXA RETANGULAR 4\" X 2\" MÉDIA (1,30 M DO PISO), PVC, INSTALADA EM PAREDE - FORNECIMENTO E INSTALAÇÃO. AF_03/2023","SERV","UNID.",null,null,0,{"$f":"IF( $G112 <> \"\",\nTRUNC( $H112 * $I112, 2 ),\nSUMIFS( $K113:$K$520,\n          $B113:$B$520, $B112 & \".*\",\n          $B113:$B$520, \"<>\" & $B112 & \".*.*\"\n) )","v":0},{"$f":"IF( $G112 <> \"\",\n     TRUNC( $H112 * $J112, 2 ),\n     SUMIFS( $L113:$L$520,\n              $B113:$B$520, $B112 & \".*\",\n              $B113:$B$520, \"<>\" & $B112 & \".*.*\"\n     ) )","v":0}]
[null,"6.4.13",null,null,"FORNECIMENTO E INSTALAÇÃO DE ESPELHO PARA CAIXA VERTICAL 4\" X 2\" COM 02 SAÍDAS RJ-45 (KRONE OU SIMILAR)","SERV","UNID.",null,null,0,{"$f":"IF( $G113 <> \"\",\nTRUNC( $H113 * $I113, 2 ),\nSUMIFS( $K114:$K$520,\n          $B114:$B$520, $B113 & \".*\",\n          $B114:$B$520, \"<>\" & $B113 & \".*.*\"\n) )","v":0},{"$f":"IF( $G113 <> \"\",\n     TRUNC( $H113 * $J113, 2 ),\n     SUMIFS( $L114:$L$520,\n              $B114:$B$520, $B113 & \".*\",\n              $B114:$B$520, \"<>\" & $B113 & \".*.*\"\n     ) )","v":0}]
[null,"6.4.14",null,null,"FORNECIMENTO E INSTALAÇÃO DE ESPELHO PARA CAIXA 4\" X 2\" COM 01 SAÍDA RJ-45","SERV","UNID.",null,null,0,{"$f":"IF( $G114 <> \"\",\nTRUNC( $H114 * $I114, 2 ),\nSUMIFS( $K115:$K$520,\n          $B115:$B$520, $B114 & \".*\",\n          $B115:$B$520, \"<>\" & $B114 & \".*.*\"\n) )","v":0},{"$f":"IF( $G114 <> \"\",\n     TRUNC( $H114 * $J114, 2 ),\n     SUMIFS( $L115:$L$520,\n              $B115:$B$520, $B114 & \".*\",\n              $B115:$B$520, \"<>\" & $B114 & \".*.*\"\n     ) )","v":0}]
[null,"6.4.15",null,null,"LUMINÁRIA SOBREPOR QUADRADA  LED 24W*, 6500K G- LIGHT OU SIMILAR","SERV","UNID.",null,null,0,{"$f":"IF( $G115 <> \"\",\nTRUNC( $H115 * $I115, 2 ),\nSUMIFS( $K116:$K$520,\n          $B116:$B$520, $B115 & \".*\",\n          $B116:$B$520, \"<>\" & $B115 & \".*.*\"\n) )","v":0},{"$f":"IF( $G115 <> \"\",\n     TRUNC( $H115 * $J115, 2 ),\n     SUMIFS( $L116:$L$520,\n              $B116:$B$520, $B115 & \".*\",\n              $B116:$B$520, \"<>\" & $B115 & \".*.*\"\n     ) )","v":0}]
[null,"6.4.16",null,null,"ELETRODUTO RÍGIDO ROSCÁVEL, PVC, DN 32 MM (1\"), PARA CIRCUITOS TERMINAIS, INSTALADO EM FORRO - FORNECIMENTO E INSTALAÇÃO. AF_03/2023","SERV","M",null,null,0,{"$f":"IF( $G116 <> \"\",\nTRUNC( $H116 * $I116, 2 ),\nSUMIFS( $K117:$K$520,\n          $B117:$B$520, $B116 & \".*\",\n          $B117:$B$520, \"<>\" & $B116 & \".*.*\"\n) )","v":0},{"$f":"IF( $G116 <> \"\",\n     TRUNC( $H116 * $J116, 2 ),\n     SUMIFS( $L117:$L$520,\n              $B117:$B$520, $B116 & \".*\",\n              $B117:$B$520, \"<>\" & $B116 & \".*.*\"\n     ) )","v":0}]
[null,"6.4.17",null,null,"CURVA 90 GRAUS PARA ELETRODUTO, PVC, ROSCÁVEL, DN 32 MM (1\"), PARA CIRCUITOS TERMINAIS, INSTALADA EM FORRO - FORNECIMENTO E INSTALAÇÃO. AF_03/2023","SERV","UNID.",null,null,0,{"$f":"IF( $G117 <> \"\",\nTRUNC( $H117 * $I117, 2 ),\nSUMIFS( $K118:$K$520,\n          $B118:$B$520, $B117 & \".*\",\n          $B118:$B$520, \"<>\" & $B117 & \".*.*\"\n) )","v":0},{"$f":"IF( $G117 <> \"\",\n     TRUNC( $H117 * $J117, 2 ),\n     SUMIFS( $L118:$L$520,\n              $B118:$B$520, $B117 & \".*\",\n              $B118:$B$520, \"<>\" & $B117 & \".*.*\"\n     ) )","v":0}]
[null,"6.4.18",null,null,"LUVA PARA ELETRODUTO, PVC, ROSCÁVEL, DN 32 MM (1\"), PARA CIRCUITOS TERMINAIS, INSTALADA EM FORRO - FORNECIMENTO E INSTALAÇÃO. AF_03/2023","SERV","UNID.",null,null,0,{"$f":"IF( $G118 <> \"\",\nTRUNC( $H118 * $I118, 2 ),\nSUMIFS( $K119:$K$520,\n          $B119:$B$520, $B118 & \".*\",\n          $B119:$B$520, \"<>\" & $B118 & \".*.*\"\n) )","v":0},{"$f":"IF( $G118 <> \"\",\n     TRUNC( $H118 * $J118, 2 ),\n     SUMIFS( $L119:$L$520,\n              $B119:$B$520, $B118 & \".*\",\n              $B119:$B$520, \"<>\" & $B118 & \".*.*\"\n     ) )","v":0}]
[null,"6.4.19",null,null,"ELETRODUTO RÍGIDO ROSCÁVEL, PVC, DN 25 MM (3/4\"), PARA CIRCUITOS TERMINAIS, INSTALADO EM FORRO - FORNECIMENTO E INSTALAÇÃO. AF_03/2023","SERV","M",null,null,0,{"$f":"IF( $G119 <> \"\",\nTRUNC( $H119 * $I119, 2 ),\nSUMIFS( $K120:$K$520,\n          $B120:$B$520, $B119 & \".*\",\n          $B120:$B$520, \"<>\" & $B119 & \".*.*\"\n) )","v":0},{"$f":"IF( $G119 <> \"\",\n     TRUNC( $H119 * $J119, 2 ),\n     SUMIFS( $L120:$L$520,\n              $B120:$B$520, $B119 & \".*\",\n              $B120:$B$520, \"<>\" & $B119 & \".*.*\"\n     ) )","v":0}]
[null,"6.4.20",null,null,"CURVA 90 GRAUS PARA ELETRODUTO, PVC, ROSCÁVEL, DN 25 MM (3/4\"), PARA CIRCUITOS TERMINAIS, INSTALADA EM PAREDE - FORNECIMENTO E INSTALAÇÃO. AF_03/2023","SERV","UNID.",null,null,0,{"$f":"IF( $G120 <> \"\",\nTRUNC( $H120 * $I120, 2 ),\nSUMIFS( $K121:$K$520,\n          $B121:$B$520, $B120 & \".*\",\n          $B121:$B$520, \"<>\" & $B120 & \".*.*\"\n) )","v":0},{"$f":"IF( $G120 <> \"\",\n     TRUNC( $H120 * $J120, 2 ),\n     SUMIFS( $L121:$L$520,\n              $B121:$B$520, $B120 & \".*\",\n              $B121:$B$520, \"<>\" & $B120 & \".*.*\"\n     ) )","v":0}]
[null,"6.4.21",null,null,"LUVA PARA ELETRODUTO, PVC, ROSCÁVEL, DN 25 MM (3/4\"), PARA CIRCUITOS TERMINAIS, INSTALADA EM FORRO - FORNECIMENTO E INSTALAÇÃO. AF_03/2023","SERV","UNID.",null,null,0,{"$f":"IF( $G121 <> \"\",\nTRUNC( $H121 * $I121, 2 ),\nSUMIFS( $K122:$K$520,\n          $B122:$B$520, $B121 & \".*\",\n          $B122:$B$520, \"<>\" & $B121 & \".*.*\"\n) )","v":0},{"$f":"IF( $G121 <> \"\",\n     TRUNC( $H121 * $J121, 2 ),\n     SUMIFS( $L122:$L$520,\n              $B122:$B$520, $B121 & \".*\",\n              $B122:$B$520, \"<>\" & $B121 & \".*.*\"\n     ) )","v":0}]
[null,"6.4.22",null,null,"ABRACADEIRA EM ACO PARA AMARRACAO DE ELETRODUTOS, TIPO U SIMPLES, COM 3/4\"","FORN","UNID.",null,null,0,{"$f":"IF( $G122 <> \"\",\nTRUNC( $H122 * $I122, 2 ),\nSUMIFS( $K123:$K$520,\n          $B123:$B$520, $B122 & \".*\",\n          $B123:$B$520, \"<>\" & $B122 & \".*.*\"\n) )","v":0},{"$f":"IF( $G122 <> \"\",\n     TRUNC( $H122 * $J122, 2 ),\n     SUMIFS( $L123:$L$520,\n              $B123:$B$520, $B122 & \".*\",\n              $B123:$B$520, \"<>\" & $B122 & \".*.*\"\n     ) )","v":0}]
[null,"6.4.23",null,null,"FORNECIMENTO E INSTALAÇÃO DE PARAFUSO CABEÇA CHATA ROSCA SOBERBAL 6,10 X 65MM, COM BUCHA DE NYLON S10 SEM ABAS","SERV","UNID.",null,null,0,{"$f":"IF( $G123 <> \"\",\nTRUNC( $H123 * $I123, 2 ),\nSUMIFS( $K124:$K$520,\n          $B124:$B$520, $B123 & \".*\",\n          $B124:$B$520, \"<>\" & $B123 & \".*.*\"\n) )","v":0},{"$f":"IF( $G123 <> \"\",\n     TRUNC( $H123 * $J123, 2 ),\n     SUMIFS( $L124:$L$520,\n              $B124:$B$520, $B123 & \".*\",\n              $B124:$B$520, \"<>\" & $B123 & \".*.*\"\n     ) )","v":0}]
[null,"6.4.24",null,null,"BUCHA DE NYLON SEM ABA S10, COM PARAFUSO DE 6,10 X 65 MM EM ACO ZINCADO COM ROSCA SOBERBA, CABECA CHATA E FENDA PHILLIPS","FORN","UNID.",null,null,0,{"$f":"IF( $G124 <> \"\",\nTRUNC( $H124 * $I124, 2 ),\nSUMIFS( $K125:$K$520,\n          $B125:$B$520, $B124 & \".*\",\n          $B125:$B$520, \"<>\" & $B124 & \".*.*\"\n) )","v":0},{"$f":"IF( $G124 <> \"\",\n     TRUNC( $H124 * $J124, 2 ),\n     SUMIFS( $L125:$L$520,\n              $B125:$B$520, $B124 & \".*\",\n              $B125:$B$520, \"<>\" & $B124 & \".*.*\"\n     ) )","v":0}]
[null,"6.4.25",null,null,"ARRUELA DE PRESSÃO 1/4\"","SERV","UNID.",null,null,0,{"$f":"IF( $G125 <> \"\",\nTRUNC( $H125 * $I125, 2 ),\nSUMIFS( $K126:$K$520,\n          $B126:$B$520, $B125 & \".*\",\n          $B126:$B$520, \"<>\" & $B125 & \".*.*\"\n) )","v":0},{"$f":"IF( $G125 <> \"\",\n     TRUNC( $H125 * $J125, 2 ),\n     SUMIFS( $L126:$L$520,\n              $B126:$B$520, $B125 & \".*\",\n              $B126:$B$520, \"<>\" & $B125 & \".*.*\"\n     ) )","v":0}]
[null,"6.4.26",null,null,"ARRUELA LISA ZINCADA D=1/4\"","SERV","UNID.",null,null,0,{"$f":"IF( $G126 <> \"\",\nTRUNC( $H126 * $I126, 2 ),\nSUMIFS( $K127:$K$520,\n          $B127:$B$520, $B126 & \".*\",\n          $B127:$B$520, \"<>\" & $B126 & \".*.*\"\n) )","v":0},{"$f":"IF( $G126 <> \"\",\n     TRUNC( $H126 * $J126, 2 ),\n     SUMIFS( $L127:$L$520,\n              $B127:$B$520, $B126 & \".*\",\n              $B127:$B$520, \"<>\" & $B126 & \".*.*\"\n     ) )","v":0}]
[null,"6.4.27",null,null,"PORCA ZINCADA, SEXTAVADA, DIAMETRO 1/4\"","FORN","UNID.",null,null,0,{"$f":"IF( $G127 <> \"\",\nTRUNC( $H127 * $I127, 2 ),\nSUMIFS( $K128:$K$520,\n          $B128:$B$520, $B127 & \".*\",\n          $B128:$B$520, \"<>\" & $B127 & \".*.*\"\n) )","v":0},{"$f":"IF( $G127 <> \"\",\n     TRUNC( $H127 * $J127, 2 ),\n     SUMIFS( $L128:$L$520,\n              $B128:$B$520, $B127 & \".*\",\n              $B128:$B$520, \"<>\" & $B127 & \".*.*\"\n     ) )","v":0}]
[null,"6.4.28",null,null,"BUCHA DE NYLON SEM ABA S6","FORN","UNID.",null,null,0,{"$f":"IF( $G128 <> \"\",\nTRUNC( $H128 * $I128, 2 ),\nSUMIFS( $K129:$K$520,\n          $B129:$B$520, $B128 & \".*\",\n          $B129:$B$520, \"<>\" & $B128 & \".*.*\"\n) )","v":0},{"$f":"IF( $G128 <> \"\",\n     TRUNC( $H128 * $J128, 2 ),\n     SUMIFS( $L129:$L$520,\n              $B129:$B$520, $B128 & \".*\",\n              $B129:$B$520, \"<>\" & $B128 & \".*.*\"\n     ) )","v":0}]
[null,"6.4.29",null,null,"BUCHA DE NYLON SEM ABA S8","FORN","UNID.",null,null,0,{"$f":"IF( $G129 <> \"\",\nTRUNC( $H129 * $I129, 2 ),\nSUMIFS( $K130:$K$520,\n          $B130:$B$520, $B129 & \".*\",\n          $B130:$B$520, \"<>\" & $B129 & \".*.*\"\n) )","v":0},{"$f":"IF( $G129 <> \"\",\n     TRUNC( $H129 * $J129, 2 ),\n     SUMIFS( $L130:$L$520,\n              $B130:$B$520, $B129 & \".*\",\n              $B130:$B$520, \"<>\" & $B129 & \".*.*\"\n     ) )","v":0}]
[null,"6.4.30",null,null,"BUCHA DE NYLON SEM ABA S4","FORN","UNID.",null,null,0,{"$f":"IF( $G130 <> \"\",\nTRUNC( $H130 * $I130, 2 ),\nSUMIFS( $K131:$K$520,\n          $B131:$B$520, $B130 & \".*\",\n          $B131:$B$520, \"<>\" & $B130 & \".*.*\"\n) )","v":0},{"$f":"IF( $G130 <> \"\",\n     TRUNC( $H130 * $J130, 2 ),\n     SUMIFS( $L131:$L$520,\n              $B131:$B$520, $B130 & \".*\",\n              $B131:$B$520, \"<>\" & $B130 & \".*.*\"\n     ) )","v":0}]
[null,"6.4.31",null,null,"VERGALHAO ZINCADO ROSCA TOTAL, 1/4\" (6,3 MM)","FORN","M",null,null,0,{"$f":"IF( $G131 <> \"\",\nTRUNC( $H131 * $I131, 2 ),\nSUMIFS( $K132:$K$520,\n          $B132:$B$520, $B131 & \".*\",\n          $B132:$B$520, \"<>\" & $B131 & \".*.*\"\n) )","v":0},{"$f":"IF( $G131 <> \"\",\n     TRUNC( $H131 * $J131, 2 ),\n     SUMIFS( $L132:$L$520,\n              $B132:$B$520, $B131 & \".*\",\n              $B132:$B$520, \"<>\" & $B131 & \".*.*\"\n     ) )","v":0}]
[null,"6.4.32",null,null,"CABO DE COBRE FLEXÍVEL ISOLADO, 2,5 MM², ANTI-CHAMA 0,6/1,0 KV, PARA CIRCUITOS TERMINAIS - FORNECIMENTO E INSTALAÇÃO. AF_03/2023","SERV","M",null,null,0,{"$f":"IF( $G132 <> \"\",\nTRUNC( $H132 * $I132, 2 ),\nSUMIFS( $K133:$K$520,\n          $B133:$B$520, $B132 & \".*\",\n          $B133:$B$520, \"<>\" & $B132 & \".*.*\"\n) )","v":0},{"$f":"IF( $G132 <> \"\",\n     TRUNC( $H132 * $J132, 2 ),\n     SUMIFS( $L133:$L$520,\n              $B133:$B$520, $B132 & \".*\",\n              $B133:$B$520, \"<>\" & $B132 & \".*.*\"\n     ) )","v":0}]
[null,"6.4.33",null,null,"CABO DE COBRE FLEXÍVEL ISOLADO, 4 MM², ANTI-CHAMA 0,6/1,0 KV, PARA CIRCUITOS TERMINAIS - FORNECIMENTO E INSTALAÇÃO. AF_03/2023","SERV","M",null,null,0,{"$f":"IF( $G133 <> \"\",\nTRUNC( $H133 * $I133, 2 ),\nSUMIFS( $K134:$K$520,\n          $B134:$B$520, $B133 & \".*\",\n          $B134:$B$520, \"<>\" & $B133 & \".*.*\"\n) )","v":0},{"$f":"IF( $G133 <> \"\",\n     TRUNC( $H133 * $J133, 2 ),\n     SUMIFS( $L134:$L$520,\n              $B134:$B$520, $B133 & \".*\",\n              $B134:$B$520, \"<>\" & $B133 & \".*.*\"\n     ) )","v":0}]
[null,"6.4.34",null,null,"QUADRO DE DISTRIBUIÇÃO DE ENERGIA EM CHAPA DE AÇO GALVANIZADO, DE EMBUTIR, COM BARRAMENTO TRIFÁSICO, PARA 12 DISJUNTORES DIN 100A - FORNECIMENTO E INSTALAÇÃO. AF_10/2020","SERV","UNID.",null,null,0,{"$f":"IF( $G134 <> \"\",\nTRUNC( $H134 * $I134, 2 ),\nSUMIFS( $K135:$K$520,\n          $B135:$B$520, $B134 & \".*\",\n          $B135:$B$520, \"<>\" & $B134 & \".*.*\"\n) )","v":0},{"$f":"IF( $G134 <> \"\",\n     TRUNC( $H134 * $J134, 2 ),\n     SUMIFS( $L135:$L$520,\n              $B135:$B$520, $B134 & \".*\",\n              $B135:$B$520, \"<>\" & $B134 & \".*.*\"\n     ) )","v":0}]
[null,"6.4.35",null,null,"DISJUNTOR MONOPOLAR TIPO DIN, CORRENTE NOMINAL DE 20A - FORNECIMENTO E INSTALAÇÃO. AF_10/2020","SERV","UNID.",null,null,0,{"$f":"IF( $G135 <> \"\",\nTRUNC( $H135 * $I135, 2 ),\nSUMIFS( $K136:$K$520,\n          $B136:$B$520, $B135 & \".*\",\n          $B136:$B$520, \"<>\" & $B135 & \".*.*\"\n) )","v":0},{"$f":"IF( $G135 <> \"\",\n     TRUNC( $H135 * $J135, 2 ),\n     SUMIFS( $L136:$L$520,\n              $B136:$B$520, $B135 & \".*\",\n              $B136:$B$520, \"<>\" & $B135 & \".*.*\"\n     ) )","v":0}]
[null,"6.4.36",null,null,"DISJUNTOR MONOPOLAR TIPO DIN, CORRENTE NOMINAL DE 16A - FORNECIMENTO E INSTALAÇÃO. AF_10/2020","SERV","UNID.",null,null,0,{"$f":"IF( $G136 <> \"\",\nTRUNC( $H136 * $I136, 2 ),\nSUMIFS( $K137:$K$520,\n          $B137:$B$520, $B136 & \".*\",\n          $B137:$B$520, \"<>\" & $B136 & \".*.*\"\n) )","v":0},{"$f":"IF( $G136 <> \"\",\n     TRUNC( $H136 * $J136, 2 ),\n     SUMIFS( $L137:$L$520,\n              $B137:$B$520, $B136 & \".*\",\n              $B137:$B$520, \"<>\" & $B136 & \".*.*\"\n     ) )","v":0}]
[null,"6.4.37",null,null,"DISJUNTOR MONOPOLAR TIPO DIN, CORRENTE NOMINAL DE 32A - FORNECIMENTO E INSTALAÇÃO. AF_10/2020","SERV","UNID.",null,null,{"$f":"IF(F137<>\"\",\nTRUNC(IF(F137=\"SERV\",I137*(1+$L$5/100),I137*(1+$L$6/100)),2),\n\"\" )","v":0},{"$f":"IF( $G137 <> \"\",\nTRUNC( $H137 * $I137, 2 ),\nSUMIFS( $K138:$K$520,\n          $B138:$B$520, $B137 & \".*\",\n          $B138:$B$520, \"<>\" & $B137 & \".*.*\"\n) )","v":0},{"$f":"IF( $G137 <> \"\",\n     TRUNC( $H137 * $J137, 2 ),\n     SUMIFS( $L138:$L$520,\n              $B138:$B$520, $B137 & \".*\",\n              $B138:$B$520, \"<>\" & $B137 & \".*.*\"\n     ) )","v":0}]
[null,"6.4.38",null,null,"INTERRUPTOR DIFERENCIAL RESIDUAL - IDR 4P DR 2X40A/30MA","SERV","UNID.",null,null,0,{"$f":"IF( $G138 <> \"\",\nTRUNC( $H138 * $I138, 2 ),\nSUMIFS( $K139:$K$520,\n          $B139:$B$520, $B138 & \".*\",\n          $B139:$B$520, \"<>\" & $B138 & \".*.*\"\n) )","v":0},{"$f":"IF( $G138 <> \"\",\n     TRUNC( $H138 * $J138, 2 ),\n     SUMIFS( $L139:$L$520,\n              $B139:$B$520, $B138 & \".*\",\n              $B139:$B$520, \"<>\" & $B138 & \".*.*\"\n     ) )","v":0}]
[null,"6.4.39",null,null,"BARRAMENTO NEUTRO E TERRA PARA QUADRO DE DISTRIBUIÇÃO","FORN","UNID.",null,null,0,{"$f":"IF( $G139 <> \"\",\nTRUNC( $H139 * $I139, 2 ),\nSUMIFS( $K140:$K$520,\n          $B140:$B$520, $B139 & \".*\",\n          $B140:$B$520, \"<>\" & $B139 & \".*.*\"\n) )","v":0},{"$f":"IF( $G139 <> \"\",\n     TRUNC( $H139 * $J139, 2 ),\n     SUMIFS( $L140:$L$520,\n              $B140:$B$520, $B139 & \".*\",\n              $B140:$B$520, \"<>\" & $B139 & \".*.*\"\n     ) )","v":0}]
[null,"6.4.40",null,null,"PLACA ADVERTÊNCIA 470 X 340MM, METÁLICA ( PERIGO DE MORTE )","FORN","UNID.",null,null,0,{"$f":"IF( $G140 <> \"\",\nTRUNC( $H140 * $I140, 2 ),\nSUMIFS( $K141:$K$520,\n          $B141:$B$520, $B140 & \".*\",\n          $B141:$B$520, \"<>\" & $B140 & \".*.*\"\n) )","v":0},{"$f":"IF( $G140 <> \"\",\n     TRUNC( $H140 * $J140, 2 ),\n     SUMIFS( $L141:$L$520,\n              $B141:$B$520, $B140 & \".*\",\n              $B141:$B$520, \"<>\" & $B140 & \".*.*\"\n     ) )","v":0}]
[null,"6.5",null,null,"PROJETO ELÉTRICO CIRCULAÇÃO COMUM E ÁREAS COMUNS",{"$nulls":4},"",{"$f":"IF( $G141 <> \"\",\nTRUNC( $H141 * $I141, 2 ),\nSUMIFS( $K142:$K$520,\n          $B142:$B$520, $B141 & \".*\",\n          $B142:$B$520, \"<>\" & $B141 & \".*.*\"\n) )","v":0},{"$f":"IF( $G141 <> \"\",\n     TRUNC( $H141 * $J141, 2 ),\n     SUMIFS( $L142:$L$520,\n              $B142:$B$520, $B141 & \".*\",\n              $B142:$B$520, \"<>\" & $B141 & \".*.*\"\n     ) )","v":0}]
[null,"6.5.1",null,null,"PERFILADO, PRÉ-ZINCADO  A FOGO, PERFURADO 38 X 38 X 6000MM","SERV","UNID.",null,null,0,{"$f":"IF( $G142 <> \"\",\nTRUNC( $H142 * $I142, 2 ),\nSUMIFS( $K143:$K$520,\n          $B143:$B$520, $B142 & \".*\",\n          $B143:$B$520, \"<>\" & $B142 & \".*.*\"\n) )","v":0},{"$f":"IF( $G142 <> \"\",\n     TRUNC( $H142 * $J142, 2 ),\n     SUMIFS( $L143:$L$520,\n              $B143:$B$520, $B142 & \".*\",\n              $B143:$B$520, \"<>\" & $B142 & \".*.*\"\n     ) )","v":0}]
[null,"6.5.2",null,null,"GANCHO CURTO PARA PERFILADO, ( REF.: MOPA OU SIMILAR)","SERV","UNID.",null,null,0,{"$f":"IF( $G143 <> \"\",\nTRUNC( $H143 * $I143, 2 ),\nSUMIFS( $K144:$K$520,\n          $B144:$B$520, $B143 & \".*\",\n          $B144:$B$520, \"<>\" & $B143 & \".*.*\"\n) )","v":0},{"$f":"IF( $G143 <> \"\",\n     TRUNC( $H143 * $J143, 2 ),\n     SUMIFS( $L144:$L$520,\n              $B144:$B$520, $B143 & \".*\",\n              $B144:$B$520, \"<>\" & $B143 & \".*.*\"\n     ) )","v":0}]
[null,"6.5.3",null,null,"FORNECIMENTO E INSTALAÇÃO DE SAÍDA HORIZONTAL PARA ELETRODUTO 3/4\" (REF. VL 33 VALEMAM OU SIMILAR)","SERV","UNID.",null,null,0,{"$f":"IF( $G144 <> \"\",\nTRUNC( $H144 * $I144, 2 ),\nSUMIFS( $K145:$K$520,\n          $B145:$B$520, $B144 & \".*\",\n          $B145:$B$520, \"<>\" & $B144 & \".*.*\"\n) )","v":0},{"$f":"IF( $G144 <> \"\",\n     TRUNC( $H144 * $J144, 2 ),\n     SUMIFS( $L145:$L$520,\n              $B145:$B$520, $B144 & \".*\",\n              $B145:$B$520, \"<>\" & $B144 & \".*.*\"\n     ) )","v":0}]
[null,"6.5.4",null,null,"FORNECIMENTO E INSTALAÇÃO DE SAÍDA HORIZONTAL PARA ELETRODUTO 1\" (REF. VL 33 VALEMAM OU SIMILAR)","SERV","UNID.",null,null,0,{"$f":"IF( $G145 <> \"\",\nTRUNC( $H145 * $I145, 2 ),\nSUMIFS( $K146:$K$520,\n          $B146:$B$520, $B145 & \".*\",\n          $B146:$B$520, \"<>\" & $B145 & \".*.*\"\n) )","v":0},{"$f":"IF( $G145 <> \"\",\n     TRUNC( $H145 * $J145, 2 ),\n     SUMIFS( $L146:$L$520,\n              $B146:$B$520, $B145 & \".*\",\n              $B146:$B$520, \"<>\" & $B145 & \".*.*\"\n     ) )","v":0}]
[null,"6.5.5",null,null,"JUNÇÃO INTERNA TIPO \"L\" PARA PERFILADO, REF. MOPA OU SIMILAR","FORN","UNID.",null,null,0,{"$f":"IF( $G146 <> \"\",\nTRUNC( $H146 * $I146, 2 ),\nSUMIFS( $K147:$K$520,\n          $B147:$B$520, $B146 & \".*\",\n          $B147:$B$520, \"<>\" & $B146 & \".*.*\"\n) )","v":0},{"$f":"IF( $G146 <> \"\",\n     TRUNC( $H146 * $J146, 2 ),\n     SUMIFS( $L147:$L$520,\n              $B147:$B$520, $B146 & \".*\",\n              $B147:$B$520, \"<>\" & $B146 & \".*.*\"\n     ) )","v":0}]
[null,"6.5.6",null,null,"CANTONEIRA \"ZZ\" PARA FIXAÇÃO DE  PERFILADO, REF. MOPA OU SIMILAR","SERV","UNID.",null,null,0,{"$f":"IF( $G147 <> \"\",\nTRUNC( $H147 * $I147, 2 ),\nSUMIFS( $K148:$K$520,\n          $B148:$B$520, $B147 & \".*\",\n          $B148:$B$520, \"<>\" & $B147 & \".*.*\"\n) )","v":0},{"$f":"IF( $G147 <> \"\",\n     TRUNC( $H147 * $J147, 2 ),\n     SUMIFS( $L148:$L$520,\n              $B148:$B$520, $B147 & \".*\",\n              $B148:$B$520, \"<>\" & $B147 & \".*.*\"\n     ) )","v":0}]
[null,"6.5.7",null,null,"EMENDA EXTERNA, PARA PERFILADO TIPO \"X\", 38 X 38 MM, REF. CKP 119 OU SIMILAR","SERV","UNID.",null,null,0,{"$f":"IF( $G148 <> \"\",\nTRUNC( $H148 * $I148, 2 ),\nSUMIFS( $K149:$K$520,\n          $B149:$B$520, $B148 & \".*\",\n          $B149:$B$520, \"<>\" & $B148 & \".*.*\"\n) )","v":0},{"$f":"IF( $G148 <> \"\",\n     TRUNC( $H148 * $J148, 2 ),\n     SUMIFS( $L149:$L$520,\n              $B149:$B$520, $B148 & \".*\",\n              $B149:$B$520, \"<>\" & $B148 & \".*.*\"\n     ) )","v":0}]
[null,"6.5.8",null,null,"ELETRODUTO RÍGIDO ROSCÁVEL, PVC, DN 25 MM (3/4\"), PARA CIRCUITOS TERMINAIS, INSTALADO EM FORRO - FORNECIMENTO E INSTALAÇÃO. AF_03/2023","SERV","M",null,null,0,{"$f":"IF( $G149 <> \"\",\nTRUNC( $H149 * $I149, 2 ),\nSUMIFS( $K150:$K$520,\n          $B150:$B$520, $B149 & \".*\",\n          $B150:$B$520, \"<>\" & $B149 & \".*.*\"\n) )","v":0},{"$f":"IF( $G149 <> \"\",\n     TRUNC( $H149 * $J149, 2 ),\n     SUMIFS( $L150:$L$520,\n              $B150:$B$520, $B149 & \".*\",\n              $B150:$B$520, \"<>\" & $B149 & \".*.*\"\n     ) )","v":0}]
[null,"6.5.9",null,null,"CURVA 90 GRAUS PARA ELETRODUTO, PVC, ROSCÁVEL, DN 25 MM (3/4\"), PARA CIRCUITOS TERMINAIS, INSTALADA EM PAREDE - FORNECIMENTO E INSTALAÇÃO. AF_03/2023","SERV","UNID.",null,null,0,{"$f":"IF( $G150 <> \"\",\nTRUNC( $H150 * $I150, 2 ),\nSUMIFS( $K151:$K$520,\n          $B151:$B$520, $B150 & \".*\",\n          $B151:$B$520, \"<>\" & $B150 & \".*.*\"\n) )","v":0},{"$f":"IF( $G150 <> \"\",\n     TRUNC( $H150 * $J150, 2 ),\n     SUMIFS( $L151:$L$520,\n              $B151:$B$520, $B150 & \".*\",\n              $B151:$B$520, \"<>\" & $B150 & \".*.*\"\n     ) )","v":0}]
[null,"6.5.10",null,null,"LUVA PARA ELETRODUTO, PVC, ROSCÁVEL, DN 25 MM (3/4\"), PARA CIRCUITOS TERMINAIS, INSTALADA EM FORRO - FORNECIMENTO E INSTALAÇÃO. AF_03/2023","SERV","UNID.",null,null,0,{"$f":"IF( $G151 <> \"\",\nTRUNC( $H151 * $I151, 2 ),\nSUMIFS( $K152:$K$520,\n          $B152:$B$520, $B151 & \".*\",\n          $B152:$B$520, \"<>\" & $B151 & \".*.*\"\n) )","v":0},{"$f":"IF( $G151 <> \"\",\n     TRUNC( $H151 * $J151, 2 ),\n     SUMIFS( $L152:$L$520,\n              $B152:$B$520, $B151 & \".*\",\n              $B152:$B$520, \"<>\" & $B151 & \".*.*\"\n     ) )","v":0}]
[null,"6.5.11",null,null,"ABRACADEIRA EM ACO PARA AMARRACAO DE ELETRODUTOS, TIPO U SIMPLES, COM 3/4\"","FORN","UNID.",null,null,0,{"$f":"IF( $G152 <> \"\",\nTRUNC( $H152 * $I152, 2 ),\nSUMIFS( $K153:$K$520,\n          $B153:$B$520, $B152 & \".*\",\n          $B153:$B$520, \"<>\" & $B152 & \".*.*\"\n) )","v":0},{"$f":"IF( $G152 <> \"\",\n     TRUNC( $H152 * $J152, 2 ),\n     SUMIFS( $L153:$L$520,\n              $B153:$B$520, $B152 & \".*\",\n              $B153:$B$520, \"<>\" & $B152 & \".*.*\"\n     ) )","v":0}]
[null,"6.5.12",null,null,"TALA PLANA PERFURADA 100MM PARA ELETROCALHA METÁLICA (REF.: MOPA OU SIMILAR) - REV 01","SERV","UNID.",null,null,0,{"$f":"IF( $G153 <> \"\",\nTRUNC( $H153 * $I153, 2 ),\nSUMIFS( $K154:$K$520,\n          $B154:$B$520, $B153 & \".*\",\n          $B154:$B$520, \"<>\" & $B153 & \".*.*\"\n) )","v":0},{"$f":"IF( $G153 <> \"\",\n     TRUNC( $H153 * $J153, 2 ),\n     SUMIFS( $L154:$L$520,\n              $B154:$B$520, $B153 & \".*\",\n              $B154:$B$520, \"<>\" & $B153 & \".*.*\"\n     ) )","v":0}]
[null,"6.5.13",null,null,"FLANGE 300X100MM PARA ELETROCALHA METÁLICA (REF. MOPA OU SIMILAR)","SERV","UNID.",null,null,0,{"$f":"IF( $G154 <> \"\",\nTRUNC( $H154 * $I154, 2 ),\nSUMIFS( $K155:$K$520,\n          $B155:$B$520, $B154 & \".*\",\n          $B155:$B$520, \"<>\" & $B154 & \".*.*\"\n) )","v":0},{"$f":"IF( $G154 <> \"\",\n     TRUNC( $H154 * $J154, 2 ),\n     SUMIFS( $L155:$L$520,\n              $B155:$B$520, $B154 & \".*\",\n              $B155:$B$520, \"<>\" & $B154 & \".*.*\"\n     ) )","v":0}]
[null,"6.5.14",null,null,"INTERRUPTOR SIMPLES (1 MÓDULO), 10A/250V, INCLUINDO SUPORTE E PLACA - FORNECIMENTO E INSTALAÇÃO. AF_03/2023","SERV","UNID.",null,null,0,{"$f":"IF( $G155 <> \"\",\nTRUNC( $H155 * $I155, 2 ),\nSUMIFS( $K156:$K$520,\n          $B156:$B$520, $B155 & \".*\",\n          $B156:$B$520, \"<>\" & $B155 & \".*.*\"\n) )","v":0},{"$f":"IF( $G155 <> \"\",\n     TRUNC( $H155 * $J155, 2 ),\n     SUMIFS( $L156:$L$520,\n              $B156:$B$520, $B155 & \".*\",\n              $B156:$B$520, \"<>\" & $B155 & \".*.*\"\n     ) )","v":0}]
[null,"6.5.15",null,null,"TOMADA MÉDIA DE EMBUTIR (1 MÓDULO), 2P+T 10 A, INCLUINDO SUPORTE E PLACA - FORNECIMENTO E INSTALAÇÃO. AF_03/2023","SERV","UNID.",null,null,0,{"$f":"IF( $G156 <> \"\",\nTRUNC( $H156 * $I156, 2 ),\nSUMIFS( $K157:$K$520,\n          $B157:$B$520, $B156 & \".*\",\n          $B157:$B$520, \"<>\" & $B156 & \".*.*\"\n) )","v":0},{"$f":"IF( $G156 <> \"\",\n     TRUNC( $H156 * $J156, 2 ),\n     SUMIFS( $L157:$L$520,\n              $B157:$B$520, $B156 & \".*\",\n              $B157:$B$520, \"<>\" & $B156 & \".*.*\"\n     ) )","v":0}]
[null,"6.5.16",null,null,"TOMADA MÉDIA DE EMBUTIR (1 MÓDULO), 2P+T 20 A, INCLUINDO SUPORTE E PLACA - FORNECIMENTO E INSTALAÇÃO. AF_03/2023","SERV","UNID.",null,null,0,{"$f":"IF( $G157 <> \"\",\nTRUNC( $H157 * $I157, 2 ),\nSUMIFS( $K158:$K$520,\n          $B158:$B$520, $B157 & \".*\",\n          $B158:$B$520, \"<>\" & $B157 & \".*.*\"\n) )","v":0},{"$f":"IF( $G157 <> \"\",\n     TRUNC( $H157 * $J157, 2 ),\n     SUMIFS( $L158:$L$520,\n              $B158:$B$520, $B157 & \".*\",\n              $B158:$B$520, \"<>\" & $B157 & \".*.*\"\n     ) )","v":0}]
[null,"6.5.17",null,null,"CAIXA RETANGULAR 4\" X 2\" MÉDIA (1,30 M DO PISO), PVC, INSTALADA EM PAREDE - FORNECIMENTO E INSTALAÇÃO. AF_03/2023","SERV","UNID.",null,null,0,{"$f":"IF( $G158 <> \"\",\nTRUNC( $H158 * $I158, 2 ),\nSUMIFS( $K159:$K$520,\n          $B159:$B$520, $B158 & \".*\",\n          $B159:$B$520, \"<>\" & $B158 & \".*.*\"\n) )","v":0},{"$f":"IF( $G158 <> \"\",\n     TRUNC( $H158 * $J158, 2 ),\n     SUMIFS( $L159:$L$520,\n              $B159:$B$520, $B158 & \".*\",\n              $B159:$B$520, \"<>\" & $B158 & \".*.*\"\n     ) )","v":0}]
[null,"6.5.18",null,null,"FORNECIMENTO E INSTALAÇÃO DE ESPELHO PARA CAIXA VERTICAL 4\" X 2\" COM 02 SAÍDAS RJ-45 (KRONE OU SIMILAR)","SERV","UNID.",null,null,0,{"$f":"IF( $G159 <> \"\",\nTRUNC( $H159 * $I159, 2 ),\nSUMIFS( $K160:$K$520,\n          $B160:$B$520, $B159 & \".*\",\n          $B160:$B$520, \"<>\" & $B159 & \".*.*\"\n) )","v":0},{"$f":"IF( $G159 <> \"\",\n     TRUNC( $H159 * $J159, 2 ),\n     SUMIFS( $L160:$L$520,\n              $B160:$B$520, $B159 & \".*\",\n              $B160:$B$520, \"<>\" & $B159 & \".*.*\"\n     ) )","v":0}]
[null,"6.5.19",null,null,"FORNECIMENTO E INSTALAÇÃO DE ESPELHO PARA CAIXA 4\" X 2\" COM 01 SAÍDA RJ-45","SERV","UNID.",null,null,0,{"$f":"IF( $G160 <> \"\",\nTRUNC( $H160 * $I160, 2 ),\nSUMIFS( $K161:$K$520,\n          $B161:$B$520, $B160 & \".*\",\n          $B161:$B$520, \"<>\" & $B160 & \".*.*\"\n) )","v":0},{"$f":"IF( $G160 <> \"\",\n     TRUNC( $H160 * $J160, 2 ),\n     SUMIFS( $L161:$L$520,\n              $B161:$B$520, $B160 & \".*\",\n              $B161:$B$520, \"<>\" & $B160 & \".*.*\"\n     ) )","v":0}]
[null,"6.5.20",null,null,"SENSOR DE PRESENÇA COM FOTOCÉLULA, FIXAÇÃO EM TETO - FORNECIMENTO E INSTALAÇÃO. AF_09/2024","SERV","UNID.",null,null,0,{"$f":"IF( $G161 <> \"\",\nTRUNC( $H161 * $I161, 2 ),\nSUMIFS( $K162:$K$520,\n          $B162:$B$520, $B161 & \".*\",\n          $B162:$B$520, \"<>\" & $B161 & \".*.*\"\n) )","v":0},{"$f":"IF( $G161 <> \"\",\n     TRUNC( $H161 * $J161, 2 ),\n     SUMIFS( $L162:$L$520,\n              $B162:$B$520, $B161 & \".*\",\n              $B162:$B$520, \"<>\" & $B161 & \".*.*\"\n     ) )","v":0}]
[null,"6.5.21",null,null,"LUMINÁRIA SOBREPOR QUADRADA  LED 24W*, 6500K G- LIGHT OU SIMILAR","SERV","UNID.",null,null,0,{"$f":"IF( $G162 <> \"\",\nTRUNC( $H162 * $I162, 2 ),\nSUMIFS( $K163:$K$520,\n          $B163:$B$520, $B162 & \".*\",\n          $B163:$B$520, \"<>\" & $B162 & \".*.*\"\n) )","v":0},{"$f":"IF( $G162 <> \"\",\n     TRUNC( $H162 * $J162, 2 ),\n     SUMIFS( $L163:$L$520,\n              $B163:$B$520, $B162 & \".*\",\n              $B163:$B$520, \"<>\" & $B162 & \".*.*\"\n     ) )","v":0}]
[null,"6.5.22",null,null,"LUMINÁRIA PLAFON (SOBREPOR) 22,5 X 22,5 - 18 W - 6000K - G- LIGHT OU SIMILAR","SERV","UNID.",null,null,0,{"$f":"IF( $G163 <> \"\",\nTRUNC( $H163 * $I163, 2 ),\nSUMIFS( $K164:$K$520,\n          $B164:$B$520, $B163 & \".*\",\n          $B164:$B$520, \"<>\" & $B163 & \".*.*\"\n) )","v":0},{"$f":"IF( $G163 <> \"\",\n     TRUNC( $H163 * $J163, 2 ),\n     SUMIFS( $L164:$L$520,\n              $B164:$B$520, $B163 & \".*\",\n              $B164:$B$520, \"<>\" & $B163 & \".*.*\"\n     ) )","v":0}]
[null,"6.5.23",null,null,"FORNECIMENTO E INSTALAÇÃO DE PARAFUSO CABEÇA CHATA ROSCA SOBERBAL 6,10 X 65MM, COM BUCHA DE NYLON S10 SEM ABAS","SERV","UNID.",null,null,0,{"$f":"IF( $G164 <> \"\",\nTRUNC( $H164 * $I164, 2 ),\nSUMIFS( $K165:$K$520,\n          $B165:$B$520, $B164 & \".*\",\n          $B165:$B$520, \"<>\" & $B164 & \".*.*\"\n) )","v":0},{"$f":"IF( $G164 <> \"\",\n     TRUNC( $H164 * $J164, 2 ),\n     SUMIFS( $L165:$L$520,\n              $B165:$B$520, $B164 & \".*\",\n              $B165:$B$520, \"<>\" & $B164 & \".*.*\"\n     ) )","v":0}]
[null,"6.5.24",null,null,"BUCHA DE NYLON SEM ABA S10, COM PARAFUSO DE 6,10 X 65 MM EM ACO ZINCADO COM ROSCA SOBERBA, CABECA CHATA E FENDA PHILLIPS","FORN","UNID.",null,null,0,{"$f":"IF( $G165 <> \"\",\nTRUNC( $H165 * $I165, 2 ),\nSUMIFS( $K166:$K$520,\n          $B166:$B$520, $B165 & \".*\",\n          $B166:$B$520, \"<>\" & $B165 & \".*.*\"\n) )","v":0},{"$f":"IF( $G165 <> \"\",\n     TRUNC( $H165 * $J165, 2 ),\n     SUMIFS( $L166:$L$520,\n              $B166:$B$520, $B165 & \".*\",\n              $B166:$B$520, \"<>\" & $B165 & \".*.*\"\n     ) )","v":0}]
[null,"6.5.25",null,null,"PARAFUSO FENDA EM AÇO INOX AUTO-ATARRACHANTE D=4,2 X 32MM, REF:TEL-5333","FORN","UNID.",null,null,0,{"$f":"IF( $G166 <> \"\",\nTRUNC( $H166 * $I166, 2 ),\nSUMIFS( $K167:$K$520,\n          $B167:$B$520, $B166 & \".*\",\n          $B167:$B$520, \"<>\" & $B166 & \".*.*\"\n) )","v":0},{"$f":"IF( $G166 <> \"\",\n     TRUNC( $H166 * $J166, 2 ),\n     SUMIFS( $L167:$L$520,\n              $B167:$B$520, $B166 & \".*\",\n              $B167:$B$520, \"<>\" & $B166 & \".*.*\"\n     ) )","v":0}]
[null,"6.5.26",null,null,"PARAFUSO DE ACO ZINCADO COM ROSCA SOBERBA, CABECA CHATA E FENDA SIMPLES, DIAMETRO 4,8 MM, COMPRIMENTO 45 MM","FORN","UNID.",null,null,0,{"$f":"IF( $G167 <> \"\",\nTRUNC( $H167 * $I167, 2 ),\nSUMIFS( $K168:$K$520,\n          $B168:$B$520, $B167 & \".*\",\n          $B168:$B$520, \"<>\" & $B167 & \".*.*\"\n) )","v":0},{"$f":"IF( $G167 <> \"\",\n     TRUNC( $H167 * $J167, 2 ),\n     SUMIFS( $L168:$L$520,\n              $B168:$B$520, $B167 & \".*\",\n              $B168:$B$520, \"<>\" & $B167 & \".*.*\"\n     ) )","v":0}]
[null,"6.5.27",null,null,"ARRUELA DE PRESSÃO 1/4\"","SERV","UNID.",null,null,0,{"$f":"IF( $G168 <> \"\",\nTRUNC( $H168 * $I168, 2 ),\nSUMIFS( $K169:$K$520,\n          $B169:$B$520, $B168 & \".*\",\n          $B169:$B$520, \"<>\" & $B168 & \".*.*\"\n) )","v":0},{"$f":"IF( $G168 <> \"\",\n     TRUNC( $H168 * $J168, 2 ),\n     SUMIFS( $L169:$L$520,\n              $B169:$B$520, $B168 & \".*\",\n              $B169:$B$520, \"<>\" & $B168 & \".*.*\"\n     ) )","v":0}]
[null,"6.5.28",null,null,"ARRUELA LISA ZINCADA D=1/4\"","SERV","UNID.",null,null,0,{"$f":"IF( $G169 <> \"\",\nTRUNC( $H169 * $I169, 2 ),\nSUMIFS( $K170:$K$520,\n          $B170:$B$520, $B169 & \".*\",\n          $B170:$B$520, \"<>\" & $B169 & \".*.*\"\n) )","v":0},{"$f":"IF( $G169 <> \"\",\n     TRUNC( $H169 * $J169, 2 ),\n     SUMIFS( $L170:$L$520,\n              $B170:$B$520, $B169 & \".*\",\n              $B170:$B$520, \"<>\" & $B169 & \".*.*\"\n     ) )","v":0}]
[null,"6.5.29",null,null,"PORCA ZINCADA, SEXTAVADA, DIAMETRO 1/4\"","FORN","UNID.",null,null,0,{"$f":"IF( $G170 <> \"\",\nTRUNC( $H170 * $I170, 2 ),\nSUMIFS( $K171:$K$520,\n          $B171:$B$520, $B170 & \".*\",\n          $B171:$B$520, \"<>\" & $B170 & \".*.*\"\n) )","v":0},{"$f":"IF( $G170 <> \"\",\n     TRUNC( $H170 * $J170, 2 ),\n     SUMIFS( $L171:$L$520,\n              $B171:$B$520, $B170 & \".*\",\n              $B171:$B$520, \"<>\" & $B170 & \".*.*\"\n     ) )","v":0}]
[null,"6.5.30",null,null,"BUCHA DE NYLON SEM ABA S8","FORN","UNID.",null,null,0,{"$f":"IF( $G171 <> \"\",\nTRUNC( $H171 * $I171, 2 ),\nSUMIFS( $K172:$K$520,\n          $B172:$B$520, $B171 & \".*\",\n          $B172:$B$520, \"<>\" & $B171 & \".*.*\"\n) )","v":0},{"$f":"IF( $G171 <> \"\",\n     TRUNC( $H171 * $J171, 2 ),\n     SUMIFS( $L172:$L$520,\n              $B172:$B$520, $B171 & \".*\",\n              $B172:$B$520, \"<>\" & $B171 & \".*.*\"\n     ) )","v":0}]
[null,"6.5.31",null,null,"BUCHA DE NYLON SEM ABA S4","FORN","UNID.",null,null,0,{"$f":"IF( $G172 <> \"\",\nTRUNC( $H172 * $I172, 2 ),\nSUMIFS( $K173:$K$520,\n          $B173:$B$520, $B172 & \".*\",\n          $B173:$B$520, \"<>\" & $B172 & \".*.*\"\n) )","v":0},{"$f":"IF( $G172 <> \"\",\n     TRUNC( $H172 * $J172, 2 ),\n     SUMIFS( $L173:$L$520,\n              $B173:$B$520, $B172 & \".*\",\n              $B173:$B$520, \"<>\" & $B172 & \".*.*\"\n     ) )","v":0}]
[null,"6.5.32",null,null,"BUCHA DE NYLON SEM ABA S6","FORN","UNID.",null,null,0,{"$f":"IF( $G173 <> \"\",\nTRUNC( $H173 * $I173, 2 ),\nSUMIFS( $K174:$K$520,\n          $B174:$B$520, $B173 & \".*\",\n          $B174:$B$520, \"<>\" & $B173 & \".*.*\"\n) )","v":0},{"$f":"IF( $G173 <> \"\",\n     TRUNC( $H173 * $J173, 2 ),\n     SUMIFS( $L174:$L$520,\n              $B174:$B$520, $B173 & \".*\",\n              $B174:$B$520, \"<>\" & $B173 & \".*.*\"\n     ) )","v":0}]
[null,"6.5.33",null,null,"VERGALHAO ZINCADO ROSCA TOTAL, 1/4\" (6,3 MM)","FORN","M",null,null,0,{"$f":"IF( $G174 <> \"\",\nTRUNC( $H174 * $I174, 2 ),\nSUMIFS( $K175:$K$520,\n          $B175:$B$520, $B174 & \".*\",\n          $B175:$B$520, \"<>\" & $B174 & \".*.*\"\n) )","v":0},{"$f":"IF( $G174 <> \"\",\n     TRUNC( $H174 * $J174, 2 ),\n     SUMIFS( $L175:$L$520,\n              $B175:$B$520, $B174 & \".*\",\n              $B175:$B$520, \"<>\" & $B174 & \".*.*\"\n     ) )","v":0}]
[null,"6.5.34",null,null,"CABO DE COBRE FLEXÍVEL ISOLADO, 2,5 MM², ANTI-CHAMA 0,6/1,0 KV, PARA CIRCUITOS TERMINAIS - FORNECIMENTO E INSTALAÇÃO. AF_03/2023","SERV","M",null,null,0,{"$f":"IF( $G175 <> \"\",\nTRUNC( $H175 * $I175, 2 ),\nSUMIFS( $K176:$K$520,\n          $B176:$B$520, $B175 & \".*\",\n          $B176:$B$520, \"<>\" & $B175 & \".*.*\"\n) )","v":0},{"$f":"IF( $G175 <> \"\",\n     TRUNC( $H175 * $J175, 2 ),\n     SUMIFS( $L176:$L$520,\n              $B176:$B$520, $B175 & \".*\",\n              $B176:$B$520, \"<>\" & $B175 & \".*.*\"\n     ) )","v":0}]
[null,"6.5.35",null,null,"CABO DE COBRE FLEXÍVEL ISOLADO, 10 MM², ANTI-CHAMA 0,6/1,0 KV, PARA CIRCUITOS TERMINAIS - FORNECIMENTO E INSTALAÇÃO. AF_03/2023","SERV","M",null,null,0,{"$f":"IF( $G176 <> \"\",\nTRUNC( $H176 * $I176, 2 ),\nSUMIFS( $K177:$K$520,\n          $B177:$B$520, $B176 & \".*\",\n          $B177:$B$520, \"<>\" & $B176 & \".*.*\"\n) )","v":0},{"$f":"IF( $G176 <> \"\",\n     TRUNC( $H176 * $J176, 2 ),\n     SUMIFS( $L177:$L$520,\n              $B177:$B$520, $B176 & \".*\",\n              $B177:$B$520, \"<>\" & $B176 & \".*.*\"\n     ) )","v":0}]
[null,"6.5.36",null,null,"DISJUNTOR MONOPOLAR TIPO DIN, CORRENTE NOMINAL DE 20A - FORNECIMENTO E INSTALAÇÃO. AF_10/2020","SERV","UNID.",null,null,0,{"$f":"IF( $G177 <> \"\",\nTRUNC( $H177 * $I177, 2 ),\nSUMIFS( $K178:$K$520,\n          $B178:$B$520, $B177 & \".*\",\n          $B178:$B$520, \"<>\" & $B177 & \".*.*\"\n) )","v":0},{"$f":"IF( $G177 <> \"\",\n     TRUNC( $H177 * $J177, 2 ),\n     SUMIFS( $L178:$L$520,\n              $B178:$B$520, $B177 & \".*\",\n              $B178:$B$520, \"<>\" & $B177 & \".*.*\"\n     ) )","v":0}]
[null,"6.5.37",null,null,"DISJUNTOR MONOPOLAR TIPO DIN, CORRENTE NOMINAL DE 16A - FORNECIMENTO E INSTALAÇÃO. AF_10/2020","SERV","UNID.",null,null,0,{"$f":"IF( $G178 <> \"\",\nTRUNC( $H178 * $I178, 2 ),\nSUMIFS( $K179:$K$520,\n          $B179:$B$520, $B178 & \".*\",\n          $B179:$B$520, \"<>\" & $B178 & \".*.*\"\n) )","v":0},{"$f":"IF( $G178 <> \"\",\n     TRUNC( $H178 * $J178, 2 ),\n     SUMIFS( $L179:$L$520,\n              $B179:$B$520, $B178 & \".*\",\n              $B179:$B$520, \"<>\" & $B178 & \".*.*\"\n     ) )","v":0}]
[null,"6.5.38",null,null,"DISJUNTOR TRIPOLAR TIPO DIN, CORRENTE NOMINAL DE 40A - FORNECIMENTO E INSTALAÇÃO. AF_10/2020","SERV","UNID.",null,null,0,{"$f":"IF( $G179 <> \"\",\nTRUNC( $H179 * $I179, 2 ),\nSUMIFS( $K180:$K$520,\n          $B180:$B$520, $B179 & \".*\",\n          $B180:$B$520, \"<>\" & $B179 & \".*.*\"\n) )","v":0},{"$f":"IF( $G179 <> \"\",\n     TRUNC( $H179 * $J179, 2 ),\n     SUMIFS( $L180:$L$520,\n              $B180:$B$520, $B179 & \".*\",\n              $B180:$B$520, \"<>\" & $B179 & \".*.*\"\n     ) )","v":0}]
[null,"6.5.39",null,null,"DISJUNTOR TRIPOLAR TIPO DIN, CORRENTE NOMINAL DE 16A - FORNECIMENTO E INSTALAÇÃO. AF_10/2020","SERV","UNID.",null,null,0,{"$f":"IF( $G180 <> \"\",\nTRUNC( $H180 * $I180, 2 ),\nSUMIFS( $K181:$K$520,\n          $B181:$B$520, $B180 & \".*\",\n          $B181:$B$520, \"<>\" & $B180 & \".*.*\"\n) )","v":0},{"$f":"IF( $G180 <> \"\",\n     TRUNC( $H180 * $J180, 2 ),\n     SUMIFS( $L181:$L$520,\n              $B181:$B$520, $B180 & \".*\",\n              $B181:$B$520, \"<>\" & $B180 & \".*.*\"\n     ) )","v":0}]
[null,"6.5.40",null,null,"DISJUNTOR TERMOMAGNÉTICO TRIPOLAR 125 A COM CAIXA MOLDADA 10 KA","SERV","UNID.",null,null,0,{"$f":"IF( $G181 <> \"\",\nTRUNC( $H181 * $I181, 2 ),\nSUMIFS( $K182:$K$520,\n          $B182:$B$520, $B181 & \".*\",\n          $B182:$B$520, \"<>\" & $B181 & \".*.*\"\n) )","v":0},{"$f":"IF( $G181 <> \"\",\n     TRUNC( $H181 * $J181, 2 ),\n     SUMIFS( $L182:$L$520,\n              $B182:$B$520, $B181 & \".*\",\n              $B182:$B$520, \"<>\" & $B181 & \".*.*\"\n     ) )","v":0}]
[null,"6.5.41",null,null,"INTERRUPTOR DIFERENCIAL RESIDUAL - IDR 2P DR 4X63A/30MA","SERV","UNID.",null,null,0,{"$f":"IF( $G182 <> \"\",\nTRUNC( $H182 * $I182, 2 ),\nSUMIFS( $K183:$K$520,\n          $B183:$B$520, $B182 & \".*\",\n          $B183:$B$520, \"<>\" & $B182 & \".*.*\"\n) )","v":0},{"$f":"IF( $G182 <> \"\",\n     TRUNC( $H182 * $J182, 2 ),\n     SUMIFS( $L183:$L$520,\n              $B183:$B$520, $B182 & \".*\",\n              $B183:$B$520, \"<>\" & $B182 & \".*.*\"\n     ) )","v":0}]
[null,"6.5.42",null,null,"LUMINÁRIA DO TIPO PENDENTE BOLA 30CM COM LÂMPADA DE LED 50W 4500K","SERV","UNID.",null,null,0,{"$f":"IF( $G183 <> \"\",\nTRUNC( $H183 * $I183, 2 ),\nSUMIFS( $K184:$K$520,\n          $B184:$B$520, $B183 & \".*\",\n          $B184:$B$520, \"<>\" & $B183 & \".*.*\"\n) )","v":0},{"$f":"IF( $G183 <> \"\",\n     TRUNC( $H183 * $J183, 2 ),\n     SUMIFS( $L184:$L$520,\n              $B184:$B$520, $B183 & \".*\",\n              $B184:$B$520, \"<>\" & $B183 & \".*.*\"\n     ) )","v":0}]
[null,"6.5.43",null,null,"QUADRO DE COMANDO C/ BARRAMENTOS ELÉTRICOS 15X2MM² TRIFÁSICO + N + T EM  ALUMÍNIO COR CINZA 80X60X25CM TINTURA ELETROSTÁTICA A PO, COM PLACA DE  MONTAGEM COR LARANJA ESPESSURA 1,2MM","SERV","UNID.",null,null,0,{"$f":"IF( $G184 <> \"\",\nTRUNC( $H184 * $I184, 2 ),\nSUMIFS( $K185:$K$520,\n          $B185:$B$520, $B184 & \".*\",\n          $B185:$B$520, \"<>\" & $B184 & \".*.*\"\n) )","v":0},{"$f":"IF( $G184 <> \"\",\n     TRUNC( $H184 * $J184, 2 ),\n     SUMIFS( $L185:$L$520,\n              $B185:$B$520, $B184 & \".*\",\n              $B185:$B$520, \"<>\" & $B184 & \".*.*\"\n     ) )","v":0}]
[null,"6.6",null,null,"PROJETO ELÉTRICO EXTERNO",{"$nulls":4},"",{"$f":"IF( $G185 <> \"\",\nTRUNC( $H185 * $I185, 2 ),\nSUMIFS( $K186:$K$520,\n          $B186:$B$520, $B185 & \".*\",\n          $B186:$B$520, \"<>\" & $B185 & \".*.*\"\n) )","v":0},{"$f":"IF( $G185 <> \"\",\n     TRUNC( $H185 * $J185, 2 ),\n     SUMIFS( $L186:$L$520,\n              $B186:$B$520, $B185 & \".*\",\n              $B186:$B$520, \"<>\" & $B185 & \".*.*\"\n     ) )","v":0}]
[null,"6.6.1",null,null,"CAIXA DE CONCRETO PRE MOLDADO PARA ATERRAMENTO, COM TAMPA, 40 X 40 X 40, E = 5CM","SERV","UNID.",null,null,0,{"$f":"IF( $G186 <> \"\",\nTRUNC( $H186 * $I186, 2 ),\nSUMIFS( $K187:$K$520,\n          $B187:$B$520, $B186 & \".*\",\n          $B187:$B$520, \"<>\" & $B186 & \".*.*\"\n) )","v":0},{"$f":"IF( $G186 <> \"\",\n     TRUNC( $H186 * $J186, 2 ),\n     SUMIFS( $L187:$L$520,\n              $B187:$B$520, $B186 & \".*\",\n              $B187:$B$520, \"<>\" & $B186 & \".*.*\"\n     ) )","v":0}]
[null,"6.6.2",null,null,"POSTE DECORATIVO 2 PÉTALAS, EM AÇO GALVANIZADO COM DIFUSOR EM VIDRO TRANSPARENTE TEMPERADO, COM 3M/4M, INCLUSIVE LÂMPADA DE LED 50W","SERV","UNID.",null,null,0,{"$f":"IF( $G187 <> \"\",\nTRUNC( $H187 * $I187, 2 ),\nSUMIFS( $K188:$K$520,\n          $B188:$B$520, $B187 & \".*\",\n          $B188:$B$520, \"<>\" & $B187 & \".*.*\"\n) )","v":0},{"$f":"IF( $G187 <> \"\",\n     TRUNC( $H187 * $J187, 2 ),\n     SUMIFS( $L188:$L$520,\n              $B188:$B$520, $B187 & \".*\",\n              $B188:$B$520, \"<>\" & $B187 & \".*.*\"\n     ) )","v":0}]
[null,"6.6.3",null,null,"POSTE DECORATIVO 1 PÉTALAS, EM AÇO GALVANIZADO COM DIFUSOR EM VIDRO TRANSPARENTE TEMPERADO, COM 3M/4M, INCLUSIVE LÂMPADA DE LED 50W","SERV","UNID.",null,null,0,{"$f":"IF( $G188 <> \"\",\nTRUNC( $H188 * $I188, 2 ),\nSUMIFS( $K189:$K$520,\n          $B189:$B$520, $B188 & \".*\",\n          $B189:$B$520, \"<>\" & $B188 & \".*.*\"\n) )","v":0},{"$f":"IF( $G188 <> \"\",\n     TRUNC( $H188 * $J188, 2 ),\n     SUMIFS( $L189:$L$520,\n              $B189:$B$520, $B188 & \".*\",\n              $B189:$B$520, \"<>\" & $B188 & \".*.*\"\n     ) )","v":0}]
[null,"6.6.4",null,null,"ELETRODUTO FLEXÍVEL CORRUGADO REFORÇADO, PVC, DN 32 MM (1\"), PARA CIRCUITOS TERMINAIS, INSTALADO EM FORRO - FORNECIMENTO E INSTALAÇÃO. AF_03/2023_PA","SERV","M",null,null,0,{"$f":"IF( $G189 <> \"\",\nTRUNC( $H189 * $I189, 2 ),\nSUMIFS( $K190:$K$520,\n          $B190:$B$520, $B189 & \".*\",\n          $B190:$B$520, \"<>\" & $B189 & \".*.*\"\n) )","v":0},{"$f":"IF( $G189 <> \"\",\n     TRUNC( $H189 * $J189, 2 ),\n     SUMIFS( $L190:$L$520,\n              $B190:$B$520, $B189 & \".*\",\n              $B190:$B$520, \"<>\" & $B189 & \".*.*\"\n     ) )","v":0}]
[null,"6.6.5",null,null,"CABO DE COBRE FLEXÍVEL ISOLADO, 4 MM², ANTI-CHAMA 0,6/1,0 KV, PARA CIRCUITOS TERMINAIS - FORNECIMENTO E INSTALAÇÃO. AF_03/2023","SERV","M",null,null,0,{"$f":"IF( $G190 <> \"\",\nTRUNC( $H190 * $I190, 2 ),\nSUMIFS( $K191:$K$520,\n          $B191:$B$520, $B190 & \".*\",\n          $B191:$B$520, \"<>\" & $B190 & \".*.*\"\n) )","v":0},{"$f":"IF( $G190 <> \"\",\n     TRUNC( $H190 * $J190, 2 ),\n     SUMIFS( $L191:$L$520,\n              $B191:$B$520, $B190 & \".*\",\n              $B191:$B$520, \"<>\" & $B190 & \".*.*\"\n     ) )","v":0}]
[null,"6.6.6",null,null,"ESCAVAÇÃO MANUAL DE VALA. AF_09/2024","SERV","M³",null,null,0,{"$f":"IF( $G191 <> \"\",\nTRUNC( $H191 * $I191, 2 ),\nSUMIFS( $K192:$K$520,\n          $B192:$B$520, $B191 & \".*\",\n          $B192:$B$520, \"<>\" & $B191 & \".*.*\"\n) )","v":0},{"$f":"IF( $G191 <> \"\",\n     TRUNC( $H191 * $J191, 2 ),\n     SUMIFS( $L192:$L$520,\n              $B192:$B$520, $B191 & \".*\",\n              $B192:$B$520, \"<>\" & $B191 & \".*.*\"\n     ) )","v":0}]
[null,"6.7",null,null,"PROJETO DE ENTRADA DE ENERGIA - SUBESTAÇÃO",{"$nulls":4},"",{"$f":"IF( $G192 <> \"\",\nTRUNC( $H192 * $I192, 2 ),\nSUMIFS( $K193:$K$520,\n          $B193:$B$520, $B192 & \".*\",\n          $B193:$B$520, \"<>\" & $B192 & \".*.*\"\n) )","v":0},{"$f":"IF( $G192 <> \"\",\n     TRUNC( $H192 * $J192, 2 ),\n     SUMIFS( $L193:$L$520,\n              $B193:$B$520, $B192 & \".*\",\n              $B193:$B$520, \"<>\" & $B192 & \".*.*\"\n     ) )","v":0}]
[null,"6.7.1",null,null,"POSTE DE CONCRETO ARMADO DE SECAO CIRCULAR, EXTENSAO DE 11,00 M, RESISTENCIA DE 200 A 300 DAN, TIPO C-14","FORN","UNID.",null,null,0,{"$f":"IF( $G193 <> \"\",\nTRUNC( $H193 * $I193, 2 ),\nSUMIFS( $K194:$K$520,\n          $B194:$B$520, $B193 & \".*\",\n          $B194:$B$520, \"<>\" & $B193 & \".*.*\"\n) )","v":0},{"$f":"IF( $G193 <> \"\",\n     TRUNC( $H193 * $J193, 2 ),\n     SUMIFS( $L194:$L$520,\n              $B194:$B$520, $B193 & \".*\",\n              $B194:$B$520, \"<>\" & $B193 & \".*.*\"\n     ) )","v":0}]
[null,"6.7.2",null,null,"FORNECIMENTO DE ISOLADOR DE PINO DE PORCELANA P/ 15 KV","SERV","UNID.",null,null,0,{"$f":"IF( $G194 <> \"\",\nTRUNC( $H194 * $I194, 2 ),\nSUMIFS( $K195:$K$520,\n          $B195:$B$520, $B194 & \".*\",\n          $B195:$B$520, \"<>\" & $B194 & \".*.*\"\n) )","v":0},{"$f":"IF( $G194 <> \"\",\n     TRUNC( $H194 * $J194, 2 ),\n     SUMIFS( $L195:$L$520,\n              $B195:$B$520, $B194 & \".*\",\n              $B195:$B$520, \"<>\" & $B194 & \".*.*\"\n     ) )","v":0}]
[null,"6.7.3",null,null,"ALCA PREFORMADA DE DISTRIBUICAO, EM ACO GALVANIZADO, PARA CONDUTORES DE ALUMINIO AWG 1/0 (CAA 6/1 OU CA 7 FIOS)","FORN","UNID.",null,null,0,{"$f":"IF( $G195 <> \"\",\nTRUNC( $H195 * $I195, 2 ),\nSUMIFS( $K196:$K$520,\n          $B196:$B$520, $B195 & \".*\",\n          $B196:$B$520, \"<>\" & $B195 & \".*.*\"\n) )","v":0},{"$f":"IF( $G195 <> \"\",\n     TRUNC( $H195 * $J195, 2 ),\n     SUMIFS( $L196:$L$520,\n              $B196:$B$520, $B195 & \".*\",\n              $B196:$B$520, \"<>\" & $B195 & \".*.*\"\n     ) )","v":0}]
[null,"6.7.4",null,null,"FORNECIMENTO DE PINO P/ ISOLADOR 15KV, 294MM","SERV","UNID.",null,null,0,{"$f":"IF( $G196 <> \"\",\nTRUNC( $H196 * $I196, 2 ),\nSUMIFS( $K197:$K$520,\n          $B197:$B$520, $B196 & \".*\",\n          $B197:$B$520, \"<>\" & $B196 & \".*.*\"\n) )","v":0},{"$f":"IF( $G196 <> \"\",\n     TRUNC( $H196 * $J196, 2 ),\n     SUMIFS( $L197:$L$520,\n              $B197:$B$520, $B196 & \".*\",\n              $B197:$B$520, \"<>\" & $B196 & \".*.*\"\n     ) )","v":0}]
[null,"6.7.5",null,null,"FORNECIMENTO DE PARAFUSO CABEÇA QUADRADA 16 X 300MM","SERV","UNID.",null,null,0,{"$f":"IF( $G197 <> \"\",\nTRUNC( $H197 * $I197, 2 ),\nSUMIFS( $K198:$K$520,\n          $B198:$B$520, $B197 & \".*\",\n          $B198:$B$520, \"<>\" & $B197 & \".*.*\"\n) )","v":0},{"$f":"IF( $G197 <> \"\",\n     TRUNC( $H197 * $J197, 2 ),\n     SUMIFS( $L198:$L$520,\n              $B198:$B$520, $B197 & \".*\",\n              $B198:$B$520, \"<>\" & $B197 & \".*.*\"\n     ) )","v":0}]
[null,"6.7.6",null,null,"FORNECIMENTO DE PARAFUSO CABEÇA QUADRADA 16 X 200MM","SERV","UNID.",null,null,0,{"$f":"IF( $G198 <> \"\",\nTRUNC( $H198 * $I198, 2 ),\nSUMIFS( $K199:$K$520,\n          $B199:$B$520, $B198 & \".*\",\n          $B199:$B$520, \"<>\" & $B198 & \".*.*\"\n) )","v":0},{"$f":"IF( $G198 <> \"\",\n     TRUNC( $H198 * $J198, 2 ),\n     SUMIFS( $L199:$L$520,\n              $B199:$B$520, $B198 & \".*\",\n              $B199:$B$520, \"<>\" & $B198 & \".*.*\"\n     ) )","v":0}]
[null,"6.7.7",null,null,"ARRUELA QUADRADA GALVANIZADA 38 MM C/FURO 18 MM (11/16\")","FORN","UNID.",null,null,0,{"$f":"IF( $G199 <> \"\",\nTRUNC( $H199 * $I199, 2 ),\nSUMIFS( $K200:$K$520,\n          $B200:$B$520, $B199 & \".*\",\n          $B200:$B$520, \"<>\" & $B199 & \".*.*\"\n) )","v":0},{"$f":"IF( $G199 <> \"\",\n     TRUNC( $H199 * $J199, 2 ),\n     SUMIFS( $L200:$L$520,\n              $B200:$B$520, $B199 & \".*\",\n              $B200:$B$520, \"<>\" & $B199 & \".*.*\"\n     ) )","v":0}]
[null,"6.7.8",null,null,"PORCA SEXTAVADA ZINCADA 1/4\" (FORNECIMENTO E COLOCAÇÃO)","SERV","UNID.",null,null,0,{"$f":"IF( $G200 <> \"\",\nTRUNC( $H200 * $I200, 2 ),\nSUMIFS( $K201:$K$520,\n          $B201:$B$520, $B200 & \".*\",\n          $B201:$B$520, \"<>\" & $B200 & \".*.*\"\n) )","v":0},{"$f":"IF( $G200 <> \"\",\n     TRUNC( $H200 * $J200, 2 ),\n     SUMIFS( $L201:$L$520,\n              $B201:$B$520, $B200 & \".*\",\n              $B201:$B$520, \"<>\" & $B200 & \".*.*\"\n     ) )","v":0}]
[null,"6.7.9",null,null,"PARA-RAIOS DE DISTRIBUICAO, TENSAO NOMINAL 15 KV, CORRENTE NOMINAL DE DESCARGA 5 KA","FORN","UNID.",null,null,{"$f":"IF(F201<>\"\",\nTRUNC(IF(F201=\"SERV\",I201*(1+$L$5/100),I201*(1+$L$6/100)),2),\n\"\" )","v":0},{"$f":"IF( $G201 <> \"\",\nTRUNC( $H201 * $I201, 2 ),\nSUMIFS( $K202:$K$520,\n          $B202:$B$520, $B201 & \".*\",\n          $B202:$B$520, \"<>\" & $B201 & \".*.*\"\n) )","v":0},{"$f":"IF( $G201 <> \"\",\n     TRUNC( $H201 * $J201, 2 ),\n     SUMIFS( $L202:$L$520,\n              $B202:$B$520, $B201 & \".*\",\n              $B202:$B$520, \"<>\" & $B201 & \".*.*\"\n     ) )","v":0}]
[null,"6.7.10",null,null,"CABO DE ALUMINIO NU COM ALMA DE ACO, BITOLA 2/0 AWG","FORN","KG",null,null,0,{"$f":"IF( $G202 <> \"\",\nTRUNC( $H202 * $I202, 2 ),\nSUMIFS( $K203:$K$520,\n          $B203:$B$520, $B202 & \".*\",\n          $B203:$B$520, \"<>\" & $B202 & \".*.*\"\n) )","v":0},{"$f":"IF( $G202 <> \"\",\n     TRUNC( $H202 * $J202, 2 ),\n     SUMIFS( $L203:$L$520,\n              $B203:$B$520, $B202 & \".*\",\n              $B203:$B$520, \"<>\" & $B202 & \".*.*\"\n     ) )","v":0}]
[null,"6.7.11",null,null,"CONECTOR TERMINAL A COMPRESSÃO COM DOIS FUROS EM ALUMÍNIO OU LIGA DE ALUMÍNIO- CB-79 (2/0)","FORN","UNID.",null,null,0,{"$f":"IF( $G203 <> \"\",\nTRUNC( $H203 * $I203, 2 ),\nSUMIFS( $K204:$K$520,\n          $B204:$B$520, $B203 & \".*\",\n          $B204:$B$520, \"<>\" & $B203 & \".*.*\"\n) )","v":0},{"$f":"IF( $G203 <> \"\",\n     TRUNC( $H203 * $J203, 2 ),\n     SUMIFS( $L204:$L$520,\n              $B204:$B$520, $B203 & \".*\",\n              $B204:$B$520, \"<>\" & $B203 & \".*.*\"\n     ) )","v":0}]
[null,"6.7.12",null,null,"CABO DE COBRE NÚ 16 MM2 (4 AWG) - FORNECIMENTO","SERV","KG",null,null,0,{"$f":"IF( $G204 <> \"\",\nTRUNC( $H204 * $I204, 2 ),\nSUMIFS( $K205:$K$520,\n          $B205:$B$520, $B204 & \".*\",\n          $B205:$B$520, \"<>\" & $B204 & \".*.*\"\n) )","v":0},{"$f":"IF( $G204 <> \"\",\n     TRUNC( $H204 * $J204, 2 ),\n     SUMIFS( $L205:$L$520,\n              $B205:$B$520, $B204 & \".*\",\n              $B205:$B$520, \"<>\" & $B204 & \".*.*\"\n     ) )","v":0}]
[null,"6.7.13",null,null,"CONECTOR METALICO TIPO PARAFUSO FENDIDO (SPLIT BOLT), PARA CABOS ATE 16 MM2","FORN","UNID.",null,null,0,{"$f":"IF( $G205 <> \"\",\nTRUNC( $H205 * $I205, 2 ),\nSUMIFS( $K206:$K$520,\n          $B206:$B$520, $B205 & \".*\",\n          $B206:$B$520, \"<>\" & $B205 & \".*.*\"\n) )","v":0},{"$f":"IF( $G205 <> \"\",\n     TRUNC( $H205 * $J205, 2 ),\n     SUMIFS( $L206:$L$520,\n              $B206:$B$520, $B205 & \".*\",\n              $B206:$B$520, \"<>\" & $B205 & \".*.*\"\n     ) )","v":0}]
[null,"6.7.14",null,null,"CABO DE COBRE NÚ 50 MM2 - FORNECIMENTO E ASSENTAMENTO (2,27M/KG)","SERV","KG",null,null,0,{"$f":"IF( $G206 <> \"\",\nTRUNC( $H206 * $I206, 2 ),\nSUMIFS( $K207:$K$520,\n          $B207:$B$520, $B206 & \".*\",\n          $B207:$B$520, \"<>\" & $B206 & \".*.*\"\n) )","v":0},{"$f":"IF( $G206 <> \"\",\n     TRUNC( $H206 * $J206, 2 ),\n     SUMIFS( $L207:$L$520,\n              $B207:$B$520, $B206 & \".*\",\n              $B207:$B$520, \"<>\" & $B206 & \".*.*\"\n     ) )","v":0}]
[null,"6.7.15",null,null,"CABO DE COBRE NÚ 95 MM2 - FORNECIMENTO E ASSENTAMENTO (1,193 M/KG)","SERV","KG",null,null,0,{"$f":"IF( $G207 <> \"\",\nTRUNC( $H207 * $I207, 2 ),\nSUMIFS( $K208:$K$520,\n          $B208:$B$520, $B207 & \".*\",\n          $B208:$B$520, \"<>\" & $B207 & \".*.*\"\n) )","v":0},{"$f":"IF( $G207 <> \"\",\n     TRUNC( $H207 * $J207, 2 ),\n     SUMIFS( $L208:$L$520,\n              $B208:$B$520, $B207 & \".*\",\n              $B208:$B$520, \"<>\" & $B207 & \".*.*\"\n     ) )","v":0}]
[null,"6.7.16",null,null,"HASTE COBREADA COPPERWELD P/ ATERRAMENTO D=  5/8\" X 3,00 M, EXCLUSO CONECTOR","FORN","UNID.",null,null,0,{"$f":"IF( $G208 <> \"\",\nTRUNC( $H208 * $I208, 2 ),\nSUMIFS( $K209:$K$520,\n          $B209:$B$520, $B208 & \".*\",\n          $B209:$B$520, \"<>\" & $B208 & \".*.*\"\n) )","v":0},{"$f":"IF( $G208 <> \"\",\n     TRUNC( $H208 * $J208, 2 ),\n     SUMIFS( $L209:$L$520,\n              $B209:$B$520, $B208 & \".*\",\n              $B209:$B$520, \"<>\" & $B208 & \".*.*\"\n     ) )","v":0}]
[null,"6.7.17",null,null,"CAIXA DE INSPEÇÃO  0,30 X 0,30 X 0,40M","SERV","UNID.",null,null,0,{"$f":"IF( $G209 <> \"\",\nTRUNC( $H209 * $I209, 2 ),\nSUMIFS( $K210:$K$520,\n          $B210:$B$520, $B209 & \".*\",\n          $B210:$B$520, \"<>\" & $B209 & \".*.*\"\n) )","v":0},{"$f":"IF( $G209 <> \"\",\n     TRUNC( $H209 * $J209, 2 ),\n     SUMIFS( $L210:$L$520,\n              $B210:$B$520, $B209 & \".*\",\n              $B210:$B$520, \"<>\" & $B209 & \".*.*\"\n     ) )","v":0}]
[null,"6.7.18",null,null,"FORNECIMENTO DE CHAVE FUSÍVEL 15KV - 100A, RUPTURA ASSIM. 10 KA","SERV","UNID.",null,null,0,{"$f":"IF( $G210 <> \"\",\nTRUNC( $H210 * $I210, 2 ),\nSUMIFS( $K211:$K$520,\n          $B211:$B$520, $B210 & \".*\",\n          $B211:$B$520, \"<>\" & $B210 & \".*.*\"\n) )","v":0},{"$f":"IF( $G210 <> \"\",\n     TRUNC( $H210 * $J210, 2 ),\n     SUMIFS( $L211:$L$520,\n              $B211:$B$520, $B210 & \".*\",\n              $B211:$B$520, \"<>\" & $B210 & \".*.*\"\n     ) )","v":0}]
[null,"6.7.19",null,null,"FORNECIMENTO E INSTALAÇÃO DE ELO FUSÍVEL TIPO 10K, COMP.= 500MM","SERV","UNID.",null,null,0,{"$f":"IF( $G211 <> \"\",\nTRUNC( $H211 * $I211, 2 ),\nSUMIFS( $K212:$K$520,\n          $B212:$B$520, $B211 & \".*\",\n          $B212:$B$520, \"<>\" & $B211 & \".*.*\"\n) )","v":0},{"$f":"IF( $G211 <> \"\",\n     TRUNC( $H211 * $J211, 2 ),\n     SUMIFS( $L212:$L$520,\n              $B212:$B$520, $B211 & \".*\",\n              $B212:$B$520, \"<>\" & $B211 & \".*.*\"\n     ) )","v":0}]
[null,"6.7.20",null,null,"TRANSFORMADOR DE DISTRIBUIÇÃO, 300 KVA, TRIFÁSICO, 60 HZ, CLASSE 15 KV, IMERSO EM ÓLEO MINERAL, INSTALAÇÃO EM POSTE (NÃO INCLUSO SUPORTE) - FORNECIMENTO E INSTALAÇÃO. AF_12/2020","SERV","UNID.",null,null,0,{"$f":"IF( $G212 <> \"\",\nTRUNC( $H212 * $I212, 2 ),\nSUMIFS( $K213:$K$520,\n          $B213:$B$520, $B212 & \".*\",\n          $B213:$B$520, \"<>\" & $B212 & \".*.*\"\n) )","v":0},{"$f":"IF( $G212 <> \"\",\n     TRUNC( $H212 * $J212, 2 ),\n     SUMIFS( $L213:$L$520,\n              $B213:$B$520, $B212 & \".*\",\n              $B213:$B$520, \"<>\" & $B212 & \".*.*\"\n     ) )","v":0}]
[null,"6.7.21",null,null,"CONCRETO FCK = 30MPA, TRAÇO 1:2,1:2,5 (EM MASSA SECA DE CIMENTO/ AREIA MÉDIA/ BRITA 1) - PREPARO MECÂNICO COM BETONEIRA 600 L. AF_05/2021","SERV","M³",null,null,0,{"$f":"IF( $G213 <> \"\",\nTRUNC( $H213 * $I213, 2 ),\nSUMIFS( $K214:$K$520,\n          $B214:$B$520, $B213 & \".*\",\n          $B214:$B$520, \"<>\" & $B213 & \".*.*\"\n) )","v":0},{"$f":"IF( $G213 <> \"\",\n     TRUNC( $H213 * $J213, 2 ),\n     SUMIFS( $L214:$L$520,\n              $B214:$B$520, $B213 & \".*\",\n              $B214:$B$520, \"<>\" & $B213 & \".*.*\"\n     ) )","v":0}]
[null,"6.7.22",null,null,"ELETRODUTO DE FERRO GALVANIZADO SEM COSTURA D= 4\" - FORNECIMENTO","SERV","UNID.",null,null,0,{"$f":"IF( $G214 <> \"\",\nTRUNC( $H214 * $I214, 2 ),\nSUMIFS( $K215:$K$520,\n          $B215:$B$520, $B214 & \".*\",\n          $B215:$B$520, \"<>\" & $B214 & \".*.*\"\n) )","v":0},{"$f":"IF( $G214 <> \"\",\n     TRUNC( $H214 * $J214, 2 ),\n     SUMIFS( $L215:$L$520,\n              $B215:$B$520, $B214 & \".*\",\n              $B215:$B$520, \"<>\" & $B214 & \".*.*\"\n     ) )","v":0}]
[null,"6.7.23",null,null,"CABEÇOTE DE ALUMÍNIO DE 4\"","FORN","UNID.",null,null,0,{"$f":"IF( $G215 <> \"\",\nTRUNC( $H215 * $I215, 2 ),\nSUMIFS( $K216:$K$520,\n          $B216:$B$520, $B215 & \".*\",\n          $B216:$B$520, \"<>\" & $B215 & \".*.*\"\n) )","v":0},{"$f":"IF( $G215 <> \"\",\n     TRUNC( $H215 * $J215, 2 ),\n     SUMIFS( $L216:$L$520,\n              $B216:$B$520, $B215 & \".*\",\n              $B216:$B$520, \"<>\" & $B215 & \".*.*\"\n     ) )","v":0}]
[null,"6.7.24",null,null,"BUCHA COM ARRUELA EM ALUMÍNIO P/ELETRODUTO 100MM, D=4\"","SERV","UNID.",null,null,0,{"$f":"IF( $G216 <> \"\",\nTRUNC( $H216 * $I216, 2 ),\nSUMIFS( $K217:$K$520,\n          $B217:$B$520, $B216 & \".*\",\n          $B217:$B$520, \"<>\" & $B216 & \".*.*\"\n) )","v":0},{"$f":"IF( $G216 <> \"\",\n     TRUNC( $H216 * $J216, 2 ),\n     SUMIFS( $L217:$L$520,\n              $B217:$B$520, $B216 & \".*\",\n              $B217:$B$520, \"<>\" & $B216 & \".*.*\"\n     ) )","v":0}]
[null,"6.7.25",null,null,"LUVA PARA ELETRODUTO GALVANIZADO, DIÂM = 4\"","SERV","UNID.",null,null,0,{"$f":"IF( $G217 <> \"\",\nTRUNC( $H217 * $I217, 2 ),\nSUMIFS( $K218:$K$520,\n          $B218:$B$520, $B217 & \".*\",\n          $B218:$B$520, \"<>\" & $B217 & \".*.*\"\n) )","v":0},{"$f":"IF( $G217 <> \"\",\n     TRUNC( $H217 * $J217, 2 ),\n     SUMIFS( $L218:$L$520,\n              $B218:$B$520, $B217 & \".*\",\n              $B218:$B$520, \"<>\" & $B217 & \".*.*\"\n     ) )","v":0}]
[null,"6.7.26",null,null,"DISJUNTOR TERMOMAGNÉTICO TRIPOLAR 150 A COM CAIXA MOLDADA 10 KA","SERV","UNID.",null,null,0,{"$f":"IF( $G218 <> \"\",\nTRUNC( $H218 * $I218, 2 ),\nSUMIFS( $K219:$K$520,\n          $B219:$B$520, $B218 & \".*\",\n          $B219:$B$520, \"<>\" & $B218 & \".*.*\"\n) )","v":0},{"$f":"IF( $G218 <> \"\",\n     TRUNC( $H218 * $J218, 2 ),\n     SUMIFS( $L219:$L$520,\n              $B219:$B$520, $B218 & \".*\",\n              $B219:$B$520, \"<>\" & $B218 & \".*.*\"\n     ) )","v":0}]
[null,"6.7.27",null,null,"DISJUNTOR TRIPOLAR 630 A COM CAIXA MOLDADA, 30KA","SERV","UNID.",null,null,0,{"$f":"IF( $G219 <> \"\",\nTRUNC( $H219 * $I219, 2 ),\nSUMIFS( $K220:$K$520,\n          $B220:$B$520, $B219 & \".*\",\n          $B220:$B$520, \"<>\" & $B219 & \".*.*\"\n) )","v":0},{"$f":"IF( $G219 <> \"\",\n     TRUNC( $H219 * $J219, 2 ),\n     SUMIFS( $L220:$L$520,\n              $B220:$B$520, $B219 & \".*\",\n              $B220:$B$520, \"<>\" & $B219 & \".*.*\"\n     ) )","v":0}]
[null,"6.7.28",null,null,"DISJUNTOR TERMOMAGNÉTICO TRIPOLAR 125 A COM CAIXA MOLDADA 10 KA","SERV","UNID.",null,null,0,{"$f":"IF( $G220 <> \"\",\nTRUNC( $H220 * $I220, 2 ),\nSUMIFS( $K221:$K$520,\n          $B221:$B$520, $B220 & \".*\",\n          $B221:$B$520, \"<>\" & $B220 & \".*.*\"\n) )","v":0},{"$f":"IF( $G220 <> \"\",\n     TRUNC( $H220 * $J220, 2 ),\n     SUMIFS( $L221:$L$520,\n              $B221:$B$520, $B220 & \".*\",\n              $B221:$B$520, \"<>\" & $B220 & \".*.*\"\n     ) )","v":0}]
[null,"6.7.29",null,null,"DISJUNTOR TERMOMAGNÉTICO TRIPOLAR 400 A COM CAIXA MOLDADA 10 KA","SERV","UNID.",null,null,0,{"$f":"IF( $G221 <> \"\",\nTRUNC( $H221 * $I221, 2 ),\nSUMIFS( $K222:$K$520,\n          $B222:$B$520, $B221 & \".*\",\n          $B222:$B$520, \"<>\" & $B221 & \".*.*\"\n) )","v":0},{"$f":"IF( $G221 <> \"\",\n     TRUNC( $H221 * $J221, 2 ),\n     SUMIFS( $L222:$L$520,\n              $B222:$B$520, $B221 & \".*\",\n              $B222:$B$520, \"<>\" & $B221 & \".*.*\"\n     ) )","v":0}]
[null,"6.7.30",null,null,"DISJUNTOR TRIPOLAR TIPO NEMA, CORRENTE NOMINAL DE 60 ATÉ 100A - FORNECIMENTO E INSTALAÇÃO. AF_10/2020","SERV","UNID.",null,null,0,{"$f":"IF( $G222 <> \"\",\nTRUNC( $H222 * $I222, 2 ),\nSUMIFS( $K223:$K$520,\n          $B223:$B$520, $B222 & \".*\",\n          $B223:$B$520, \"<>\" & $B222 & \".*.*\"\n) )","v":0},{"$f":"IF( $G222 <> \"\",\n     TRUNC( $H222 * $J222, 2 ),\n     SUMIFS( $L223:$L$520,\n              $B223:$B$520, $B222 & \".*\",\n              $B223:$B$520, \"<>\" & $B222 & \".*.*\"\n     ) )","v":0}]
[null,"6.7.31",null,null,"DISPOSITIVO DPS CLASSE II, 1 POLO, TENSAO MAXIMA DE 275 V, CORRENTE MAXIMA DE *90* KA (TIPO AC)","FORN","UNID.",null,null,0,{"$f":"IF( $G223 <> \"\",\nTRUNC( $H223 * $I223, 2 ),\nSUMIFS( $K224:$K$520,\n          $B224:$B$520, $B223 & \".*\",\n          $B224:$B$520, \"<>\" & $B223 & \".*.*\"\n) )","v":0},{"$f":"IF( $G223 <> \"\",\n     TRUNC( $H223 * $J223, 2 ),\n     SUMIFS( $L224:$L$520,\n              $B224:$B$520, $B223 & \".*\",\n              $B224:$B$520, \"<>\" & $B223 & \".*.*\"\n     ) )","v":0}]
[null,"6.7.32",null,null,"BARRAMENTO CHATA COBRE ELETROLÍTICO 19,05X3,18MM","FORN","M",null,null,0,{"$f":"IF( $G224 <> \"\",\nTRUNC( $H224 * $I224, 2 ),\nSUMIFS( $K225:$K$520,\n          $B225:$B$520, $B224 & \".*\",\n          $B225:$B$520, \"<>\" & $B224 & \".*.*\"\n) )","v":0},{"$f":"IF( $G224 <> \"\",\n     TRUNC( $H224 * $J224, 2 ),\n     SUMIFS( $L225:$L$520,\n              $B225:$B$520, $B224 & \".*\",\n              $B225:$B$520, \"<>\" & $B224 & \".*.*\"\n     ) )","v":0}]
[null,"6.7.33",null,null,"BARRAMENTO CHATA COBRE ELETROLÍTICO 50,80X 3,18MM","FORN","M",null,null,0,{"$f":"IF( $G225 <> \"\",\nTRUNC( $H225 * $I225, 2 ),\nSUMIFS( $K226:$K$520,\n          $B226:$B$520, $B225 & \".*\",\n          $B226:$B$520, \"<>\" & $B225 & \".*.*\"\n) )","v":0},{"$f":"IF( $G225 <> \"\",\n     TRUNC( $H225 * $J225, 2 ),\n     SUMIFS( $L226:$L$520,\n              $B226:$B$520, $B225 & \".*\",\n              $B226:$B$520, \"<>\" & $B225 & \".*.*\"\n     ) )","v":0}]
[null,"6.7.34",null,null,"BARRAMENTO COBRE 70,20 X 6,35 MM²","FORN","M",null,null,0,{"$f":"IF( $G226 <> \"\",\nTRUNC( $H226 * $I226, 2 ),\nSUMIFS( $K227:$K$520,\n          $B227:$B$520, $B226 & \".*\",\n          $B227:$B$520, \"<>\" & $B226 & \".*.*\"\n) )","v":0},{"$f":"IF( $G226 <> \"\",\n     TRUNC( $H226 * $J226, 2 ),\n     SUMIFS( $L227:$L$520,\n              $B227:$B$520, $B226 & \".*\",\n              $B227:$B$520, \"<>\" & $B226 & \".*.*\"\n     ) )","v":0}]
[null,"6.7.35",null,null,"PLACA DE SINALIZACAO, FOTOLUMINESCENTE, EM PVC , COM LOGOTIPO \"CUIDADO RISCO DE CHOQUE ELÉTRICO\"- PLACA E5","SERV","UNID.",null,null,0,{"$f":"IF( $G227 <> \"\",\nTRUNC( $H227 * $I227, 2 ),\nSUMIFS( $K228:$K$520,\n          $B228:$B$520, $B227 & \".*\",\n          $B228:$B$520, \"<>\" & $B227 & \".*.*\"\n) )","v":0},{"$f":"IF( $G227 <> \"\",\n     TRUNC( $H227 * $J227, 2 ),\n     SUMIFS( $L228:$L$520,\n              $B228:$B$520, $B227 & \".*\",\n              $B228:$B$520, \"<>\" & $B227 & \".*.*\"\n     ) )","v":0}]
[null,"6.7.36",null,null,"CABO DE COBRE FLEXÍVEL ISOLADO, 185 MM², ANTI-CHAMA 0,6/1,0 KV, PARA REDE ENTERRADA DE DISTRIBUIÇÃO DE ENERGIA ELÉTRICA - FORNECIMENTO E INSTALAÇÃO. AF_12/2021","SERV","M",null,null,0,{"$f":"IF( $G228 <> \"\",\nTRUNC( $H228 * $I228, 2 ),\nSUMIFS( $K229:$K$520,\n          $B229:$B$520, $B228 & \".*\",\n          $B229:$B$520, \"<>\" & $B228 & \".*.*\"\n) )","v":0},{"$f":"IF( $G228 <> \"\",\n     TRUNC( $H228 * $J228, 2 ),\n     SUMIFS( $L229:$L$520,\n              $B229:$B$520, $B228 & \".*\",\n              $B229:$B$520, \"<>\" & $B228 & \".*.*\"\n     ) )","v":0}]
[null,"6.7.37",null,null,"CABO DE COBRE FLEXÍVEL ISOLADO, 95 MM², ANTI-CHAMA 0,6/1,0 KV, PARA REDE ENTERRADA DE DISTRIBUIÇÃO DE ENERGIA ELÉTRICA - FORNECIMENTO E INSTALAÇÃO. AF_12/2021","SERV","M",null,null,0,{"$f":"IF( $G229 <> \"\",\nTRUNC( $H229 * $I229, 2 ),\nSUMIFS( $K230:$K$520,\n          $B230:$B$520, $B229 & \".*\",\n          $B230:$B$520, \"<>\" & $B229 & \".*.*\"\n) )","v":0},{"$f":"IF( $G229 <> \"\",\n     TRUNC( $H229 * $J229, 2 ),\n     SUMIFS( $L230:$L$520,\n              $B230:$B$520, $B229 & \".*\",\n              $B230:$B$520, \"<>\" & $B229 & \".*.*\"\n     ) )","v":0}]
[null,"6.7.38",null,null,"MOLDE DE SOLDA EXOTÉRMICA PARA CABO COBRE NU 95 MM²","FORN","UNID.",null,null,0,{"$f":"IF( $G230 <> \"\",\nTRUNC( $H230 * $I230, 2 ),\nSUMIFS( $K231:$K$520,\n          $B231:$B$520, $B230 & \".*\",\n          $B231:$B$520, \"<>\" & $B230 & \".*.*\"\n) )","v":0},{"$f":"IF( $G230 <> \"\",\n     TRUNC( $H230 * $J230, 2 ),\n     SUMIFS( $L231:$L$520,\n              $B231:$B$520, $B230 & \".*\",\n              $B231:$B$520, \"<>\" & $B230 & \".*.*\"\n     ) )","v":0}]
[null,"6.7.39",null,null,"SOLDA EXOTÉRMICA","SERV","UNID.",null,null,0,{"$f":"IF( $G231 <> \"\",\nTRUNC( $H231 * $I231, 2 ),\nSUMIFS( $K232:$K$520,\n          $B232:$B$520, $B231 & \".*\",\n          $B232:$B$520, \"<>\" & $B231 & \".*.*\"\n) )","v":0},{"$f":"IF( $G231 <> \"\",\n     TRUNC( $H231 * $J231, 2 ),\n     SUMIFS( $L232:$L$520,\n              $B232:$B$520, $B231 & \".*\",\n              $B232:$B$520, \"<>\" & $B231 & \".*.*\"\n     ) )","v":0}]
[null,"6.7.40",null,null,"QFAC - QUADRO / PAINEL EM CHAPA DE AÇO COM PINTURA ELETROSTÁTICA A PÓ POLIESTER NA COR BEGE, GRAU DE PROTEÇÃO IP 54, COM BARRAMENTO, SEM DISJUNTORES - 1500X1000X350MM","SERV","UNID.",null,null,0,{"$f":"IF( $G232 <> \"\",\nTRUNC( $H232 * $I232, 2 ),\nSUMIFS( $K233:$K$520,\n          $B233:$B$520, $B232 & \".*\",\n          $B233:$B$520, \"<>\" & $B232 & \".*.*\"\n) )","v":0},{"$f":"IF( $G232 <> \"\",\n     TRUNC( $H232 * $J232, 2 ),\n     SUMIFS( $L233:$L$520,\n              $B233:$B$520, $B232 & \".*\",\n              $B233:$B$520, \"<>\" & $B232 & \".*.*\"\n     ) )","v":0}]
[null,"6.7.41",null,null,"VIDRO ACRÍLICO TRANSPARENTE ANTICHAMA 750 X 950 X 5 MM","FORN","UNID.",null,null,0,{"$f":"IF( $G233 <> \"\",\nTRUNC( $H233 * $I233, 2 ),\nSUMIFS( $K234:$K$520,\n          $B234:$B$520, $B233 & \".*\",\n          $B234:$B$520, \"<>\" & $B233 & \".*.*\"\n) )","v":0},{"$f":"IF( $G233 <> \"\",\n     TRUNC( $H233 * $J233, 2 ),\n     SUMIFS( $L234:$L$520,\n              $B234:$B$520, $B233 & \".*\",\n              $B234:$B$520, \"<>\" & $B233 & \".*.*\"\n     ) )","v":0}]
[null,"6.8",null,null,"PROJETOS DE RAMAIS DE CARGAS DOS QUADROS DE MEDIDORES",{"$nulls":4},"",{"$f":"IF( $G234 <> \"\",\nTRUNC( $H234 * $I234, 2 ),\nSUMIFS( $K235:$K$520,\n          $B235:$B$520, $B234 & \".*\",\n          $B235:$B$520, \"<>\" & $B234 & \".*.*\"\n) )","v":0},{"$f":"IF( $G234 <> \"\",\n     TRUNC( $H234 * $J234, 2 ),\n     SUMIFS( $L235:$L$520,\n              $B235:$B$520, $B234 & \".*\",\n              $B235:$B$520, \"<>\" & $B234 & \".*.*\"\n     ) )","v":0}]
[null,"6.8.1",null,null,"CABO DE COBRE FLEXÍVEL ISOLADO, 120 MM², ANTI-CHAMA 0,6/1,0 KV, PARA REDE ENTERRADA DE DISTRIBUIÇÃO DE ENERGIA ELÉTRICA - FORNECIMENTO E INSTALAÇÃO. AF_12/2021","SERV","M",null,null,0,{"$f":"IF( $G235 <> \"\",\nTRUNC( $H235 * $I235, 2 ),\nSUMIFS( $K236:$K$520,\n          $B236:$B$520, $B235 & \".*\",\n          $B236:$B$520, \"<>\" & $B235 & \".*.*\"\n) )","v":0},{"$f":"IF( $G235 <> \"\",\n     TRUNC( $H235 * $J235, 2 ),\n     SUMIFS( $L236:$L$520,\n              $B236:$B$520, $B235 & \".*\",\n              $B236:$B$520, \"<>\" & $B235 & \".*.*\"\n     ) )","v":0}]
[null,"6.8.2",null,null,"CABO DE COBRE FLEXÍVEL ISOLADO, 70 MM², ANTI-CHAMA 0,6/1,0 KV, PARA REDE ENTERRADA DE DISTRIBUIÇÃO DE ENERGIA ELÉTRICA - FORNECIMENTO E INSTALAÇÃO. AF_12/2021","SERV","M",null,null,0,{"$f":"IF( $G236 <> \"\",\nTRUNC( $H236 * $I236, 2 ),\nSUMIFS( $K237:$K$520,\n          $B237:$B$520, $B236 & \".*\",\n          $B237:$B$520, \"<>\" & $B236 & \".*.*\"\n) )","v":0},{"$f":"IF( $G236 <> \"\",\n     TRUNC( $H236 * $J236, 2 ),\n     SUMIFS( $L237:$L$520,\n              $B237:$B$520, $B236 & \".*\",\n              $B237:$B$520, \"<>\" & $B236 & \".*.*\"\n     ) )","v":0}]
[null,"6.8.3",null,null,"CABO DE COBRE FLEXÍVEL ISOLADO, 35 MM², ANTI-CHAMA 0,6/1,0 KV, PARA REDE ENTERRADA DE DISTRIBUIÇÃO DE ENERGIA ELÉTRICA - FORNECIMENTO E INSTALAÇÃO. AF_12/2021","SERV","M",null,null,0,{"$f":"IF( $G237 <> \"\",\nTRUNC( $H237 * $I237, 2 ),\nSUMIFS( $K238:$K$520,\n          $B238:$B$520, $B237 & \".*\",\n          $B238:$B$520, \"<>\" & $B237 & \".*.*\"\n) )","v":0},{"$f":"IF( $G237 <> \"\",\n     TRUNC( $H237 * $J237, 2 ),\n     SUMIFS( $L238:$L$520,\n              $B238:$B$520, $B237 & \".*\",\n              $B238:$B$520, \"<>\" & $B237 & \".*.*\"\n     ) )","v":0}]
[null,"6.8.4",null,null,"CABO DE COBRE FLEXÍVEL ISOLADO, 50 MM², ANTI-CHAMA 0,6/1,0 KV, PARA REDE ENTERRADA DE DISTRIBUIÇÃO DE ENERGIA ELÉTRICA - FORNECIMENTO E INSTALAÇÃO. AF_12/2021","SERV","M",null,null,0,{"$f":"IF( $G238 <> \"\",\nTRUNC( $H238 * $I238, 2 ),\nSUMIFS( $K239:$K$520,\n          $B239:$B$520, $B238 & \".*\",\n          $B239:$B$520, \"<>\" & $B238 & \".*.*\"\n) )","v":0},{"$f":"IF( $G238 <> \"\",\n     TRUNC( $H238 * $J238, 2 ),\n     SUMIFS( $L239:$L$520,\n              $B239:$B$520, $B238 & \".*\",\n              $B239:$B$520, \"<>\" & $B238 & \".*.*\"\n     ) )","v":0}]
[null,"6.8.5",null,null,"CABO DE COBRE ISOLADO, 25 MM², ANTI-CHAMA 0,6/1 KV, INSTALADO EM ELETROCALHA OU PERFILADO - FORNECIMENTO E INSTALAÇÃO. AF_10/2020","SERV","M",null,null,0,{"$f":"IF( $G239 <> \"\",\nTRUNC( $H239 * $I239, 2 ),\nSUMIFS( $K240:$K$520,\n          $B240:$B$520, $B239 & \".*\",\n          $B240:$B$520, \"<>\" & $B239 & \".*.*\"\n) )","v":0},{"$f":"IF( $G239 <> \"\",\n     TRUNC( $H239 * $J239, 2 ),\n     SUMIFS( $L240:$L$520,\n              $B240:$B$520, $B239 & \".*\",\n              $B240:$B$520, \"<>\" & $B239 & \".*.*\"\n     ) )","v":0}]
[null,"6.8.6",null,null,"ELETRODUTO FLEXÍVEL CORRUGADO, PEAD, DN 100 (4\"), PARA REDE ENTERRADA DE DISTRIBUIÇÃO DE ENERGIA ELÉTRICA - FORNECIMENTO E INSTALAÇÃO. AF_12/2021","SERV","M",null,null,0,{"$f":"IF( $G240 <> \"\",\nTRUNC( $H240 * $I240, 2 ),\nSUMIFS( $K241:$K$520,\n          $B241:$B$520, $B240 & \".*\",\n          $B241:$B$520, \"<>\" & $B240 & \".*.*\"\n) )","v":0},{"$f":"IF( $G240 <> \"\",\n     TRUNC( $H240 * $J240, 2 ),\n     SUMIFS( $L241:$L$520,\n              $B241:$B$520, $B240 & \".*\",\n              $B241:$B$520, \"<>\" & $B240 & \".*.*\"\n     ) )","v":0}]
[null,"6.8.7",null,null,"CAIXA DE PASSAGEM / POÇO DE VISITA EM CONCRETO ARMADO FCK=21 MPA, INCLUSIVE TAMPA, DIMENSÕES INTERNAS 1.00 X 1.00 X 0.70 M","SERV","UNID.",null,null,0,{"$f":"IF( $G241 <> \"\",\nTRUNC( $H241 * $I241, 2 ),\nSUMIFS( $K242:$K$520,\n          $B242:$B$520, $B241 & \".*\",\n          $B242:$B$520, \"<>\" & $B241 & \".*.*\"\n) )","v":0},{"$f":"IF( $G241 <> \"\",\n     TRUNC( $H241 * $J241, 2 ),\n     SUMIFS( $L242:$L$520,\n              $B242:$B$520, $B241 & \".*\",\n              $B242:$B$520, \"<>\" & $B241 & \".*.*\"\n     ) )","v":0}]
[null,"6.8.8",null,null,"QUADRO DE MEDIDOR P/ 22 MEDIDORES, COMPLETO P/ DISJUNTOR GERAL DE 125 A. MOD. TAF DIMENSÕES: 2650X1710X300MM","FORN","UNID.",null,null,0,{"$f":"IF( $G242 <> \"\",\nTRUNC( $H242 * $I242, 2 ),\nSUMIFS( $K243:$K$520,\n          $B243:$B$520, $B242 & \".*\",\n          $B243:$B$520, \"<>\" & $B242 & \".*.*\"\n) )","v":0},{"$f":"IF( $G242 <> \"\",\n     TRUNC( $H242 * $J242, 2 ),\n     SUMIFS( $L243:$L$520,\n              $B243:$B$520, $B242 & \".*\",\n              $B243:$B$520, \"<>\" & $B242 & \".*.*\"\n     ) )","v":0}]
[null,"6.8.9",null,null,"CABINE DO QPG EXECUTADA EM ALVENARIA PARA INSTALAÇÃO DO PAINEL DO QPG. DIMENSÕES 135X220X200CM (LXPXA).","FORN","UNID.",null,null,0,{"$f":"IF( $G243 <> \"\",\nTRUNC( $H243 * $I243, 2 ),\nSUMIFS( $K244:$K$520,\n          $B244:$B$520, $B243 & \".*\",\n          $B244:$B$520, \"<>\" & $B243 & \".*.*\"\n) )","v":0},{"$f":"IF( $G243 <> \"\",\n     TRUNC( $H243 * $J243, 2 ),\n     SUMIFS( $L244:$L$520,\n              $B244:$B$520, $B243 & \".*\",\n              $B244:$B$520, \"<>\" & $B243 & \".*.*\"\n     ) )","v":0}]
[null,"6.8.10",null,null,"QUADRO DE MEDIDOR P/ 24 MEDIDORES, COMPLETO P/ DISJUNTOR GERAL DE 400 A, MOD. TAF DIMENSÕES: 2910 X 1710 X 300 MM","FORN","UNID.",null,null,0,{"$f":"IF( $G244 <> \"\",\nTRUNC( $H244 * $I244, 2 ),\nSUMIFS( $K245:$K$520,\n          $B245:$B$520, $B244 & \".*\",\n          $B245:$B$520, \"<>\" & $B244 & \".*.*\"\n) )","v":0},{"$f":"IF( $G244 <> \"\",\n     TRUNC( $H244 * $J244, 2 ),\n     SUMIFS( $L245:$L$520,\n              $B245:$B$520, $B244 & \".*\",\n              $B245:$B$520, \"<>\" & $B244 & \".*.*\"\n     ) )","v":0}]
[null,"6.8.11",null,null,"QUADRO DE MEDIDOR P/ 28 MEDIDORES, COMPLETO P/ DISJUNTOR GERAL DE 150 A, MOD. TAF DIMENSÕES: 3170 X 1710 X 300 MM","FORN","UNID.",null,null,0,{"$f":"IF( $G245 <> \"\",\nTRUNC( $H245 * $I245, 2 ),\nSUMIFS( $K246:$K$520,\n          $B246:$B$520, $B245 & \".*\",\n          $B246:$B$520, \"<>\" & $B245 & \".*.*\"\n) )","v":0},{"$f":"IF( $G245 <> \"\",\n     TRUNC( $H245 * $J245, 2 ),\n     SUMIFS( $L246:$L$520,\n              $B246:$B$520, $B245 & \".*\",\n              $B246:$B$520, \"<>\" & $B245 & \".*.*\"\n     ) )","v":0}]
[null,"6.9",null,null,"PROJETO ELÉTRICO DE CABEAMENTO ESTRUTURADO",{"$nulls":4},"",{"$f":"IF( $G246 <> \"\",\nTRUNC( $H246 * $I246, 2 ),\nSUMIFS( $K247:$K$520,\n          $B247:$B$520, $B246 & \".*\",\n          $B247:$B$520, \"<>\" & $B246 & \".*.*\"\n) )","v":0},{"$f":"IF( $G246 <> \"\",\n     TRUNC( $H246 * $J246, 2 ),\n     SUMIFS( $L247:$L$520,\n              $B247:$B$520, $B246 & \".*\",\n              $B247:$B$520, \"<>\" & $B246 & \".*.*\"\n     ) )","v":0}]
[null,"6.9.1",null,null,"CAIXA DE PASSAGEM EM ALVENARIA DE TIJOLOS MACIÇOS ESP. = 0,12M,  DIM. INT. = 0.60 X 0.60 X 0.60M","SERV","UNID.",null,null,0,{"$f":"IF( $G247 <> \"\",\nTRUNC( $H247 * $I247, 2 ),\nSUMIFS( $K248:$K$520,\n          $B248:$B$520, $B247 & \".*\",\n          $B248:$B$520, \"<>\" & $B247 & \".*.*\"\n) )","v":0},{"$f":"IF( $G247 <> \"\",\n     TRUNC( $H247 * $J247, 2 ),\n     SUMIFS( $L248:$L$520,\n              $B248:$B$520, $B247 & \".*\",\n              $B248:$B$520, \"<>\" & $B247 & \".*.*\"\n     ) )","v":0}]
[null,"6.9.2",null,null,"TAMPA ARTICULADA DE FERRO FUNDIDO 60 X 60CM, INCLUSIVE INSTALAÇÃO","SERV","UNID.",null,null,0,{"$f":"IF( $G248 <> \"\",\nTRUNC( $H248 * $I248, 2 ),\nSUMIFS( $K249:$K$520,\n          $B249:$B$520, $B248 & \".*\",\n          $B249:$B$520, \"<>\" & $B248 & \".*.*\"\n) )","v":0},{"$f":"IF( $G248 <> \"\",\n     TRUNC( $H248 * $J248, 2 ),\n     SUMIFS( $L249:$L$520,\n              $B249:$B$520, $B248 & \".*\",\n              $B249:$B$520, \"<>\" & $B248 & \".*.*\"\n     ) )","v":0}]
[null,"6.9.3",null,null,"CAIXA DE CONCRETO PRE MOLDADO PARA ATERRAMENTO, COM TAMPA, 40 X 40 X 40, E = 5CM","SERV","UNID.",null,null,0,{"$f":"IF( $G249 <> \"\",\nTRUNC( $H249 * $I249, 2 ),\nSUMIFS( $K250:$K$520,\n          $B250:$B$520, $B249 & \".*\",\n          $B250:$B$520, \"<>\" & $B249 & \".*.*\"\n) )","v":0},{"$f":"IF( $G249 <> \"\",\n     TRUNC( $H249 * $J249, 2 ),\n     SUMIFS( $L250:$L$520,\n              $B250:$B$520, $B249 & \".*\",\n              $B250:$B$520, \"<>\" & $B249 & \".*.*\"\n     ) )","v":0}]
[null,"6.9.4",null,null,"TAMPA DE CONCRETO PARA CAIXAS DE PASSAGEM 0,40X0,40MX0,07M","SERV","UNID.",null,null,0,{"$f":"IF( $G250 <> \"\",\nTRUNC( $H250 * $I250, 2 ),\nSUMIFS( $K251:$K$520,\n          $B251:$B$520, $B250 & \".*\",\n          $B251:$B$520, \"<>\" & $B250 & \".*.*\"\n) )","v":0},{"$f":"IF( $G250 <> \"\",\n     TRUNC( $H250 * $J250, 2 ),\n     SUMIFS( $L251:$L$520,\n              $B251:$B$520, $B250 & \".*\",\n              $B251:$B$520, \"<>\" & $B250 & \".*.*\"\n     ) )","v":0}]
[null,"6.9.5",null,null,"ELETRODUTO DE FERRO GALVANIZADO SEM COSTURA D= 4\" - FORNECIMENTO","SERV","UNID.",null,null,0,{"$f":"IF( $G251 <> \"\",\nTRUNC( $H251 * $I251, 2 ),\nSUMIFS( $K252:$K$520,\n          $B252:$B$520, $B251 & \".*\",\n          $B252:$B$520, \"<>\" & $B251 & \".*.*\"\n) )","v":0},{"$f":"IF( $G251 <> \"\",\n     TRUNC( $H251 * $J251, 2 ),\n     SUMIFS( $L252:$L$520,\n              $B252:$B$520, $B251 & \".*\",\n              $B252:$B$520, \"<>\" & $B251 & \".*.*\"\n     ) )","v":0}]
[null,"6.9.6",null,null,"CABEÇOTE DE ALUMÍNIO DE 4\"","FORN","UNID.",null,null,0,{"$f":"IF( $G252 <> \"\",\nTRUNC( $H252 * $I252, 2 ),\nSUMIFS( $K253:$K$520,\n          $B253:$B$520, $B252 & \".*\",\n          $B253:$B$520, \"<>\" & $B252 & \".*.*\"\n) )","v":0},{"$f":"IF( $G252 <> \"\",\n     TRUNC( $H252 * $J252, 2 ),\n     SUMIFS( $L253:$L$520,\n              $B253:$B$520, $B252 & \".*\",\n              $B253:$B$520, \"<>\" & $B252 & \".*.*\"\n     ) )","v":0}]
[null,"6.9.7",null,null,"CURVA 90° FERRO GALVANIZADO D= 3/4\"","FORN","UNID.",null,null,0,{"$f":"IF( $G253 <> \"\",\nTRUNC( $H253 * $I253, 2 ),\nSUMIFS( $K254:$K$520,\n          $B254:$B$520, $B253 & \".*\",\n          $B254:$B$520, \"<>\" & $B253 & \".*.*\"\n) )","v":0},{"$f":"IF( $G253 <> \"\",\n     TRUNC( $H253 * $J253, 2 ),\n     SUMIFS( $L254:$L$520,\n              $B254:$B$520, $B253 & \".*\",\n              $B254:$B$520, \"<>\" & $B253 & \".*.*\"\n     ) )","v":0}]
[null,"6.9.8",null,null,"CONDULETE DE ALUMÍNIO, TIPO E, ELETRODUTO DE AÇO GALVANIZADO DN 25 MM (1''), APARENTE - FORNECIMENTO E INSTALAÇÃO. AF_10/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G254 <> \"\",\nTRUNC( $H254 * $I254, 2 ),\nSUMIFS( $K255:$K$520,\n          $B255:$B$520, $B254 & \".*\",\n          $B255:$B$520, \"<>\" & $B254 & \".*.*\"\n) )","v":0},{"$f":"IF( $G254 <> \"\",\n     TRUNC( $H254 * $J254, 2 ),\n     SUMIFS( $L255:$L$520,\n              $B255:$B$520, $B254 & \".*\",\n              $B255:$B$520, \"<>\" & $B254 & \".*.*\"\n     ) )","v":0}]
[null,"6.9.9",null,null,"ABRAÇADEIRA DE ALUMÍNIO 1 \" 25MM (DAISA BC-100) OU SIMILAR","SERV","UNID.",null,null,0,{"$f":"IF( $G255 <> \"\",\nTRUNC( $H255 * $I255, 2 ),\nSUMIFS( $K256:$K$520,\n          $B256:$B$520, $B255 & \".*\",\n          $B256:$B$520, \"<>\" & $B255 & \".*.*\"\n) )","v":0},{"$f":"IF( $G255 <> \"\",\n     TRUNC( $H255 * $J255, 2 ),\n     SUMIFS( $L256:$L$520,\n              $B256:$B$520, $B255 & \".*\",\n              $B256:$B$520, \"<>\" & $B255 & \".*.*\"\n     ) )","v":0}]
[null,"6.9.10",null,null,"ELETRODUTO FLEXÍVEL CORRUGADO REFORÇADO, PVC, DN 32 MM (1\"), PARA CIRCUITOS TERMINAIS, INSTALADO EM LAJE - FORNECIMENTO E INSTALAÇÃO. AF_03/2023","SERV","M",null,null,0,{"$f":"IF( $G256 <> \"\",\nTRUNC( $H256 * $I256, 2 ),\nSUMIFS( $K257:$K$520,\n          $B257:$B$520, $B256 & \".*\",\n          $B257:$B$520, \"<>\" & $B256 & \".*.*\"\n) )","v":0},{"$f":"IF( $G256 <> \"\",\n     TRUNC( $H256 * $J256, 2 ),\n     SUMIFS( $L257:$L$520,\n              $B257:$B$520, $B256 & \".*\",\n              $B257:$B$520, \"<>\" & $B256 & \".*.*\"\n     ) )","v":0}]
[null,"6.9.11",null,null,"ELETRODUTO RÍGIDO ROSCÁVEL, PVC, DN 25 MM (3/4\"), PARA CIRCUITOS TERMINAIS, INSTALADO EM PAREDE - FORNECIMENTO E INSTALAÇÃO. AF_03/2023","SERV","M",null,null,0,{"$f":"IF( $G257 <> \"\",\nTRUNC( $H257 * $I257, 2 ),\nSUMIFS( $K258:$K$520,\n          $B258:$B$520, $B257 & \".*\",\n          $B258:$B$520, \"<>\" & $B257 & \".*.*\"\n) )","v":0},{"$f":"IF( $G257 <> \"\",\n     TRUNC( $H257 * $J257, 2 ),\n     SUMIFS( $L258:$L$520,\n              $B258:$B$520, $B257 & \".*\",\n              $B258:$B$520, \"<>\" & $B257 & \".*.*\"\n     ) )","v":0}]
[null,"6.9.12",null,null,"CURVA 90 GRAUS PARA ELETRODUTO, PVC, ROSCÁVEL, DN 25 MM (3/4\"), PARA CIRCUITOS TERMINAIS, INSTALADA EM FORRO - FORNECIMENTO E INSTALAÇÃO. AF_03/2023","SERV","UNID.",null,null,0,{"$f":"IF( $G258 <> \"\",\nTRUNC( $H258 * $I258, 2 ),\nSUMIFS( $K259:$K$520,\n          $B259:$B$520, $B258 & \".*\",\n          $B259:$B$520, \"<>\" & $B258 & \".*.*\"\n) )","v":0},{"$f":"IF( $G258 <> \"\",\n     TRUNC( $H258 * $J258, 2 ),\n     SUMIFS( $L259:$L$520,\n              $B259:$B$520, $B258 & \".*\",\n              $B259:$B$520, \"<>\" & $B258 & \".*.*\"\n     ) )","v":0}]
[null,"6.9.13",null,null,"FORNECIMENTO E INSTALAÇÃO DE PARAFUSO CABEÇA CHATA ROSCA SOBERBAL 6,10 X 65MM, COM BUCHA DE NYLON S10 SEM ABAS","SERV","UNID.",null,null,0,{"$f":"IF( $G259 <> \"\",\nTRUNC( $H259 * $I259, 2 ),\nSUMIFS( $K260:$K$520,\n          $B260:$B$520, $B259 & \".*\",\n          $B260:$B$520, \"<>\" & $B259 & \".*.*\"\n) )","v":0},{"$f":"IF( $G259 <> \"\",\n     TRUNC( $H259 * $J259, 2 ),\n     SUMIFS( $L260:$L$520,\n              $B260:$B$520, $B259 & \".*\",\n              $B260:$B$520, \"<>\" & $B259 & \".*.*\"\n     ) )","v":0}]
[null,"6.9.14",null,null,"BUCHA DE NYLON SEM ABA S10, COM PARAFUSO DE 6,10 X 65 MM EM ACO ZINCADO COM ROSCA SOBERBA, CABECA CHATA E FENDA PHILLIPS","FORN","UNID.",null,null,0,{"$f":"IF( $G260 <> \"\",\nTRUNC( $H260 * $I260, 2 ),\nSUMIFS( $K261:$K$520,\n          $B261:$B$520, $B260 & \".*\",\n          $B261:$B$520, \"<>\" & $B260 & \".*.*\"\n) )","v":0},{"$f":"IF( $G260 <> \"\",\n     TRUNC( $H260 * $J260, 2 ),\n     SUMIFS( $L261:$L$520,\n              $B261:$B$520, $B260 & \".*\",\n              $B261:$B$520, \"<>\" & $B260 & \".*.*\"\n     ) )","v":0}]
[null,"6.9.15",null,null,"PARAFUSO FENDA EM AÇO INOX AUTO-ATARRACHANTE D=4,2 X 32MM, REF:TEL-5333","FORN","UNID.",null,null,0,{"$f":"IF( $G261 <> \"\",\nTRUNC( $H261 * $I261, 2 ),\nSUMIFS( $K262:$K$520,\n          $B262:$B$520, $B261 & \".*\",\n          $B262:$B$520, \"<>\" & $B261 & \".*.*\"\n) )","v":0},{"$f":"IF( $G261 <> \"\",\n     TRUNC( $H261 * $J261, 2 ),\n     SUMIFS( $L262:$L$520,\n              $B262:$B$520, $B261 & \".*\",\n              $B262:$B$520, \"<>\" & $B261 & \".*.*\"\n     ) )","v":0}]
[null,"6.9.16",null,null,"PARAFUSO DE ACO ZINCADO COM ROSCA SOBERBA, CABECA CHATA E FENDA SIMPLES, DIAMETRO 4,8 MM, COMPRIMENTO 45 MM","FORN","UNID.",null,null,0,{"$f":"IF( $G262 <> \"\",\nTRUNC( $H262 * $I262, 2 ),\nSUMIFS( $K263:$K$520,\n          $B263:$B$520, $B262 & \".*\",\n          $B263:$B$520, \"<>\" & $B262 & \".*.*\"\n) )","v":0},{"$f":"IF( $G262 <> \"\",\n     TRUNC( $H262 * $J262, 2 ),\n     SUMIFS( $L263:$L$520,\n              $B263:$B$520, $B262 & \".*\",\n              $B263:$B$520, \"<>\" & $B262 & \".*.*\"\n     ) )","v":0}]
[null,"6.9.17",null,null,"ARRUELA DE PRESSÃO 1/4\"","SERV","UNID.",null,null,0,{"$f":"IF( $G263 <> \"\",\nTRUNC( $H263 * $I263, 2 ),\nSUMIFS( $K264:$K$520,\n          $B264:$B$520, $B263 & \".*\",\n          $B264:$B$520, \"<>\" & $B263 & \".*.*\"\n) )","v":0},{"$f":"IF( $G263 <> \"\",\n     TRUNC( $H263 * $J263, 2 ),\n     SUMIFS( $L264:$L$520,\n              $B264:$B$520, $B263 & \".*\",\n              $B264:$B$520, \"<>\" & $B263 & \".*.*\"\n     ) )","v":0}]
[null,"6.9.18",null,null,"ARRUELA LISA ZINCADA D=1/4\"","SERV","UNID.",null,null,0,{"$f":"IF( $G264 <> \"\",\nTRUNC( $H264 * $I264, 2 ),\nSUMIFS( $K265:$K$520,\n          $B265:$B$520, $B264 & \".*\",\n          $B265:$B$520, \"<>\" & $B264 & \".*.*\"\n) )","v":0},{"$f":"IF( $G264 <> \"\",\n     TRUNC( $H264 * $J264, 2 ),\n     SUMIFS( $L265:$L$520,\n              $B265:$B$520, $B264 & \".*\",\n              $B265:$B$520, \"<>\" & $B264 & \".*.*\"\n     ) )","v":0}]
[null,"6.9.19",null,null,"PORCA ZINCADA, SEXTAVADA, DIAMETRO 1/4\"","FORN","UNID.",null,null,{"$f":"IF(F265<>\"\",\nTRUNC(IF(F265=\"SERV\",I265*(1+$L$5/100),I265*(1+$L$6/100)),2),\n\"\" )","v":0},{"$f":"IF( $G265 <> \"\",\nTRUNC( $H265 * $I265, 2 ),\nSUMIFS( $K266:$K$520,\n          $B266:$B$520, $B265 & \".*\",\n          $B266:$B$520, \"<>\" & $B265 & \".*.*\"\n) )","v":0},{"$f":"IF( $G265 <> \"\",\n     TRUNC( $H265 * $J265, 2 ),\n     SUMIFS( $L266:$L$520,\n              $B266:$B$520, $B265 & \".*\",\n              $B266:$B$520, \"<>\" & $B265 & \".*.*\"\n     ) )","v":0}]
[null,"6.9.20",null,null,"BUCHA DE NYLON SEM ABA S4","FORN","UNID.",null,null,0,{"$f":"IF( $G266 <> \"\",\nTRUNC( $H266 * $I266, 2 ),\nSUMIFS( $K267:$K$520,\n          $B267:$B$520, $B266 & \".*\",\n          $B267:$B$520, \"<>\" & $B266 & \".*.*\"\n) )","v":0},{"$f":"IF( $G266 <> \"\",\n     TRUNC( $H266 * $J266, 2 ),\n     SUMIFS( $L267:$L$520,\n              $B267:$B$520, $B266 & \".*\",\n              $B267:$B$520, \"<>\" & $B266 & \".*.*\"\n     ) )","v":0}]
[null,"6.9.21",null,null,"POSTE EM TUBO DE AÇO GALVANIZADO, PESADO, D=2\" (50MM), ALTURA ÚTIL=2,50M, ALTURA TOTAL=3,20M","SERV","UNID.",null,null,0,{"$f":"IF( $G267 <> \"\",\nTRUNC( $H267 * $I267, 2 ),\nSUMIFS( $K268:$K$520,\n          $B268:$B$520, $B267 & \".*\",\n          $B268:$B$520, \"<>\" & $B267 & \".*.*\"\n) )","v":0},{"$f":"IF( $G267 <> \"\",\n     TRUNC( $H267 * $J267, 2 ),\n     SUMIFS( $L268:$L$520,\n              $B268:$B$520, $B267 & \".*\",\n              $B268:$B$520, \"<>\" & $B267 & \".*.*\"\n     ) )","v":0}]
[null,"6.9.22",null,null,"CÂMERA VM S5040 VF 1/3, 760 LINHAS 2.8 A 12MM, DA INTELBRAS OU SIMILAR","SERV","UNID.",null,null,0,{"$f":"IF( $G268 <> \"\",\nTRUNC( $H268 * $I268, 2 ),\nSUMIFS( $K269:$K$520,\n          $B269:$B$520, $B268 & \".*\",\n          $B269:$B$520, \"<>\" & $B268 & \".*.*\"\n) )","v":0},{"$f":"IF( $G268 <> \"\",\n     TRUNC( $H268 * $J268, 2 ),\n     SUMIFS( $L269:$L$520,\n              $B269:$B$520, $B268 & \".*\",\n              $B269:$B$520, \"<>\" & $B268 & \".*.*\"\n     ) )","v":0}]
[null,"6.9.23",null,null,"CABO COAXIAL RG-6","SERV","M",null,null,0,{"$f":"IF( $G269 <> \"\",\nTRUNC( $H269 * $I269, 2 ),\nSUMIFS( $K270:$K$520,\n          $B270:$B$520, $B269 & \".*\",\n          $B270:$B$520, \"<>\" & $B269 & \".*.*\"\n) )","v":0},{"$f":"IF( $G269 <> \"\",\n     TRUNC( $H269 * $J269, 2 ),\n     SUMIFS( $L270:$L$520,\n              $B270:$B$520, $B269 & \".*\",\n              $B270:$B$520, \"<>\" & $B269 & \".*.*\"\n     ) )","v":0}]
[null,"6.9.24",null,null,"SISTEMA DE VDR PARA 40 CÂMERAS COM GRAVAÇÃO CONTÍNUA. CAPACIDADE DE ARMAZENAMENTO DO SISTEMA DE 30TB. FORNECIDO COM MATERIAIS E EQUIPAMENTOS COMPLEMENTARES PARA CORRETO FUNCIONAMENTO DO SISTEMA.","FORN","UNID.",null,null,0,{"$f":"IF( $G270 <> \"\",\nTRUNC( $H270 * $I270, 2 ),\nSUMIFS( $K271:$K$520,\n          $B271:$B$520, $B270 & \".*\",\n          $B271:$B$520, \"<>\" & $B270 & \".*.*\"\n) )","v":0},{"$f":"IF( $G270 <> \"\",\n     TRUNC( $H270 * $J270, 2 ),\n     SUMIFS( $L271:$L$520,\n              $B271:$B$520, $B270 & \".*\",\n              $B271:$B$520, \"<>\" & $B270 & \".*.*\"\n     ) )","v":0}]
[null,"6.9.25",null,null,"FORNECIMENTO E INSTALAÇÃO DE NOBREAK NHS PRIME SENOIDALL, REF. 91.C1.030004 (PRIME 3000VA COM 08 BATERIAS SELADAS 7AH/S.120V/C.ETH). COR PRETA. OU SIMILAR.","SERV","UNID.",null,null,0,{"$f":"IF( $G271 <> \"\",\nTRUNC( $H271 * $I271, 2 ),\nSUMIFS( $K272:$K$520,\n          $B272:$B$520, $B271 & \".*\",\n          $B272:$B$520, \"<>\" & $B271 & \".*.*\"\n) )","v":0},{"$f":"IF( $G271 <> \"\",\n     TRUNC( $H271 * $J271, 2 ),\n     SUMIFS( $L272:$L$520,\n              $B272:$B$520, $B271 & \".*\",\n              $B272:$B$520, \"<>\" & $B271 & \".*.*\"\n     ) )","v":0}]
[null,"6.9.26",null,null,"CAIXA DE PASSAGEM PARA TELEFONE 15X15X10CM (SOBREPOR), FORNECIMENTO E INSTALACAO. AF_11/2019","SERV","UNID.",null,null,0,{"$f":"IF( $G272 <> \"\",\nTRUNC( $H272 * $I272, 2 ),\nSUMIFS( $K273:$K$520,\n          $B273:$B$520, $B272 & \".*\",\n          $B273:$B$520, \"<>\" & $B272 & \".*.*\"\n) )","v":0},{"$f":"IF( $G272 <> \"\",\n     TRUNC( $H272 * $J272, 2 ),\n     SUMIFS( $L273:$L$520,\n              $B273:$B$520, $B272 & \".*\",\n              $B273:$B$520, \"<>\" & $B272 & \".*.*\"\n     ) )","v":0}]
[null,"6.9.27",null,null,"CABO ELETRÔNICO CATEGORIA 6, INSTALADO EM EDIFICAÇÃO INSTITUCIONAL - FORNECIMENTO E INSTALAÇÃO. AF_11/2019","SERV","M",null,null,0,{"$f":"IF( $G273 <> \"\",\nTRUNC( $H273 * $I273, 2 ),\nSUMIFS( $K274:$K$520,\n          $B274:$B$520, $B273 & \".*\",\n          $B274:$B$520, \"<>\" & $B273 & \".*.*\"\n) )","v":0},{"$f":"IF( $G273 <> \"\",\n     TRUNC( $H273 * $J273, 2 ),\n     SUMIFS( $L274:$L$520,\n              $B274:$B$520, $B273 & \".*\",\n              $B274:$B$520, \"<>\" & $B273 & \".*.*\"\n     ) )","v":0}]
[null,"6.9.28",null,null,"TOMADA DE REDE RJ45 - FORNECIMENTO E INSTALAÇÃO. AF_11/2019","SERV","UNID.",null,null,0,{"$f":"IF( $G274 <> \"\",\nTRUNC( $H274 * $I274, 2 ),\nSUMIFS( $K275:$K$520,\n          $B275:$B$520, $B274 & \".*\",\n          $B275:$B$520, \"<>\" & $B274 & \".*.*\"\n) )","v":0},{"$f":"IF( $G274 <> \"\",\n     TRUNC( $H274 * $J274, 2 ),\n     SUMIFS( $L275:$L$520,\n              $B275:$B$520, $B274 & \".*\",\n              $B275:$B$520, \"<>\" & $B274 & \".*.*\"\n     ) )","v":0}]
[null,"6.9.29",null,null,"TOMADA LÓGICA RJ-45, COM 2 MÓDULOS - SISTEMA X","SERV","UNID.",null,null,0,{"$f":"IF( $G275 <> \"\",\nTRUNC( $H275 * $I275, 2 ),\nSUMIFS( $K276:$K$520,\n          $B276:$B$520, $B275 & \".*\",\n          $B276:$B$520, \"<>\" & $B275 & \".*.*\"\n) )","v":0},{"$f":"IF( $G275 <> \"\",\n     TRUNC( $H275 * $J275, 2 ),\n     SUMIFS( $L276:$L$520,\n              $B276:$B$520, $B275 & \".*\",\n              $B276:$B$520, \"<>\" & $B275 & \".*.*\"\n     ) )","v":0}]
[null,"6.9.30",null,null,"RACK FECHADO PARA SERVIDOR - FORNECIMENTO E INSTALAÇÃO. AF_11/2019","SERV","UNID.",null,null,0,{"$f":"IF( $G276 <> \"\",\nTRUNC( $H276 * $I276, 2 ),\nSUMIFS( $K277:$K$520,\n          $B277:$B$520, $B276 & \".*\",\n          $B277:$B$520, \"<>\" & $B276 & \".*.*\"\n) )","v":0},{"$f":"IF( $G276 <> \"\",\n     TRUNC( $H276 * $J276, 2 ),\n     SUMIFS( $L277:$L$520,\n              $B277:$B$520, $B276 & \".*\",\n              $B277:$B$520, \"<>\" & $B276 & \".*.*\"\n     ) )","v":0}]
[null,"6.9.31",null,null,"SWITCH 24 PORTAS 10/100 MBPS - FORNECIMENTO","SERV","UNID.",null,null,0,{"$f":"IF( $G277 <> \"\",\nTRUNC( $H277 * $I277, 2 ),\nSUMIFS( $K278:$K$520,\n          $B278:$B$520, $B277 & \".*\",\n          $B278:$B$520, \"<>\" & $B277 & \".*.*\"\n) )","v":0},{"$f":"IF( $G277 <> \"\",\n     TRUNC( $H277 * $J277, 2 ),\n     SUMIFS( $L278:$L$520,\n              $B278:$B$520, $B277 & \".*\",\n              $B278:$B$520, \"<>\" & $B277 & \".*.*\"\n     ) )","v":0}]
[null,"6.9.32",null,null,"FORNECIMENTO E INSTALAÇÃO DE PATCH CORDS 110/RJ45 C/1,50M - REV 01","SERV","UNID.",null,null,0,{"$f":"IF( $G278 <> \"\",\nTRUNC( $H278 * $I278, 2 ),\nSUMIFS( $K279:$K$520,\n          $B279:$B$520, $B278 & \".*\",\n          $B279:$B$520, \"<>\" & $B278 & \".*.*\"\n) )","v":0},{"$f":"IF( $G278 <> \"\",\n     TRUNC( $H278 * $J278, 2 ),\n     SUMIFS( $L279:$L$520,\n              $B279:$B$520, $B278 & \".*\",\n              $B279:$B$520, \"<>\" & $B278 & \".*.*\"\n     ) )","v":0}]
[null,"6.9.33",null,null,"FORNECIMENTO E INSTALAÇÃO DE ELETROCALHA PERFURADA 100 X   100 X 3000 MM (REF. MOPA OU SIMILAR)","SERV","UNID.",null,null,0,{"$f":"IF( $G279 <> \"\",\nTRUNC( $H279 * $I279, 2 ),\nSUMIFS( $K280:$K$520,\n          $B280:$B$520, $B279 & \".*\",\n          $B280:$B$520, \"<>\" & $B279 & \".*.*\"\n) )","v":0},{"$f":"IF( $G279 <> \"\",\n     TRUNC( $H279 * $J279, 2 ),\n     SUMIFS( $L280:$L$520,\n              $B280:$B$520, $B279 & \".*\",\n              $B280:$B$520, \"<>\" & $B279 & \".*.*\"\n     ) )","v":0}]
[null,"6.9.34",null,null,"CURVA HORIZONTAL 100 X 100 MM, LISA, ZINCADA, PARA ELETROCALHA METÁLICA, COM ÂNGULO 90°, (REF.: MOPA OU SIMILAR)","SERV","UNID.",null,null,0,{"$f":"IF( $G280 <> \"\",\nTRUNC( $H280 * $I280, 2 ),\nSUMIFS( $K281:$K$520,\n          $B281:$B$520, $B280 & \".*\",\n          $B281:$B$520, \"<>\" & $B280 & \".*.*\"\n) )","v":0},{"$f":"IF( $G280 <> \"\",\n     TRUNC( $H280 * $J280, 2 ),\n     SUMIFS( $L281:$L$520,\n              $B281:$B$520, $B280 & \".*\",\n              $B281:$B$520, \"<>\" & $B280 & \".*.*\"\n     ) )","v":0}]
[null,"6.9.35",null,null,"TÊ HORIZONTAL 100 X 100 MM PARA ELETROCALHA METÁLICA (REF. MOPA OU SIMILAR)","SERV","UNID.",null,null,0,{"$f":"IF( $G281 <> \"\",\nTRUNC( $H281 * $I281, 2 ),\nSUMIFS( $K282:$K$520,\n          $B282:$B$520, $B281 & \".*\",\n          $B282:$B$520, \"<>\" & $B281 & \".*.*\"\n) )","v":0},{"$f":"IF( $G281 <> \"\",\n     TRUNC( $H281 * $J281, 2 ),\n     SUMIFS( $L282:$L$520,\n              $B282:$B$520, $B281 & \".*\",\n              $B282:$B$520, \"<>\" & $B281 & \".*.*\"\n     ) )","v":0}]
[null,"6.9.36",null,null,"TÊ VERTICAL DESCIDA LATERAL 100 X 75 MM, LISO, ZINCADO, PARA ELETROCALHA METÁLICA (REF.: MOPA OU SIMILAR)","SERV","UNID.",null,null,0,{"$f":"IF( $G282 <> \"\",\nTRUNC( $H282 * $I282, 2 ),\nSUMIFS( $K283:$K$520,\n          $B283:$B$520, $B282 & \".*\",\n          $B283:$B$520, \"<>\" & $B282 & \".*.*\"\n) )","v":0},{"$f":"IF( $G282 <> \"\",\n     TRUNC( $H282 * $J282, 2 ),\n     SUMIFS( $L283:$L$520,\n              $B283:$B$520, $B282 & \".*\",\n              $B283:$B$520, \"<>\" & $B282 & \".*.*\"\n     ) )","v":0}]
[null,"6.9.37",null,null,"TÊ VERTICAL  DE SUBIDA 100 X 75 MM, LISO, ZINCADA, PARA ELETROCALHA METÁLICA (REF. MOPA OU SIMILAR)","SERV","UNID.",null,null,0,{"$f":"IF( $G283 <> \"\",\nTRUNC( $H283 * $I283, 2 ),\nSUMIFS( $K284:$K$520,\n          $B284:$B$520, $B283 & \".*\",\n          $B284:$B$520, \"<>\" & $B283 & \".*.*\"\n) )","v":0},{"$f":"IF( $G283 <> \"\",\n     TRUNC( $H283 * $J283, 2 ),\n     SUMIFS( $L284:$L$520,\n              $B284:$B$520, $B283 & \".*\",\n              $B284:$B$520, \"<>\" & $B283 & \".*.*\"\n     ) )","v":0}]
[null,"6.9.38",null,null,"FORNECIMENTO E INSTALAÇÃO DE SAÍDA HORIZONTAL PARA ELETRODUTO 4\" (REF. MOPA OU SIMILAR)","SERV","UNID.",null,null,0,{"$f":"IF( $G284 <> \"\",\nTRUNC( $H284 * $I284, 2 ),\nSUMIFS( $K285:$K$520,\n          $B285:$B$520, $B284 & \".*\",\n          $B285:$B$520, \"<>\" & $B284 & \".*.*\"\n) )","v":0},{"$f":"IF( $G284 <> \"\",\n     TRUNC( $H284 * $J284, 2 ),\n     SUMIFS( $L285:$L$520,\n              $B285:$B$520, $B284 & \".*\",\n              $B285:$B$520, \"<>\" & $B284 & \".*.*\"\n     ) )","v":0}]
[null,"6.9.39",null,null,"TALA PLANA PERFURADA 100MM PARA ELETROCALHA METÁLICA (REF.: MOPA OU SIMILAR) - REV 01","SERV","UNID.",null,null,0,{"$f":"IF( $G285 <> \"\",\nTRUNC( $H285 * $I285, 2 ),\nSUMIFS( $K286:$K$520,\n          $B286:$B$520, $B285 & \".*\",\n          $B286:$B$520, \"<>\" & $B285 & \".*.*\"\n) )","v":0},{"$f":"IF( $G285 <> \"\",\n     TRUNC( $H285 * $J285, 2 ),\n     SUMIFS( $L286:$L$520,\n              $B286:$B$520, $B285 & \".*\",\n              $B286:$B$520, \"<>\" & $B285 & \".*.*\"\n     ) )","v":0}]
[null,"6.9.40",null,null,"EMENDA INTERNA 100 X 100 MM COM BASE LISA PERFURADA PARA ELETROCALHA METÁLICA(REF. MOPA OU SIMILAR)","SERV","UNID.",null,null,0,{"$f":"IF( $G286 <> \"\",\nTRUNC( $H286 * $I286, 2 ),\nSUMIFS( $K287:$K$520,\n          $B287:$B$520, $B286 & \".*\",\n          $B287:$B$520, \"<>\" & $B286 & \".*.*\"\n) )","v":0},{"$f":"IF( $G286 <> \"\",\n     TRUNC( $H286 * $J286, 2 ),\n     SUMIFS( $L287:$L$520,\n              $B287:$B$520, $B286 & \".*\",\n              $B287:$B$520, \"<>\" & $B286 & \".*.*\"\n     ) )","v":0}]
[null,"6.9.41",null,null,"TERMINAL 100 X 100 MM, ZINCADO, PARA ELETROCALHA METALICA (REF. MOPA OU SIMILAR)","SERV","UNID.",null,null,0,{"$f":"IF( $G287 <> \"\",\nTRUNC( $H287 * $I287, 2 ),\nSUMIFS( $K288:$K$520,\n          $B288:$B$520, $B287 & \".*\",\n          $B288:$B$520, \"<>\" & $B287 & \".*.*\"\n) )","v":0},{"$f":"IF( $G287 <> \"\",\n     TRUNC( $H287 * $J287, 2 ),\n     SUMIFS( $L288:$L$520,\n              $B288:$B$520, $B287 & \".*\",\n              $B288:$B$520, \"<>\" & $B287 & \".*.*\"\n     ) )","v":0}]
[null,"6.9.42",null,null,"TAMPA DE ENCAIXE 100 X 3000 MM, ZINCADA, PARA ELETROCALHA METÁLICA (REF.: MOPA OU SIMILAR)","SERV","M",null,null,0,{"$f":"IF( $G288 <> \"\",\nTRUNC( $H288 * $I288, 2 ),\nSUMIFS( $K289:$K$520,\n          $B289:$B$520, $B288 & \".*\",\n          $B289:$B$520, \"<>\" & $B288 & \".*.*\"\n) )","v":0},{"$f":"IF( $G288 <> \"\",\n     TRUNC( $H288 * $J288, 2 ),\n     SUMIFS( $L289:$L$520,\n              $B289:$B$520, $B288 & \".*\",\n              $B289:$B$520, \"<>\" & $B288 & \".*.*\"\n     ) )","v":0}]
[null,"6.9.43",null,null,"TAMPA DE ENCAIXE 100MM PARA TÊ HORIZONTAL, ZINCADA, PARA ELETROCALHA METÁLICA(REF.: MOPA OU SIMILAR)","SERV","UNID.",null,null,0,{"$f":"IF( $G289 <> \"\",\nTRUNC( $H289 * $I289, 2 ),\nSUMIFS( $K290:$K$520,\n          $B290:$B$520, $B289 & \".*\",\n          $B290:$B$520, \"<>\" & $B289 & \".*.*\"\n) )","v":0},{"$f":"IF( $G289 <> \"\",\n     TRUNC( $H289 * $J289, 2 ),\n     SUMIFS( $L290:$L$520,\n              $B290:$B$520, $B289 & \".*\",\n              $B290:$B$520, \"<>\" & $B289 & \".*.*\"\n     ) )","v":0}]
[null,"6.9.44",null,null,"TAMPA DE ENCAIXE PARA CURVA 90º, HORIZONTAL, 100MM, ZINCADA, PARA ELETROCALHAMETÁLICA","SERV","UNID.",null,null,0,{"$f":"IF( $G290 <> \"\",\nTRUNC( $H290 * $I290, 2 ),\nSUMIFS( $K291:$K$520,\n          $B291:$B$520, $B290 & \".*\",\n          $B291:$B$520, \"<>\" & $B290 & \".*.*\"\n) )","v":0},{"$f":"IF( $G290 <> \"\",\n     TRUNC( $H290 * $J290, 2 ),\n     SUMIFS( $L291:$L$520,\n              $B291:$B$520, $B290 & \".*\",\n              $B291:$B$520, \"<>\" & $B290 & \".*.*\"\n     ) )","v":0}]
[null,"6.9.45",null,null,"ESCAVAÇÃO MANUAL DE VALA. AF_09/2024","SERV","M³",null,null,0,{"$f":"IF( $G291 <> \"\",\nTRUNC( $H291 * $I291, 2 ),\nSUMIFS( $K292:$K$520,\n          $B292:$B$520, $B291 & \".*\",\n          $B292:$B$520, \"<>\" & $B291 & \".*.*\"\n) )","v":0},{"$f":"IF( $G291 <> \"\",\n     TRUNC( $H291 * $J291, 2 ),\n     SUMIFS( $L292:$L$520,\n              $B292:$B$520, $B291 & \".*\",\n              $B292:$B$520, \"<>\" & $B291 & \".*.*\"\n     ) )","v":0}]
[null,7,null,null,"INSTALAÇÕES HIDROSSANITÁRIAS",{"$nulls":4},"",{"$f":"IF( $G292 <> \"\",\nTRUNC( $H292 * $I292, 2 ),\nSUMIFS( $K293:$K$520,\n          $B293:$B$520, $B292 & \".*\",\n          $B293:$B$520, \"<>\" & $B292 & \".*.*\"\n) )","v":0},{"$f":"IF( $G292 <> \"\",\n     TRUNC( $H292 * $J292, 2 ),\n     SUMIFS( $L293:$L$520,\n              $B293:$B$520, $B292 & \".*\",\n              $B293:$B$520, \"<>\" & $B292 & \".*.*\"\n     ) )","v":0}]
[null,"7.1",null,null,"INSTALAÇÕES DE ÁGUA FRIA",{"$nulls":4},"",{"$f":"IF( $G293 <> \"\",\nTRUNC( $H293 * $I293, 2 ),\nSUMIFS( $K294:$K$520,\n          $B294:$B$520, $B293 & \".*\",\n          $B294:$B$520, \"<>\" & $B293 & \".*.*\"\n) )","v":0},{"$f":"IF( $G293 <> \"\",\n     TRUNC( $H293 * $J293, 2 ),\n     SUMIFS( $L294:$L$520,\n              $B294:$B$520, $B293 & \".*\",\n              $B294:$B$520, \"<>\" & $B293 & \".*.*\"\n     ) )","v":0}]
[null,"7.1.1",null,null,"MICTÓRIO SIFONADO LOUÇA BRANCA - PADRÃO MÉDIO - FORNECIMENTO E INSTALAÇÃO. AF_01/2020","SERV","UNID.",null,null,0,{"$f":"IF( $G294 <> \"\",\nTRUNC( $H294 * $I294, 2 ),\nSUMIFS( $K295:$K$520,\n          $B295:$B$520, $B294 & \".*\",\n          $B295:$B$520, \"<>\" & $B294 & \".*.*\"\n) )","v":0},{"$f":"IF( $G294 <> \"\",\n     TRUNC( $H294 * $J294, 2 ),\n     SUMIFS( $L295:$L$520,\n              $B295:$B$520, $B294 & \".*\",\n              $B295:$B$520, \"<>\" & $B294 & \".*.*\"\n     ) )","v":0}]
[null,"7.1.2",null,null,"TORNEIRA CROMADA TUBO MÓVEL, DE MESA, 1/2\" OU 3/4\", PARA PIA DE COZINHA, PADRÃO ALTO - FORNECIMENTO E INSTALAÇÃO. AF_01/2020","SERV","UNID.",null,null,0,{"$f":"IF( $G295 <> \"\",\nTRUNC( $H295 * $I295, 2 ),\nSUMIFS( $K296:$K$520,\n          $B296:$B$520, $B295 & \".*\",\n          $B296:$B$520, \"<>\" & $B295 & \".*.*\"\n) )","v":0},{"$f":"IF( $G295 <> \"\",\n     TRUNC( $H295 * $J295, 2 ),\n     SUMIFS( $L296:$L$520,\n              $B296:$B$520, $B295 & \".*\",\n              $B296:$B$520, \"<>\" & $B295 & \".*.*\"\n     ) )","v":0}]
[null,"7.1.3",null,null,"TORNEIRA PLÁSTICA 3/4\" PARA TANQUE - FORNECIMENTO E INSTALAÇÃO. AF_01/2020","SERV","UNID.",null,null,0,{"$f":"IF( $G296 <> \"\",\nTRUNC( $H296 * $I296, 2 ),\nSUMIFS( $K297:$K$520,\n          $B297:$B$520, $B296 & \".*\",\n          $B297:$B$520, \"<>\" & $B296 & \".*.*\"\n) )","v":0},{"$f":"IF( $G296 <> \"\",\n     TRUNC( $H296 * $J296, 2 ),\n     SUMIFS( $L297:$L$520,\n              $B297:$B$520, $B296 & \".*\",\n              $B297:$B$520, \"<>\" & $B296 & \".*.*\"\n     ) )","v":0}]
[null,"7.1.4",null,null,"TORNEIRA CROMADA DE MESA, 1/2\" OU 3/4\", PARA LAVATÓRIO, PADRÃO MÉDIO - FORNECIMENTO E INSTALAÇÃO. AF_01/2020","SERV","UNID.",null,null,0,{"$f":"IF( $G297 <> \"\",\nTRUNC( $H297 * $I297, 2 ),\nSUMIFS( $K298:$K$520,\n          $B298:$B$520, $B297 & \".*\",\n          $B298:$B$520, \"<>\" & $B297 & \".*.*\"\n) )","v":0},{"$f":"IF( $G297 <> \"\",\n     TRUNC( $H297 * $J297, 2 ),\n     SUMIFS( $L298:$L$520,\n              $B298:$B$520, $B297 & \".*\",\n              $B298:$B$520, \"<>\" & $B297 & \".*.*\"\n     ) )","v":0}]
[null,"7.1.5",null,null,"VASO SANITARIO SIFONADO CONVENCIONAL PARA PCD SEM FURO FRONTAL COM LOUÇA BRANCA SEM ASSENTO, INCLUSO CONJUNTO DE LIGAÇÃO PARA BACIA SANITÁRIA AJUSTÁVEL - FORNECIMENTO E INSTALAÇÃO. AF_01/2020","SERV","UNID.",null,null,0,{"$f":"IF( $G298 <> \"\",\nTRUNC( $H298 * $I298, 2 ),\nSUMIFS( $K299:$K$520,\n          $B299:$B$520, $B298 & \".*\",\n          $B299:$B$520, \"<>\" & $B298 & \".*.*\"\n) )","v":0},{"$f":"IF( $G298 <> \"\",\n     TRUNC( $H298 * $J298, 2 ),\n     SUMIFS( $L299:$L$520,\n              $B299:$B$520, $B298 & \".*\",\n              $B299:$B$520, \"<>\" & $B298 & \".*.*\"\n     ) )","v":0}]
[null,"7.1.6",null,null,"VASO SANITÁRIO SIFONADO COM CAIXA ACOPLADA LOUÇA BRANCA, INCLUSO ENGATE FLEXÍVEL EM PLÁSTICO BRANCO, 1/2  X 40CM - FORNECIMENTO E INSTALAÇÃO. AF_01/2020","SERV","UNID.",null,null,0,{"$f":"IF( $G299 <> \"\",\nTRUNC( $H299 * $I299, 2 ),\nSUMIFS( $K300:$K$520,\n          $B300:$B$520, $B299 & \".*\",\n          $B300:$B$520, \"<>\" & $B299 & \".*.*\"\n) )","v":0},{"$f":"IF( $G299 <> \"\",\n     TRUNC( $H299 * $J299, 2 ),\n     SUMIFS( $L300:$L$520,\n              $B300:$B$520, $B299 & \".*\",\n              $B300:$B$520, \"<>\" & $B299 & \".*.*\"\n     ) )","v":0}]
[null,"7.1.7",null,null,"REGISTRO DE ESFERA, PVC, SOLDÁVEL, COM VOLANTE, DN  25 MM - FORNECIMENTO E INSTALAÇÃO. AF_08/2021","SERV","UNID.",null,null,0,{"$f":"IF( $G300 <> \"\",\nTRUNC( $H300 * $I300, 2 ),\nSUMIFS( $K301:$K$520,\n          $B301:$B$520, $B300 & \".*\",\n          $B301:$B$520, \"<>\" & $B300 & \".*.*\"\n) )","v":0},{"$f":"IF( $G300 <> \"\",\n     TRUNC( $H300 * $J300, 2 ),\n     SUMIFS( $L301:$L$520,\n              $B301:$B$520, $B300 & \".*\",\n              $B301:$B$520, \"<>\" & $B300 & \".*.*\"\n     ) )","v":0}]
[null,"7.1.8",null,null,"REGISTRO DE GAVETA BRUTO, LATÃO, ROSCÁVEL, 3/4\" - FORNECIMENTO E INSTALAÇÃO. AF_08/2021","SERV","UNID.",null,null,0,{"$f":"IF( $G301 <> \"\",\nTRUNC( $H301 * $I301, 2 ),\nSUMIFS( $K302:$K$520,\n          $B302:$B$520, $B301 & \".*\",\n          $B302:$B$520, \"<>\" & $B301 & \".*.*\"\n) )","v":0},{"$f":"IF( $G301 <> \"\",\n     TRUNC( $H301 * $J301, 2 ),\n     SUMIFS( $L302:$L$520,\n              $B302:$B$520, $B301 & \".*\",\n              $B302:$B$520, \"<>\" & $B301 & \".*.*\"\n     ) )","v":0}]
[null,"7.1.9",null,null,"REGISTRO DE GAVETA BRUTO, LATÃO, ROSCÁVEL, 1 1/4\", COM ACABAMENTO E CANOPLA CROMADOS - FORNECIMENTO E INSTALAÇÃO. AF_08/2021","SERV","UNID.",null,null,0,{"$f":"IF( $G302 <> \"\",\nTRUNC( $H302 * $I302, 2 ),\nSUMIFS( $K303:$K$520,\n          $B303:$B$520, $B302 & \".*\",\n          $B303:$B$520, \"<>\" & $B302 & \".*.*\"\n) )","v":0},{"$f":"IF( $G302 <> \"\",\n     TRUNC( $H302 * $J302, 2 ),\n     SUMIFS( $L303:$L$520,\n              $B303:$B$520, $B302 & \".*\",\n              $B303:$B$520, \"<>\" & $B302 & \".*.*\"\n     ) )","v":0}]
[null,"7.1.10",null,null,"REGISTRO DE GAVETA BRUTO, LATÃO, ROSCÁVEL, 3/4\", COM ACABAMENTO E CANOPLA CROMADOS - FORNECIMENTO E INSTALAÇÃO. AF_08/2021","SERV","UNID.",null,null,0,{"$f":"IF( $G303 <> \"\",\nTRUNC( $H303 * $I303, 2 ),\nSUMIFS( $K304:$K$520,\n          $B304:$B$520, $B303 & \".*\",\n          $B304:$B$520, \"<>\" & $B303 & \".*.*\"\n) )","v":0},{"$f":"IF( $G303 <> \"\",\n     TRUNC( $H303 * $J303, 2 ),\n     SUMIFS( $L304:$L$520,\n              $B304:$B$520, $B303 & \".*\",\n              $B304:$B$520, \"<>\" & $B303 & \".*.*\"\n     ) )","v":0}]
[null,"7.1.11",null,null,"ENGATE FLEXÍVEL EM INOX, 1/2  X 30CM - FORNECIMENTO E INSTALAÇÃO. AF_01/2020","SERV","UNID.",null,null,0,{"$f":"IF( $G304 <> \"\",\nTRUNC( $H304 * $I304, 2 ),\nSUMIFS( $K305:$K$520,\n          $B305:$B$520, $B304 & \".*\",\n          $B305:$B$520, \"<>\" & $B304 & \".*.*\"\n) )","v":0},{"$f":"IF( $G304 <> \"\",\n     TRUNC( $H304 * $J304, 2 ),\n     SUMIFS( $L305:$L$520,\n              $B305:$B$520, $B304 & \".*\",\n              $B305:$B$520, \"<>\" & $B304 & \".*.*\"\n     ) )","v":0}]
[null,"7.1.12",null,null,"ENGATE FLEXÍVEL EM PLÁSTICO BRANCO, 1/2\" X 40CM - FORNECIMENTO E INSTALAÇÃO. AF_01/2020","SERV","UNID.",null,null,0,{"$f":"IF( $G305 <> \"\",\nTRUNC( $H305 * $I305, 2 ),\nSUMIFS( $K306:$K$520,\n          $B306:$B$520, $B305 & \".*\",\n          $B306:$B$520, \"<>\" & $B305 & \".*.*\"\n) )","v":0},{"$f":"IF( $G305 <> \"\",\n     TRUNC( $H305 * $J305, 2 ),\n     SUMIFS( $L306:$L$520,\n              $B306:$B$520, $B305 & \".*\",\n              $B306:$B$520, \"<>\" & $B305 & \".*.*\"\n     ) )","v":0}]
[null,"7.1.13",null,null,"JOELHO DE REDUÇÃO, 90 GRAUS, PVC, SOLDÁVEL, DN 25 MM X 20 MM, INSTALADO EM RAMAL OU SUB-RAMAL DE ÁGUA - FORNECIMENTO E INSTALAÇÃO. AF_06/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G306 <> \"\",\nTRUNC( $H306 * $I306, 2 ),\nSUMIFS( $K307:$K$520,\n          $B307:$B$520, $B306 & \".*\",\n          $B307:$B$520, \"<>\" & $B306 & \".*.*\"\n) )","v":0},{"$f":"IF( $G306 <> \"\",\n     TRUNC( $H306 * $J306, 2 ),\n     SUMIFS( $L307:$L$520,\n              $B307:$B$520, $B306 & \".*\",\n              $B307:$B$520, \"<>\" & $B306 & \".*.*\"\n     ) )","v":0}]
[null,"7.1.14",null,null,"CURVA 90 GRAUS, PPR, DN 25 MM, INSTALADO EM RAMAL OU SUB-RAMAL DE ÁGUA - FORNECIMENTO E INSTALAÇÃO. AF_08/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G307 <> \"\",\nTRUNC( $H307 * $I307, 2 ),\nSUMIFS( $K308:$K$520,\n          $B308:$B$520, $B307 & \".*\",\n          $B308:$B$520, \"<>\" & $B307 & \".*.*\"\n) )","v":0},{"$f":"IF( $G307 <> \"\",\n     TRUNC( $H307 * $J307, 2 ),\n     SUMIFS( $L308:$L$520,\n              $B308:$B$520, $B307 & \".*\",\n              $B308:$B$520, \"<>\" & $B307 & \".*.*\"\n     ) )","v":0}]
[null,"7.1.15",null,null,"TUBO, PVC, SOLDÁVEL, DE 25MM, INSTALADO EM RAMAL DE DISTRIBUIÇÃO DE ÁGUA - FORNECIMENTO E INSTALAÇÃO. AF_06/2022","SERV","M",null,null,0,{"$f":"IF( $G308 <> \"\",\nTRUNC( $H308 * $I308, 2 ),\nSUMIFS( $K309:$K$520,\n          $B309:$B$520, $B308 & \".*\",\n          $B309:$B$520, \"<>\" & $B308 & \".*.*\"\n) )","v":0},{"$f":"IF( $G308 <> \"\",\n     TRUNC( $H308 * $J308, 2 ),\n     SUMIFS( $L309:$L$520,\n              $B309:$B$520, $B308 & \".*\",\n              $B309:$B$520, \"<>\" & $B308 & \".*.*\"\n     ) )","v":0}]
[null,"7.1.16",null,null,"ADAPTADOR COM FLANGE E ANEL DE VEDAÇÃO, PVC, SOLDÁVEL, DN 32 MM X 1\", INSTALADO EM RESERVAÇÃO PREDIAL DE ÁGUA - FORNECIMENTO E INSTALAÇÃO. AF_04/2024","SERV","UNID.",null,null,0,{"$f":"IF( $G309 <> \"\",\nTRUNC( $H309 * $I309, 2 ),\nSUMIFS( $K310:$K$520,\n          $B310:$B$520, $B309 & \".*\",\n          $B310:$B$520, \"<>\" & $B309 & \".*.*\"\n) )","v":0},{"$f":"IF( $G309 <> \"\",\n     TRUNC( $H309 * $J309, 2 ),\n     SUMIFS( $L310:$L$520,\n              $B310:$B$520, $B309 & \".*\",\n              $B310:$B$520, \"<>\" & $B309 & \".*.*\"\n     ) )","v":0}]
[null,"7.1.17",null,null,"ADAPTADOR COM FLANGE E ANEL DE VEDAÇÃO, PVC, SOLDÁVEL, DN 40 MM X 1 1/4\", INSTALADO EM RESERVAÇÃO PREDIAL DE ÁGUA - FORNECIMENTO E INSTALAÇÃO. AF_04/2024","SERV","UNID.",null,null,0,{"$f":"IF( $G310 <> \"\",\nTRUNC( $H310 * $I310, 2 ),\nSUMIFS( $K311:$K$520,\n          $B311:$B$520, $B310 & \".*\",\n          $B311:$B$520, \"<>\" & $B310 & \".*.*\"\n) )","v":0},{"$f":"IF( $G310 <> \"\",\n     TRUNC( $H310 * $J310, 2 ),\n     SUMIFS( $L311:$L$520,\n              $B311:$B$520, $B310 & \".*\",\n              $B311:$B$520, \"<>\" & $B310 & \".*.*\"\n     ) )","v":0}]
[null,"7.1.18",null,null,"ADAPTADOR CURTO COM BOLSA E ROSCA PARA REGISTRO, PVC, SOLDÁVEL, DN 25MM X 3/4 , INSTALADO EM RAMAL DE DISTRIBUIÇÃO DE ÁGUA - FORNECIMENTO E INSTALAÇÃO. AF_06/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G311 <> \"\",\nTRUNC( $H311 * $I311, 2 ),\nSUMIFS( $K312:$K$520,\n          $B312:$B$520, $B311 & \".*\",\n          $B312:$B$520, \"<>\" & $B311 & \".*.*\"\n) )","v":0},{"$f":"IF( $G311 <> \"\",\n     TRUNC( $H311 * $J311, 2 ),\n     SUMIFS( $L312:$L$520,\n              $B312:$B$520, $B311 & \".*\",\n              $B312:$B$520, \"<>\" & $B311 & \".*.*\"\n     ) )","v":0}]
[null,"7.1.19",null,null,"ADAPTADOR CURTO COM BOLSA E ROSCA PARA REGISTRO, PVC, SOLDÁVEL, DN 32 MM X 1\", INSTALADO EM RESERVAÇÃO PREDIAL DE ÁGUA - FORNECIMENTO E INSTALAÇÃO. AF_04/2024","SERV","UNID.",null,null,0,{"$f":"IF( $G312 <> \"\",\nTRUNC( $H312 * $I312, 2 ),\nSUMIFS( $K313:$K$520,\n          $B313:$B$520, $B312 & \".*\",\n          $B313:$B$520, \"<>\" & $B312 & \".*.*\"\n) )","v":0},{"$f":"IF( $G312 <> \"\",\n     TRUNC( $H312 * $J312, 2 ),\n     SUMIFS( $L313:$L$520,\n              $B313:$B$520, $B312 & \".*\",\n              $B313:$B$520, \"<>\" & $B312 & \".*.*\"\n     ) )","v":0}]
[null,"7.1.20",null,null,"ADAPTADOR CURTO COM BOLSA E ROSCA PARA REGISTRO, PVC, SOLDÁVEL, DN 40MM X 1.1/4\", INSTALADO EM RAMAL DE DISTRIBUIÇÃO DE ÁGUA - FORNECIMENTO E INSTALAÇÃO. AF_06/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G313 <> \"\",\nTRUNC( $H313 * $I313, 2 ),\nSUMIFS( $K314:$K$520,\n          $B314:$B$520, $B313 & \".*\",\n          $B314:$B$520, \"<>\" & $B313 & \".*.*\"\n) )","v":0},{"$f":"IF( $G313 <> \"\",\n     TRUNC( $H313 * $J313, 2 ),\n     SUMIFS( $L314:$L$520,\n              $B314:$B$520, $B313 & \".*\",\n              $B314:$B$520, \"<>\" & $B313 & \".*.*\"\n     ) )","v":0}]
[null,"7.1.21",null,null,"BUCHA DE REDUÇÃO, PPR, DN 32 X 25 MM, INSTALADO EM RESERVAÇÃO PREDIAL DE ÁGUA - FORNECIMENTO E INSTALAÇÃO. AF_04/2024","SERV","UNID.",null,null,0,{"$f":"IF( $G314 <> \"\",\nTRUNC( $H314 * $I314, 2 ),\nSUMIFS( $K315:$K$520,\n          $B315:$B$520, $B314 & \".*\",\n          $B315:$B$520, \"<>\" & $B314 & \".*.*\"\n) )","v":0},{"$f":"IF( $G314 <> \"\",\n     TRUNC( $H314 * $J314, 2 ),\n     SUMIFS( $L315:$L$520,\n              $B315:$B$520, $B314 & \".*\",\n              $B315:$B$520, \"<>\" & $B314 & \".*.*\"\n     ) )","v":0}]
[null,"7.1.22",null,null,"BUCHA DE REDUÇÃO, PVC, SOLDÁVEL, DN 40MM X 32MM, INSTALADO EM RAMAL DE DISTRIBUIÇÃO DE ÁGUA - FORNECIMENTO E INSTALAÇÃO. AF_06/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G315 <> \"\",\nTRUNC( $H315 * $I315, 2 ),\nSUMIFS( $K316:$K$520,\n          $B316:$B$520, $B315 & \".*\",\n          $B316:$B$520, \"<>\" & $B315 & \".*.*\"\n) )","v":0},{"$f":"IF( $G315 <> \"\",\n     TRUNC( $H315 * $J315, 2 ),\n     SUMIFS( $L316:$L$520,\n              $B316:$B$520, $B315 & \".*\",\n              $B316:$B$520, \"<>\" & $B315 & \".*.*\"\n     ) )","v":0}]
[null,"7.1.23",null,null,"JOELHO PVC, SOLDÁVEL, 45 GRAUS, DN 40 MM, INSTALADO EM RESERVAÇÃO PREDIAL DE ÁGUA - FORNECIMENTO E INSTALAÇÃO. AF_04/2024","SERV","UNID.",null,null,0,{"$f":"IF( $G316 <> \"\",\nTRUNC( $H316 * $I316, 2 ),\nSUMIFS( $K317:$K$520,\n          $B317:$B$520, $B316 & \".*\",\n          $B317:$B$520, \"<>\" & $B316 & \".*.*\"\n) )","v":0},{"$f":"IF( $G316 <> \"\",\n     TRUNC( $H316 * $J316, 2 ),\n     SUMIFS( $L317:$L$520,\n              $B317:$B$520, $B316 & \".*\",\n              $B317:$B$520, \"<>\" & $B316 & \".*.*\"\n     ) )","v":0}]
[null,"7.1.24",null,null,"CRUZETA DE FERRO GALVANIZADO, COM ROSCA BSP, DE 1\"","FORN","UNID.",null,null,0,{"$f":"IF( $G317 <> \"\",\nTRUNC( $H317 * $I317, 2 ),\nSUMIFS( $K318:$K$520,\n          $B318:$B$520, $B317 & \".*\",\n          $B318:$B$520, \"<>\" & $B317 & \".*.*\"\n) )","v":0},{"$f":"IF( $G317 <> \"\",\n     TRUNC( $H317 * $J317, 2 ),\n     SUMIFS( $L318:$L$520,\n              $B318:$B$520, $B317 & \".*\",\n              $B318:$B$520, \"<>\" & $B317 & \".*.*\"\n     ) )","v":0}]
[null,"7.1.25",null,null,"CRUZETA DE FERRO GALVANIZADO, COM ROSCA BSP, DE 1 1/2\"","FORN","UNID.",null,null,0,{"$f":"IF( $G318 <> \"\",\nTRUNC( $H318 * $I318, 2 ),\nSUMIFS( $K319:$K$520,\n          $B319:$B$520, $B318 & \".*\",\n          $B319:$B$520, \"<>\" & $B318 & \".*.*\"\n) )","v":0},{"$f":"IF( $G318 <> \"\",\n     TRUNC( $H318 * $J318, 2 ),\n     SUMIFS( $L319:$L$520,\n              $B319:$B$520, $B318 & \".*\",\n              $B319:$B$520, \"<>\" & $B318 & \".*.*\"\n     ) )","v":0}]
[null,"7.1.26",null,null,"JOELHO 90 GRAUS, PVC, SOLDÁVEL, DN 25MM, INSTALADO EM RAMAL DE DISTRIBUIÇÃO DE ÁGUA - FORNECIMENTO E INSTALAÇÃO. AF_06/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G319 <> \"\",\nTRUNC( $H319 * $I319, 2 ),\nSUMIFS( $K320:$K$520,\n          $B320:$B$520, $B319 & \".*\",\n          $B320:$B$520, \"<>\" & $B319 & \".*.*\"\n) )","v":0},{"$f":"IF( $G319 <> \"\",\n     TRUNC( $H319 * $J319, 2 ),\n     SUMIFS( $L320:$L$520,\n              $B320:$B$520, $B319 & \".*\",\n              $B320:$B$520, \"<>\" & $B319 & \".*.*\"\n     ) )","v":0}]
[null,"7.1.27",null,null,"JOELHO 90 GRAUS, PVC, SOLDÁVEL, DN 32MM, INSTALADO EM RAMAL DE DISTRIBUIÇÃO DE ÁGUA - FORNECIMENTO E INSTALAÇÃO. AF_06/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G320 <> \"\",\nTRUNC( $H320 * $I320, 2 ),\nSUMIFS( $K321:$K$520,\n          $B321:$B$520, $B320 & \".*\",\n          $B321:$B$520, \"<>\" & $B320 & \".*.*\"\n) )","v":0},{"$f":"IF( $G320 <> \"\",\n     TRUNC( $H320 * $J320, 2 ),\n     SUMIFS( $L321:$L$520,\n              $B321:$B$520, $B320 & \".*\",\n              $B321:$B$520, \"<>\" & $B320 & \".*.*\"\n     ) )","v":0}]
[null,"7.1.28",null,null,"JOELHO 90 GRAUS, PVC, SOLDÁVEL, DN 40MM, INSTALADO EM PRUMADA DE ÁGUA - FORNECIMENTO E INSTALAÇÃO. AF_06/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G321 <> \"\",\nTRUNC( $H321 * $I321, 2 ),\nSUMIFS( $K322:$K$520,\n          $B322:$B$520, $B321 & \".*\",\n          $B322:$B$520, \"<>\" & $B321 & \".*.*\"\n) )","v":0},{"$f":"IF( $G321 <> \"\",\n     TRUNC( $H321 * $J321, 2 ),\n     SUMIFS( $L322:$L$520,\n              $B322:$B$520, $B321 & \".*\",\n              $B322:$B$520, \"<>\" & $B321 & \".*.*\"\n     ) )","v":0}]
[null,"7.1.29",null,null,"JOELHO DE REDUÇÃO, 90 GRAUS, PVC, SOLDÁVEL, DN 32 MM X 25 MM, INSTALADO EM RAMAL OU SUB-RAMAL DE ÁGUA - FORNECIMENTO E INSTALAÇÃO. AF_06/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G322 <> \"\",\nTRUNC( $H322 * $I322, 2 ),\nSUMIFS( $K323:$K$520,\n          $B323:$B$520, $B322 & \".*\",\n          $B323:$B$520, \"<>\" & $B322 & \".*.*\"\n) )","v":0},{"$f":"IF( $G322 <> \"\",\n     TRUNC( $H322 * $J322, 2 ),\n     SUMIFS( $L323:$L$520,\n              $B323:$B$520, $B322 & \".*\",\n              $B323:$B$520, \"<>\" & $B322 & \".*.*\"\n     ) )","v":0}]
[null,"7.1.30",null,null,"LUVA DE CORRER, PVC, SOLDÁVEL, DN 32MM, INSTALADO EM RAMAL OU SUB-RAMAL DE ÁGUA   FORNECIMENTO E INSTALAÇÃO. AF_06/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G323 <> \"\",\nTRUNC( $H323 * $I323, 2 ),\nSUMIFS( $K324:$K$520,\n          $B324:$B$520, $B323 & \".*\",\n          $B324:$B$520, \"<>\" & $B323 & \".*.*\"\n) )","v":0},{"$f":"IF( $G323 <> \"\",\n     TRUNC( $H323 * $J323, 2 ),\n     SUMIFS( $L324:$L$520,\n              $B324:$B$520, $B323 & \".*\",\n              $B324:$B$520, \"<>\" & $B323 & \".*.*\"\n     ) )","v":0}]
[null,"7.1.31",null,null,"LUVA, PVC, SOLDÁVEL, DN 40MM, INSTALADO EM RAMAL DE DISTRIBUIÇÃO DE ÁGUA - FORNECIMENTO E INSTALAÇÃO. AF_06/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G324 <> \"\",\nTRUNC( $H324 * $I324, 2 ),\nSUMIFS( $K325:$K$520,\n          $B325:$B$520, $B324 & \".*\",\n          $B325:$B$520, \"<>\" & $B324 & \".*.*\"\n) )","v":0},{"$f":"IF( $G324 <> \"\",\n     TRUNC( $H324 * $J324, 2 ),\n     SUMIFS( $L325:$L$520,\n              $B325:$B$520, $B324 & \".*\",\n              $B325:$B$520, \"<>\" & $B324 & \".*.*\"\n     ) )","v":0}]
[null,"7.1.32",null,null,"TUBO, PVC, SOLDÁVEL, DE 32MM, INSTALADO EM RAMAL DE DISTRIBUIÇÃO DE ÁGUA - FORNECIMENTO E INSTALAÇÃO. AF_06/2022","SERV","M",null,null,0,{"$f":"IF( $G325 <> \"\",\nTRUNC( $H325 * $I325, 2 ),\nSUMIFS( $K326:$K$520,\n          $B326:$B$520, $B325 & \".*\",\n          $B326:$B$520, \"<>\" & $B325 & \".*.*\"\n) )","v":0},{"$f":"IF( $G325 <> \"\",\n     TRUNC( $H325 * $J325, 2 ),\n     SUMIFS( $L326:$L$520,\n              $B326:$B$520, $B325 & \".*\",\n              $B326:$B$520, \"<>\" & $B325 & \".*.*\"\n     ) )","v":0}]
[null,"7.1.33",null,null,"TUBO, PVC, SOLDÁVEL, DE 40MM, INSTALADO EM RAMAL DE DISTRIBUIÇÃO DE ÁGUA - FORNECIMENTO E INSTALAÇÃO. AF_06/2022","SERV","M",null,null,0,{"$f":"IF( $G326 <> \"\",\nTRUNC( $H326 * $I326, 2 ),\nSUMIFS( $K327:$K$520,\n          $B327:$B$520, $B326 & \".*\",\n          $B327:$B$520, \"<>\" & $B326 & \".*.*\"\n) )","v":0},{"$f":"IF( $G326 <> \"\",\n     TRUNC( $H326 * $J326, 2 ),\n     SUMIFS( $L327:$L$520,\n              $B327:$B$520, $B326 & \".*\",\n              $B327:$B$520, \"<>\" & $B326 & \".*.*\"\n     ) )","v":0}]
[null,"7.1.34",null,null,"TE, PVC, SOLDÁVEL, DN 25MM, INSTALADO EM RAMAL DE DISTRIBUIÇÃO DE ÁGUA - FORNECIMENTO E INSTALAÇÃO. AF_06/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G327 <> \"\",\nTRUNC( $H327 * $I327, 2 ),\nSUMIFS( $K328:$K$520,\n          $B328:$B$520, $B327 & \".*\",\n          $B328:$B$520, \"<>\" & $B327 & \".*.*\"\n) )","v":0},{"$f":"IF( $G327 <> \"\",\n     TRUNC( $H327 * $J327, 2 ),\n     SUMIFS( $L328:$L$520,\n              $B328:$B$520, $B327 & \".*\",\n              $B328:$B$520, \"<>\" & $B327 & \".*.*\"\n     ) )","v":0}]
[null,"7.1.35",null,null,"TE, PVC, SOLDÁVEL, DN 32MM, INSTALADO EM RAMAL DE DISTRIBUIÇÃO DE ÁGUA - FORNECIMENTO E INSTALAÇÃO. AF_06/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G328 <> \"\",\nTRUNC( $H328 * $I328, 2 ),\nSUMIFS( $K329:$K$520,\n          $B329:$B$520, $B328 & \".*\",\n          $B329:$B$520, \"<>\" & $B328 & \".*.*\"\n) )","v":0},{"$f":"IF( $G328 <> \"\",\n     TRUNC( $H328 * $J328, 2 ),\n     SUMIFS( $L329:$L$520,\n              $B329:$B$520, $B328 & \".*\",\n              $B329:$B$520, \"<>\" & $B328 & \".*.*\"\n     ) )","v":0}]
[null,"7.1.36",null,null,"TE, PVC, SOLDÁVEL, DN 40MM, INSTALADO EM RAMAL DE DISTRIBUIÇÃO DE ÁGUA - FORNECIMENTO E INSTALAÇÃO. AF_06/2022","SERV","UNID.",null,null,{"$f":"IF(F329<>\"\",\nTRUNC(IF(F329=\"SERV\",I329*(1+$L$5/100),I329*(1+$L$6/100)),2),\n\"\" )","v":0},{"$f":"IF( $G329 <> \"\",\nTRUNC( $H329 * $I329, 2 ),\nSUMIFS( $K330:$K$520,\n          $B330:$B$520, $B329 & \".*\",\n          $B330:$B$520, \"<>\" & $B329 & \".*.*\"\n) )","v":0},{"$f":"IF( $G329 <> \"\",\n     TRUNC( $H329 * $J329, 2 ),\n     SUMIFS( $L330:$L$520,\n              $B330:$B$520, $B329 & \".*\",\n              $B330:$B$520, \"<>\" & $B329 & \".*.*\"\n     ) )","v":0}]
[null,"7.1.37",null,null,"JOELHO 90 GRAUS COM BUCHA DE LATÃO, PVC, SOLDÁVEL, DN 25MM, X 3/4  INSTALADO EM RAMAL OU SUB-RAMAL DE ÁGUA - FORNECIMENTO E INSTALAÇÃO. AF_06/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G330 <> \"\",\nTRUNC( $H330 * $I330, 2 ),\nSUMIFS( $K331:$K$520,\n          $B331:$B$520, $B330 & \".*\",\n          $B331:$B$520, \"<>\" & $B330 & \".*.*\"\n) )","v":0},{"$f":"IF( $G330 <> \"\",\n     TRUNC( $H330 * $J330, 2 ),\n     SUMIFS( $L331:$L$520,\n              $B331:$B$520, $B330 & \".*\",\n              $B331:$B$520, \"<>\" & $B330 & \".*.*\"\n     ) )","v":0}]
[null,"7.1.38",null,null,"JOELHO 90 GRAUS COM BUCHA DE LATÃO, PVC, SOLDÁVEL, DN 25MM, X 1/2  INSTALADO EM RAMAL OU SUB-RAMAL DE ÁGUA - FORNECIMENTO E INSTALAÇÃO. AF_06/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G331 <> \"\",\nTRUNC( $H331 * $I331, 2 ),\nSUMIFS( $K332:$K$520,\n          $B332:$B$520, $B331 & \".*\",\n          $B332:$B$520, \"<>\" & $B331 & \".*.*\"\n) )","v":0},{"$f":"IF( $G331 <> \"\",\n     TRUNC( $H331 * $J331, 2 ),\n     SUMIFS( $L332:$L$520,\n              $B332:$B$520, $B331 & \".*\",\n              $B332:$B$520, \"<>\" & $B331 & \".*.*\"\n     ) )","v":0}]
[null,"7.1.39",null,null,"TÊ COM BUCHA DE LATÃO NA BOLSA CENTRAL, PVC, SOLDÁVEL, DN 32MM X 3/4 , INSTALADO EM RAMAL DE DISTRIBUIÇÃO DE ÁGUA - FORNECIMENTO E INSTALAÇÃO. AF_06/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G332 <> \"\",\nTRUNC( $H332 * $I332, 2 ),\nSUMIFS( $K333:$K$520,\n          $B333:$B$520, $B332 & \".*\",\n          $B333:$B$520, \"<>\" & $B332 & \".*.*\"\n) )","v":0},{"$f":"IF( $G332 <> \"\",\n     TRUNC( $H332 * $J332, 2 ),\n     SUMIFS( $L333:$L$520,\n              $B333:$B$520, $B332 & \".*\",\n              $B333:$B$520, \"<>\" & $B332 & \".*.*\"\n     ) )","v":0}]
[null,"7.1.40",null,null,"CAIXA D´ÁGUA EM POLIÉSTER REFORÇADO COM FIBRA DE VIDRO, 5000 LITROS - FORNECIMENTO E INSTALAÇÃO. AF_06/2021","SERV","UNID.",null,null,0,{"$f":"IF( $G333 <> \"\",\nTRUNC( $H333 * $I333, 2 ),\nSUMIFS( $K334:$K$520,\n          $B334:$B$520, $B333 & \".*\",\n          $B334:$B$520, \"<>\" & $B333 & \".*.*\"\n) )","v":0},{"$f":"IF( $G333 <> \"\",\n     TRUNC( $H333 * $J333, 2 ),\n     SUMIFS( $L334:$L$520,\n              $B334:$B$520, $B333 & \".*\",\n              $B334:$B$520, \"<>\" & $B333 & \".*.*\"\n     ) )","v":0}]
[null,"7.1.41",null,null,"SUPORTE PARA AUXÍLIO DE DEFICIENTES FÍSICOS (BARRA DE APOIO) L = 50CM EM TUBODE FERRO GALVANIZADO D = 1 1/2\"","SERV","UNID.",null,null,0,{"$f":"IF( $G334 <> \"\",\nTRUNC( $H334 * $I334, 2 ),\nSUMIFS( $K335:$K$520,\n          $B335:$B$520, $B334 & \".*\",\n          $B335:$B$520, \"<>\" & $B334 & \".*.*\"\n) )","v":0},{"$f":"IF( $G334 <> \"\",\n     TRUNC( $H334 * $J334, 2 ),\n     SUMIFS( $L335:$L$520,\n              $B335:$B$520, $B334 & \".*\",\n              $B335:$B$520, \"<>\" & $B334 & \".*.*\"\n     ) )","v":0}]
[null,"7.1.42",null,null,"COLAR TOMADA PVC, COM TRAVAS, SAIDA COM ROSCA, DE 32 MM X 1/2\" OU 32 MM X 3/4\", PARA LIGACAO PREDIAL DE AGUA","FORN","UNID.",null,null,0,{"$f":"IF( $G335 <> \"\",\nTRUNC( $H335 * $I335, 2 ),\nSUMIFS( $K336:$K$520,\n          $B336:$B$520, $B335 & \".*\",\n          $B336:$B$520, \"<>\" & $B335 & \".*.*\"\n) )","v":0},{"$f":"IF( $G335 <> \"\",\n     TRUNC( $H335 * $J335, 2 ),\n     SUMIFS( $L336:$L$520,\n              $B336:$B$520, $B335 & \".*\",\n              $B336:$B$520, \"<>\" & $B335 & \".*.*\"\n     ) )","v":0}]
[null,"7.2",null,null,"INSTALAÇÕES DE ESGOTO",{"$nulls":4},"",{"$f":"IF( $G336 <> \"\",\nTRUNC( $H336 * $I336, 2 ),\nSUMIFS( $K337:$K$520,\n          $B337:$B$520, $B336 & \".*\",\n          $B337:$B$520, \"<>\" & $B336 & \".*.*\"\n) )","v":0},{"$f":"IF( $G336 <> \"\",\n     TRUNC( $H336 * $J336, 2 ),\n     SUMIFS( $L337:$L$520,\n              $B337:$B$520, $B336 & \".*\",\n              $B337:$B$520, \"<>\" & $B336 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.1",null,null,"RALO SECO LINEAR PVC SANITÁRIO D=90 COM GRELHA ALUMINIO","SERV","UNID.",null,null,0,{"$f":"IF( $G337 <> \"\",\nTRUNC( $H337 * $I337, 2 ),\nSUMIFS( $K338:$K$520,\n          $B338:$B$520, $B337 & \".*\",\n          $B338:$B$520, \"<>\" & $B337 & \".*.*\"\n) )","v":0},{"$f":"IF( $G337 <> \"\",\n     TRUNC( $H337 * $J337, 2 ),\n     SUMIFS( $L338:$L$520,\n              $B338:$B$520, $B337 & \".*\",\n              $B338:$B$520, \"<>\" & $B337 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.2",null,null,"CAIXA SIFONADA QUADRADA, COM SETE ENTRADAS E UMA SAÍDA, D = 150 X 150 X 50MM,REF. Nº25, ACABAMENTO BRANCO, MARCA AKROS OU SIMILAR","SERV","UNID.",null,null,0,{"$f":"IF( $G338 <> \"\",\nTRUNC( $H338 * $I338, 2 ),\nSUMIFS( $K339:$K$520,\n          $B339:$B$520, $B338 & \".*\",\n          $B339:$B$520, \"<>\" & $B338 & \".*.*\"\n) )","v":0},{"$f":"IF( $G338 <> \"\",\n     TRUNC( $H338 * $J338, 2 ),\n     SUMIFS( $L339:$L$520,\n              $B339:$B$520, $B338 & \".*\",\n              $B339:$B$520, \"<>\" & $B338 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.3",null,null,"JOELHO 45 GRAUS, PVC, SERIE NORMAL, ESGOTO PREDIAL, DN 150 MM, JUNTA ELÁSTICA, FORNECIDO E INSTALADO EM SUBCOLETOR AÉREO DE ESGOTO SANITÁRIO. AF_08/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G339 <> \"\",\nTRUNC( $H339 * $I339, 2 ),\nSUMIFS( $K340:$K$520,\n          $B340:$B$520, $B339 & \".*\",\n          $B340:$B$520, \"<>\" & $B339 & \".*.*\"\n) )","v":0},{"$f":"IF( $G339 <> \"\",\n     TRUNC( $H339 * $J339, 2 ),\n     SUMIFS( $L340:$L$520,\n              $B340:$B$520, $B339 & \".*\",\n              $B340:$B$520, \"<>\" & $B339 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.4",null,null,"CAIXA ENTERRADA HIDRÁULICA RETANGULAR EM ALVENARIA COM TIJOLOS CERÂMICOS MACIÇOS, DIMENSÕES INTERNAS: 0,6X0,6X0,6 M PARA REDE DE ESGOTO. AF_12/2020","SERV","UNID.",null,null,0,{"$f":"IF( $G340 <> \"\",\nTRUNC( $H340 * $I340, 2 ),\nSUMIFS( $K341:$K$520,\n          $B341:$B$520, $B340 & \".*\",\n          $B341:$B$520, \"<>\" & $B340 & \".*.*\"\n) )","v":0},{"$f":"IF( $G340 <> \"\",\n     TRUNC( $H340 * $J340, 2 ),\n     SUMIFS( $L341:$L$520,\n              $B341:$B$520, $B340 & \".*\",\n              $B341:$B$520, \"<>\" & $B340 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.5",null,null,"CAIXA SIFONADA, COM GRELHA REDONDA, PVC, DN 150 X 150 X 50 MM, JUNTA SOLDÁVEL, FORNECIDA E INSTALADA EM RAMAL DE DESCARGA OU EM RAMAL DE ESGOTO SANITÁRIO. AF_08/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G341 <> \"\",\nTRUNC( $H341 * $I341, 2 ),\nSUMIFS( $K342:$K$520,\n          $B342:$B$520, $B341 & \".*\",\n          $B342:$B$520, \"<>\" & $B341 & \".*.*\"\n) )","v":0},{"$f":"IF( $G341 <> \"\",\n     TRUNC( $H341 * $J341, 2 ),\n     SUMIFS( $L342:$L$520,\n              $B342:$B$520, $B341 & \".*\",\n              $B342:$B$520, \"<>\" & $B341 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.6",null,null,"SIFÃO DO TIPO GARRAFA/COPO EM PVC 1.1/4  X 1.1/2\" - FORNECIMENTO E INSTALAÇÃO. AF_01/2020","SERV","UNID.",null,null,0,{"$f":"IF( $G342 <> \"\",\nTRUNC( $H342 * $I342, 2 ),\nSUMIFS( $K343:$K$520,\n          $B343:$B$520, $B342 & \".*\",\n          $B343:$B$520, \"<>\" & $B342 & \".*.*\"\n) )","v":0},{"$f":"IF( $G342 <> \"\",\n     TRUNC( $H342 * $J342, 2 ),\n     SUMIFS( $L343:$L$520,\n              $B343:$B$520, $B342 & \".*\",\n              $B343:$B$520, \"<>\" & $B342 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.7",null,null,"SIFÃO DO TIPO FLEXÍVEL EM PVC 1  X 1.1/2  - FORNECIMENTO E INSTALAÇÃO. AF_01/2020","SERV","UNID.",null,null,0,{"$f":"IF( $G343 <> \"\",\nTRUNC( $H343 * $I343, 2 ),\nSUMIFS( $K344:$K$520,\n          $B344:$B$520, $B343 & \".*\",\n          $B344:$B$520, \"<>\" & $B343 & \".*.*\"\n) )","v":0},{"$f":"IF( $G343 <> \"\",\n     TRUNC( $H343 * $J343, 2 ),\n     SUMIFS( $L344:$L$520,\n              $B344:$B$520, $B343 & \".*\",\n              $B344:$B$520, \"<>\" & $B343 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.8",null,null,"VÁLVULA EM PLÁSTICO 1\" PARA PIA, TANQUE OU LAVATÓRIO, COM OU SEM LADRÃO - FORNECIMENTO E INSTALAÇÃO. AF_01/2020","SERV","UNID.",null,null,0,{"$f":"IF( $G344 <> \"\",\nTRUNC( $H344 * $I344, 2 ),\nSUMIFS( $K345:$K$520,\n          $B345:$B$520, $B344 & \".*\",\n          $B345:$B$520, \"<>\" & $B344 & \".*.*\"\n) )","v":0},{"$f":"IF( $G344 <> \"\",\n     TRUNC( $H344 * $J344, 2 ),\n     SUMIFS( $L345:$L$520,\n              $B345:$B$520, $B344 & \".*\",\n              $B345:$B$520, \"<>\" & $B344 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.9",null,null,"BUCHA DE REDUÇÃO LONGA, PVC, SÉRIE NORMAL, ESGOTO PREDIAL, DN 50 X 40 MM, JUNTA SOLDÁVEL E ELÁSTICA, FORNECIDO E INSTALADO EM RAMAL DE DESCARGA OU RAMAL DE ESGOTO SANITÁRIO. AF_08/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G345 <> \"\",\nTRUNC( $H345 * $I345, 2 ),\nSUMIFS( $K346:$K$520,\n          $B346:$B$520, $B345 & \".*\",\n          $B346:$B$520, \"<>\" & $B345 & \".*.*\"\n) )","v":0},{"$f":"IF( $G345 <> \"\",\n     TRUNC( $H345 * $J345, 2 ),\n     SUMIFS( $L346:$L$520,\n              $B346:$B$520, $B345 & \".*\",\n              $B346:$B$520, \"<>\" & $B345 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.10",null,null,"CURVA CURTA 90 GRAUS, PVC, SERIE NORMAL, ESGOTO PREDIAL, DN 40 MM, JUNTA SOLDÁVEL, FORNECIDO E INSTALADO EM RAMAL DE DESCARGA OU RAMAL DE ESGOTO SANITÁRIO. AF_08/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G346 <> \"\",\nTRUNC( $H346 * $I346, 2 ),\nSUMIFS( $K347:$K$520,\n          $B347:$B$520, $B346 & \".*\",\n          $B347:$B$520, \"<>\" & $B346 & \".*.*\"\n) )","v":0},{"$f":"IF( $G346 <> \"\",\n     TRUNC( $H346 * $J346, 2 ),\n     SUMIFS( $L347:$L$520,\n              $B347:$B$520, $B346 & \".*\",\n              $B347:$B$520, \"<>\" & $B346 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.11",null,null,"JOELHO 45 GRAUS, PVC, SERIE NORMAL, ESGOTO PREDIAL, DN 100 MM, JUNTA ELÁSTICA, FORNECIDO E INSTALADO EM PRUMADA DE ESGOTO SANITÁRIO OU VENTILAÇÃO. AF_08/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G347 <> \"\",\nTRUNC( $H347 * $I347, 2 ),\nSUMIFS( $K348:$K$520,\n          $B348:$B$520, $B347 & \".*\",\n          $B348:$B$520, \"<>\" & $B347 & \".*.*\"\n) )","v":0},{"$f":"IF( $G347 <> \"\",\n     TRUNC( $H347 * $J347, 2 ),\n     SUMIFS( $L348:$L$520,\n              $B348:$B$520, $B347 & \".*\",\n              $B348:$B$520, \"<>\" & $B347 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.12",null,null,"JOELHO 45 GRAUS, PVC, SERIE R, ÁGUA PLUVIAL, DN 40 MM, JUNTA SOLDÁVEL, FORNECIDO E INSTALADO EM RAMAL DE ENCAMINHAMENTO. AF_06/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G348 <> \"\",\nTRUNC( $H348 * $I348, 2 ),\nSUMIFS( $K349:$K$520,\n          $B349:$B$520, $B348 & \".*\",\n          $B349:$B$520, \"<>\" & $B348 & \".*.*\"\n) )","v":0},{"$f":"IF( $G348 <> \"\",\n     TRUNC( $H348 * $J348, 2 ),\n     SUMIFS( $L349:$L$520,\n              $B349:$B$520, $B348 & \".*\",\n              $B349:$B$520, \"<>\" & $B348 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.13",null,null,"JOELHO 45 GRAUS, PVC, SERIE R, ÁGUA PLUVIAL, DN 50 MM, JUNTA ELÁSTICA, FORNECIDO E INSTALADO EM RAMAL DE ENCAMINHAMENTO. AF_06/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G349 <> \"\",\nTRUNC( $H349 * $I349, 2 ),\nSUMIFS( $K350:$K$520,\n          $B350:$B$520, $B349 & \".*\",\n          $B350:$B$520, \"<>\" & $B349 & \".*.*\"\n) )","v":0},{"$f":"IF( $G349 <> \"\",\n     TRUNC( $H349 * $J349, 2 ),\n     SUMIFS( $L350:$L$520,\n              $B350:$B$520, $B349 & \".*\",\n              $B350:$B$520, \"<>\" & $B349 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.14",null,null,"JOELHO 45 GRAUS, PVC, SERIE NORMAL, ESGOTO PREDIAL, DN 75 MM, JUNTA ELÁSTICA, FORNECIDO E INSTALADO EM RAMAL DE DESCARGA OU RAMAL DE ESGOTO SANITÁRIO. AF_08/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G350 <> \"\",\nTRUNC( $H350 * $I350, 2 ),\nSUMIFS( $K351:$K$520,\n          $B351:$B$520, $B350 & \".*\",\n          $B351:$B$520, \"<>\" & $B350 & \".*.*\"\n) )","v":0},{"$f":"IF( $G350 <> \"\",\n     TRUNC( $H350 * $J350, 2 ),\n     SUMIFS( $L351:$L$520,\n              $B351:$B$520, $B350 & \".*\",\n              $B351:$B$520, \"<>\" & $B350 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.15",null,null,"JOELHO 90 GRAUS, PVC, SERIE NORMAL, ESGOTO PREDIAL, DN 100 MM, JUNTA ELÁSTICA, FORNECIDO E INSTALADO EM RAMAL DE DESCARGA OU RAMAL DE ESGOTO SANITÁRIO. AF_08/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G351 <> \"\",\nTRUNC( $H351 * $I351, 2 ),\nSUMIFS( $K352:$K$520,\n          $B352:$B$520, $B351 & \".*\",\n          $B352:$B$520, \"<>\" & $B351 & \".*.*\"\n) )","v":0},{"$f":"IF( $G351 <> \"\",\n     TRUNC( $H351 * $J351, 2 ),\n     SUMIFS( $L352:$L$520,\n              $B352:$B$520, $B351 & \".*\",\n              $B352:$B$520, \"<>\" & $B351 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.16",null,null,"JOELHO 90 GRAUS, PVC, SERIE NORMAL, ESGOTO PREDIAL, DN 40 MM, JUNTA SOLDÁVEL, FORNECIDO E INSTALADO EM RAMAL DE DESCARGA OU RAMAL DE ESGOTO SANITÁRIO. AF_08/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G352 <> \"\",\nTRUNC( $H352 * $I352, 2 ),\nSUMIFS( $K353:$K$520,\n          $B353:$B$520, $B352 & \".*\",\n          $B353:$B$520, \"<>\" & $B352 & \".*.*\"\n) )","v":0},{"$f":"IF( $G352 <> \"\",\n     TRUNC( $H352 * $J352, 2 ),\n     SUMIFS( $L353:$L$520,\n              $B353:$B$520, $B352 & \".*\",\n              $B353:$B$520, \"<>\" & $B352 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.17",null,null,"JOELHO 90 GRAUS, PVC, SERIE NORMAL, ESGOTO PREDIAL, DN 50 MM, JUNTA ELÁSTICA, FORNECIDO E INSTALADO EM RAMAL DE DESCARGA OU RAMAL DE ESGOTO SANITÁRIO. AF_08/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G353 <> \"\",\nTRUNC( $H353 * $I353, 2 ),\nSUMIFS( $K354:$K$520,\n          $B354:$B$520, $B353 & \".*\",\n          $B354:$B$520, \"<>\" & $B353 & \".*.*\"\n) )","v":0},{"$f":"IF( $G353 <> \"\",\n     TRUNC( $H353 * $J353, 2 ),\n     SUMIFS( $L354:$L$520,\n              $B354:$B$520, $B353 & \".*\",\n              $B354:$B$520, \"<>\" & $B353 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.18",null,null,"JOELHO 90 GRAUS, PVC, SERIE NORMAL, ESGOTO PREDIAL, DN 75 MM, JUNTA ELÁSTICA, FORNECIDO E INSTALADO EM RAMAL DE DESCARGA OU RAMAL DE ESGOTO SANITÁRIO. AF_08/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G354 <> \"\",\nTRUNC( $H354 * $I354, 2 ),\nSUMIFS( $K355:$K$520,\n          $B355:$B$520, $B354 & \".*\",\n          $B355:$B$520, \"<>\" & $B354 & \".*.*\"\n) )","v":0},{"$f":"IF( $G354 <> \"\",\n     TRUNC( $H354 * $J354, 2 ),\n     SUMIFS( $L355:$L$520,\n              $B355:$B$520, $B354 & \".*\",\n              $B355:$B$520, \"<>\" & $B354 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.19",null,null,"JOELHO PVC, COM BOLSA E ANEL, 90 GRAUS, DN 40 X *38* MM, SERIE NORMAL, PARA ESGOTO PREDIAL","FORN","UNID.",null,null,0,{"$f":"IF( $G355 <> \"\",\nTRUNC( $H355 * $I355, 2 ),\nSUMIFS( $K356:$K$520,\n          $B356:$B$520, $B355 & \".*\",\n          $B356:$B$520, \"<>\" & $B355 & \".*.*\"\n) )","v":0},{"$f":"IF( $G355 <> \"\",\n     TRUNC( $H355 * $J355, 2 ),\n     SUMIFS( $L356:$L$520,\n              $B356:$B$520, $B355 & \".*\",\n              $B356:$B$520, \"<>\" & $B355 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.20",null,null,"JUNÇÃO DE REDUÇÃO INVERTIDA, PVC, SÉRIE NORMAL, ESGOTO PREDIAL, DN 100 X 50 MM, JUNTA ELÁSTICA, FORNECIDO E INSTALADO EM PRUMADA DE ESGOTO SANITÁRIO OU VENTILAÇÃO. AF_08/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G356 <> \"\",\nTRUNC( $H356 * $I356, 2 ),\nSUMIFS( $K357:$K$520,\n          $B357:$B$520, $B356 & \".*\",\n          $B357:$B$520, \"<>\" & $B356 & \".*.*\"\n) )","v":0},{"$f":"IF( $G356 <> \"\",\n     TRUNC( $H356 * $J356, 2 ),\n     SUMIFS( $L357:$L$520,\n              $B357:$B$520, $B356 & \".*\",\n              $B357:$B$520, \"<>\" & $B356 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.21",null,null,"JUNÇÃO DE REDUCAO INVERTIDA, PVC, SÉRIE NORMAL, ESGOTO PREDIAL, DN 100 X 75 MM, JUNTA ELÁSTICA, FORNECIDO E INSTALADO EM RAMAL DE DESCARGA OU RAMAL DE ESGOTO SANITÁRIO. AF_08/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G357 <> \"\",\nTRUNC( $H357 * $I357, 2 ),\nSUMIFS( $K358:$K$520,\n          $B358:$B$520, $B357 & \".*\",\n          $B358:$B$520, \"<>\" & $B357 & \".*.*\"\n) )","v":0},{"$f":"IF( $G357 <> \"\",\n     TRUNC( $H357 * $J357, 2 ),\n     SUMIFS( $L358:$L$520,\n              $B358:$B$520, $B357 & \".*\",\n              $B358:$B$520, \"<>\" & $B357 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.22",null,null,"JUNÇÃO DE REDUÇÃO INVERTIDA, PVC, SÉRIE NORMAL, ESGOTO PREDIAL, DN 75 X 50 MM, JUNTA ELÁSTICA, FORNECIDO E INSTALADO EM PRUMADA DE ESGOTO SANITÁRIO OU VENTILAÇÃO. AF_08/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G358 <> \"\",\nTRUNC( $H358 * $I358, 2 ),\nSUMIFS( $K359:$K$520,\n          $B359:$B$520, $B358 & \".*\",\n          $B359:$B$520, \"<>\" & $B358 & \".*.*\"\n) )","v":0},{"$f":"IF( $G358 <> \"\",\n     TRUNC( $H358 * $J358, 2 ),\n     SUMIFS( $L359:$L$520,\n              $B359:$B$520, $B358 & \".*\",\n              $B359:$B$520, \"<>\" & $B358 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.23",null,null,"JUNÇÃO SIMPLES, PVC, SERIE NORMAL, ESGOTO PREDIAL, DN 100 X 100 MM, JUNTA ELÁSTICA, FORNECIDO E INSTALADO EM RAMAL DE DESCARGA OU RAMAL DE ESGOTO SANITÁRIO. AF_08/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G359 <> \"\",\nTRUNC( $H359 * $I359, 2 ),\nSUMIFS( $K360:$K$520,\n          $B360:$B$520, $B359 & \".*\",\n          $B360:$B$520, \"<>\" & $B359 & \".*.*\"\n) )","v":0},{"$f":"IF( $G359 <> \"\",\n     TRUNC( $H359 * $J359, 2 ),\n     SUMIFS( $L360:$L$520,\n              $B360:$B$520, $B359 & \".*\",\n              $B360:$B$520, \"<>\" & $B359 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.24",null,null,"JUNÇÃO SIMPLES, PVC, SERIE NORMAL, ESGOTO PREDIAL, DN 40 MM, JUNTA SOLDÁVEL, FORNECIDO E INSTALADO EM RAMAL DE DESCARGA OU RAMAL DE ESGOTO SANITÁRIO. AF_08/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G360 <> \"\",\nTRUNC( $H360 * $I360, 2 ),\nSUMIFS( $K361:$K$520,\n          $B361:$B$520, $B360 & \".*\",\n          $B361:$B$520, \"<>\" & $B360 & \".*.*\"\n) )","v":0},{"$f":"IF( $G360 <> \"\",\n     TRUNC( $H360 * $J360, 2 ),\n     SUMIFS( $L361:$L$520,\n              $B361:$B$520, $B360 & \".*\",\n              $B361:$B$520, \"<>\" & $B360 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.25",null,null,"JUNÇÃO SIMPLES, PVC, SERIE NORMAL, ESGOTO PREDIAL, DN 50 X 50 MM, JUNTA ELÁSTICA, FORNECIDO E INSTALADO EM PRUMADA DE ESGOTO SANITÁRIO OU VENTILAÇÃO. AF_08/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G361 <> \"\",\nTRUNC( $H361 * $I361, 2 ),\nSUMIFS( $K362:$K$520,\n          $B362:$B$520, $B361 & \".*\",\n          $B362:$B$520, \"<>\" & $B361 & \".*.*\"\n) )","v":0},{"$f":"IF( $G361 <> \"\",\n     TRUNC( $H361 * $J361, 2 ),\n     SUMIFS( $L362:$L$520,\n              $B362:$B$520, $B361 & \".*\",\n              $B362:$B$520, \"<>\" & $B361 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.26",null,null,"LUVA SIMPLES, PVC, SERIE NORMAL, ESGOTO PREDIAL, DN 100 MM, JUNTA ELÁSTICA, FORNECIDO E INSTALADO EM PRUMADA DE ESGOTO SANITÁRIO OU VENTILAÇÃO. AF_08/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G362 <> \"\",\nTRUNC( $H362 * $I362, 2 ),\nSUMIFS( $K363:$K$520,\n          $B363:$B$520, $B362 & \".*\",\n          $B363:$B$520, \"<>\" & $B362 & \".*.*\"\n) )","v":0},{"$f":"IF( $G362 <> \"\",\n     TRUNC( $H362 * $J362, 2 ),\n     SUMIFS( $L363:$L$520,\n              $B363:$B$520, $B362 & \".*\",\n              $B363:$B$520, \"<>\" & $B362 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.27",null,null,"LUVA SIMPLES, PVC, SERIE NORMAL, ESGOTO PREDIAL, DN 50 MM, JUNTA ELÁSTICA, FORNECIDO E INSTALADO EM RAMAL DE DESCARGA OU RAMAL DE ESGOTO SANITÁRIO. AF_08/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G363 <> \"\",\nTRUNC( $H363 * $I363, 2 ),\nSUMIFS( $K364:$K$520,\n          $B364:$B$520, $B363 & \".*\",\n          $B364:$B$520, \"<>\" & $B363 & \".*.*\"\n) )","v":0},{"$f":"IF( $G363 <> \"\",\n     TRUNC( $H363 * $J363, 2 ),\n     SUMIFS( $L364:$L$520,\n              $B364:$B$520, $B363 & \".*\",\n              $B364:$B$520, \"<>\" & $B363 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.28",null,null,"REDUÇÃO EXCÊNTRICA, PVC, SERIE R, ÁGUA PLUVIAL, DN 100 X 75 MM, JUNTA ELÁSTICA, FORNECIDO E INSTALADO EM RAMAL DE ENCAMINHAMENTO. AF_06/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G364 <> \"\",\nTRUNC( $H364 * $I364, 2 ),\nSUMIFS( $K365:$K$520,\n          $B365:$B$520, $B364 & \".*\",\n          $B365:$B$520, \"<>\" & $B364 & \".*.*\"\n) )","v":0},{"$f":"IF( $G364 <> \"\",\n     TRUNC( $H364 * $J364, 2 ),\n     SUMIFS( $L365:$L$520,\n              $B365:$B$520, $B364 & \".*\",\n              $B365:$B$520, \"<>\" & $B364 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.29",null,null,"TUBO PVC, SERIE NORMAL, ESGOTO PREDIAL, DN 100 MM, FORNECIDO E INSTALADO EM RAMAL DE DESCARGA OU RAMAL DE ESGOTO SANITÁRIO. AF_08/2022","SERV","M",null,null,0,{"$f":"IF( $G365 <> \"\",\nTRUNC( $H365 * $I365, 2 ),\nSUMIFS( $K366:$K$520,\n          $B366:$B$520, $B365 & \".*\",\n          $B366:$B$520, \"<>\" & $B365 & \".*.*\"\n) )","v":0},{"$f":"IF( $G365 <> \"\",\n     TRUNC( $H365 * $J365, 2 ),\n     SUMIFS( $L366:$L$520,\n              $B366:$B$520, $B365 & \".*\",\n              $B366:$B$520, \"<>\" & $B365 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.30",null,null,"TUBO PVC, SERIE NORMAL, ESGOTO PREDIAL, DN 150 MM, FORNECIDO E INSTALADO EM SUBCOLETOR AÉREO DE ESGOTO SANITÁRIO. AF_08/2022","SERV","M",null,null,0,{"$f":"IF( $G366 <> \"\",\nTRUNC( $H366 * $I366, 2 ),\nSUMIFS( $K367:$K$520,\n          $B367:$B$520, $B366 & \".*\",\n          $B367:$B$520, \"<>\" & $B366 & \".*.*\"\n) )","v":0},{"$f":"IF( $G366 <> \"\",\n     TRUNC( $H366 * $J366, 2 ),\n     SUMIFS( $L367:$L$520,\n              $B367:$B$520, $B366 & \".*\",\n              $B367:$B$520, \"<>\" & $B366 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.31",null,null,"TUBO PVC, SERIE NORMAL, ESGOTO PREDIAL, DN 50 MM, FORNECIDO E INSTALADO EM RAMAL DE DESCARGA OU RAMAL DE ESGOTO SANITÁRIO. AF_08/2022","SERV","M",null,null,0,{"$f":"IF( $G367 <> \"\",\nTRUNC( $H367 * $I367, 2 ),\nSUMIFS( $K368:$K$520,\n          $B368:$B$520, $B367 & \".*\",\n          $B368:$B$520, \"<>\" & $B367 & \".*.*\"\n) )","v":0},{"$f":"IF( $G367 <> \"\",\n     TRUNC( $H367 * $J367, 2 ),\n     SUMIFS( $L368:$L$520,\n              $B368:$B$520, $B367 & \".*\",\n              $B368:$B$520, \"<>\" & $B367 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.32",null,null,"TUBO PVC, SERIE NORMAL, ESGOTO PREDIAL, DN 75 MM, FORNECIDO E INSTALADO EM RAMAL DE DESCARGA OU RAMAL DE ESGOTO SANITÁRIO. AF_08/2022","SERV","M",null,null,0,{"$f":"IF( $G368 <> \"\",\nTRUNC( $H368 * $I368, 2 ),\nSUMIFS( $K369:$K$520,\n          $B369:$B$520, $B368 & \".*\",\n          $B369:$B$520, \"<>\" & $B368 & \".*.*\"\n) )","v":0},{"$f":"IF( $G368 <> \"\",\n     TRUNC( $H368 * $J368, 2 ),\n     SUMIFS( $L369:$L$520,\n              $B369:$B$520, $B368 & \".*\",\n              $B369:$B$520, \"<>\" & $B368 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.33",null,null,"TUBO PVC RIGIDO SOLDAVEL, SERIE REFORÇADA, P/ESGOTO E AGUAS PLUVIAIS, D= 100MM","SERV","M",null,null,0,{"$f":"IF( $G369 <> \"\",\nTRUNC( $H369 * $I369, 2 ),\nSUMIFS( $K370:$K$520,\n          $B370:$B$520, $B369 & \".*\",\n          $B370:$B$520, \"<>\" & $B369 & \".*.*\"\n) )","v":0},{"$f":"IF( $G369 <> \"\",\n     TRUNC( $H369 * $J369, 2 ),\n     SUMIFS( $L370:$L$520,\n              $B370:$B$520, $B369 & \".*\",\n              $B370:$B$520, \"<>\" & $B369 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.34",null,null,"TUBO PVC RÍGIDO SOLDÁVEL, SERIE REFORÇADA, P/ESGOTO E AGUAS PLUVIAIS, D =  40MM","SERV","M",null,null,0,{"$f":"IF( $G370 <> \"\",\nTRUNC( $H370 * $I370, 2 ),\nSUMIFS( $K371:$K$520,\n          $B371:$B$520, $B370 & \".*\",\n          $B371:$B$520, \"<>\" & $B370 & \".*.*\"\n) )","v":0},{"$f":"IF( $G370 <> \"\",\n     TRUNC( $H370 * $J370, 2 ),\n     SUMIFS( $L371:$L$520,\n              $B371:$B$520, $B370 & \".*\",\n              $B371:$B$520, \"<>\" & $B370 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.35",null,null,"TUBO PVC RÍGIDO SOLDÁVEL, SERIE REFORÇADA, P/ESGOTO E AGUAS PLUVIAIS, D =  50MM","SERV","M",null,null,0,{"$f":"IF( $G371 <> \"\",\nTRUNC( $H371 * $I371, 2 ),\nSUMIFS( $K372:$K$520,\n          $B372:$B$520, $B371 & \".*\",\n          $B372:$B$520, \"<>\" & $B371 & \".*.*\"\n) )","v":0},{"$f":"IF( $G371 <> \"\",\n     TRUNC( $H371 * $J371, 2 ),\n     SUMIFS( $L372:$L$520,\n              $B372:$B$520, $B371 & \".*\",\n              $B372:$B$520, \"<>\" & $B371 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.36",null,null,"TUBO PVC RIGIDO SOLDAVEL, SÉRIE REFORÇADA, P/ESGOTO E AGUAS PLUVIAIS, D=  75MM","SERV","M",null,null,0,{"$f":"IF( $G372 <> \"\",\nTRUNC( $H372 * $I372, 2 ),\nSUMIFS( $K373:$K$520,\n          $B373:$B$520, $B372 & \".*\",\n          $B373:$B$520, \"<>\" & $B372 & \".*.*\"\n) )","v":0},{"$f":"IF( $G372 <> \"\",\n     TRUNC( $H372 * $J372, 2 ),\n     SUMIFS( $L373:$L$520,\n              $B373:$B$520, $B372 & \".*\",\n              $B373:$B$520, \"<>\" & $B372 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.37",null,null,"TE, PVC, SERIE NORMAL, ESGOTO PREDIAL, DN 50 X 50 MM, JUNTA ELÁSTICA, FORNECIDO E INSTALADO EM RAMAL DE DESCARGA OU RAMAL DE ESGOTO SANITÁRIO. AF_08/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G373 <> \"\",\nTRUNC( $H373 * $I373, 2 ),\nSUMIFS( $K374:$K$520,\n          $B374:$B$520, $B373 & \".*\",\n          $B374:$B$520, \"<>\" & $B373 & \".*.*\"\n) )","v":0},{"$f":"IF( $G373 <> \"\",\n     TRUNC( $H373 * $J373, 2 ),\n     SUMIFS( $L374:$L$520,\n              $B374:$B$520, $B373 & \".*\",\n              $B374:$B$520, \"<>\" & $B373 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.38",null,null,"TE, PVC, SERIE NORMAL, ESGOTO PREDIAL, DN 75 X 75 MM, JUNTA ELÁSTICA, FORNECIDO E INSTALADO EM RAMAL DE DESCARGA OU RAMAL DE ESGOTO SANITÁRIO. AF_08/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G374 <> \"\",\nTRUNC( $H374 * $I374, 2 ),\nSUMIFS( $K375:$K$520,\n          $B375:$B$520, $B374 & \".*\",\n          $B375:$B$520, \"<>\" & $B374 & \".*.*\"\n) )","v":0},{"$f":"IF( $G374 <> \"\",\n     TRUNC( $H374 * $J374, 2 ),\n     SUMIFS( $L375:$L$520,\n              $B375:$B$520, $B374 & \".*\",\n              $B375:$B$520, \"<>\" & $B374 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.39",null,null,"FORNECIMENTO DE CURVA 45º DE PVC JUNTA ELÁSTICA, PONTA / BOLSA, DIAM. =   50MM","SERV","UNID.",null,null,0,{"$f":"IF( $G375 <> \"\",\nTRUNC( $H375 * $I375, 2 ),\nSUMIFS( $K376:$K$520,\n          $B376:$B$520, $B375 & \".*\",\n          $B376:$B$520, \"<>\" & $B375 & \".*.*\"\n) )","v":0},{"$f":"IF( $G375 <> \"\",\n     TRUNC( $H375 * $J375, 2 ),\n     SUMIFS( $L376:$L$520,\n              $B376:$B$520, $B375 & \".*\",\n              $B376:$B$520, \"<>\" & $B375 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.40",null,null,"JOELHO 45 GRAUS, PVC, SERIE NORMAL, ESGOTO PREDIAL, DN 50 MM, JUNTA ELÁSTICA, FORNECIDO E INSTALADO EM RAMAL DE DESCARGA OU RAMAL DE ESGOTO SANITÁRIO. AF_08/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G376 <> \"\",\nTRUNC( $H376 * $I376, 2 ),\nSUMIFS( $K377:$K$520,\n          $B377:$B$520, $B376 & \".*\",\n          $B377:$B$520, \"<>\" & $B376 & \".*.*\"\n) )","v":0},{"$f":"IF( $G376 <> \"\",\n     TRUNC( $H376 * $J376, 2 ),\n     SUMIFS( $L377:$L$520,\n              $B377:$B$520, $B376 & \".*\",\n              $B377:$B$520, \"<>\" & $B376 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.41",null,null,"JUNÇÃO SIMPLES, PVC, SERIE NORMAL, ESGOTO PREDIAL, DN 50 X 50 MM, JUNTA ELÁSTICA, FORNECIDO E INSTALADO EM RAMAL DE DESCARGA OU RAMAL DE ESGOTO SANITÁRIO. AF_08/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G377 <> \"\",\nTRUNC( $H377 * $I377, 2 ),\nSUMIFS( $K378:$K$520,\n          $B378:$B$520, $B377 & \".*\",\n          $B378:$B$520, \"<>\" & $B377 & \".*.*\"\n) )","v":0},{"$f":"IF( $G377 <> \"\",\n     TRUNC( $H377 * $J377, 2 ),\n     SUMIFS( $L378:$L$520,\n              $B378:$B$520, $B377 & \".*\",\n              $B378:$B$520, \"<>\" & $B377 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.42",null,null,"TERMINAL DE VENTILAÇÃO, PVC, SÉRIE NORMAL, ESGOTO PREDIAL, DN 100 MM, JUNTA SOLDÁVEL, FORNECIDO E INSTALADO EM PRUMADA DE ESGOTO SANITÁRIO OU VENTILAÇÃO. AF_08/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G378 <> \"\",\nTRUNC( $H378 * $I378, 2 ),\nSUMIFS( $K379:$K$520,\n          $B379:$B$520, $B378 & \".*\",\n          $B379:$B$520, \"<>\" & $B378 & \".*.*\"\n) )","v":0},{"$f":"IF( $G378 <> \"\",\n     TRUNC( $H378 * $J378, 2 ),\n     SUMIFS( $L379:$L$520,\n              $B379:$B$520, $B378 & \".*\",\n              $B379:$B$520, \"<>\" & $B378 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.43",null,null,"TERMINAL DE VENTILAÇÃO, PVC, SÉRIE NORMAL, ESGOTO PREDIAL, DN 50 MM, JUNTA SOLDÁVEL, FORNECIDO E INSTALADO EM PRUMADA DE ESGOTO SANITÁRIO OU VENTILAÇÃO. AF_08/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G379 <> \"\",\nTRUNC( $H379 * $I379, 2 ),\nSUMIFS( $K380:$K$520,\n          $B380:$B$520, $B379 & \".*\",\n          $B380:$B$520, \"<>\" & $B379 & \".*.*\"\n) )","v":0},{"$f":"IF( $G379 <> \"\",\n     TRUNC( $H379 * $J379, 2 ),\n     SUMIFS( $L380:$L$520,\n              $B380:$B$520, $B379 & \".*\",\n              $B380:$B$520, \"<>\" & $B379 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.44",null,null,"TERMINAL DE VENTILAÇÃO, PVC, SÉRIE NORMAL, ESGOTO PREDIAL, DN 75 MM, JUNTA SOLDÁVEL, FORNECIDO E INSTALADO EM PRUMADA DE ESGOTO SANITÁRIO OU VENTILAÇÃO. AF_08/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G380 <> \"\",\nTRUNC( $H380 * $I380, 2 ),\nSUMIFS( $K381:$K$520,\n          $B381:$B$520, $B380 & \".*\",\n          $B381:$B$520, \"<>\" & $B380 & \".*.*\"\n) )","v":0},{"$f":"IF( $G380 <> \"\",\n     TRUNC( $H380 * $J380, 2 ),\n     SUMIFS( $L381:$L$520,\n              $B381:$B$520, $B380 & \".*\",\n              $B381:$B$520, \"<>\" & $B380 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.45",null,null,"FURO MECANIZADO EM CONCRETO, COM MARTELO DEMOLIDOR, PARA INSTALAÇÕES HIDRÁULICAS, DIÂMETROS MAIORES QUE 40 MM E MENORES OU IGUAIS A 75 MM. AF_09/2023","SERV","UNID.",null,null,0,{"$f":"IF( $G381 <> \"\",\nTRUNC( $H381 * $I381, 2 ),\nSUMIFS( $K382:$K$520,\n          $B382:$B$520, $B381 & \".*\",\n          $B382:$B$520, \"<>\" & $B381 & \".*.*\"\n) )","v":0},{"$f":"IF( $G381 <> \"\",\n     TRUNC( $H381 * $J381, 2 ),\n     SUMIFS( $L382:$L$520,\n              $B382:$B$520, $B381 & \".*\",\n              $B382:$B$520, \"<>\" & $B381 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.46",null,null,"TANQUE SÉPTICO RETANGULAR, EM ALVENARIA COM BLOCOS DE CONCRETO, DIMENSÕES INTERNAS: 1,6 X 4,6 X H=2,4 M, VOLUME ÚTIL: 14720 L (PARA 105 CONTRIBUINTES). AF_12/2020","SERV","UNID.",null,null,0,{"$f":"IF( $G382 <> \"\",\nTRUNC( $H382 * $I382, 2 ),\nSUMIFS( $K383:$K$520,\n          $B383:$B$520, $B382 & \".*\",\n          $B383:$B$520, \"<>\" & $B382 & \".*.*\"\n) )","v":0},{"$f":"IF( $G382 <> \"\",\n     TRUNC( $H382 * $J382, 2 ),\n     SUMIFS( $L383:$L$520,\n              $B383:$B$520, $B382 & \".*\",\n              $B383:$B$520, \"<>\" & $B382 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.47",null,null,"FILTRO ANAERÓBIO RETANGULAR, EM ALVENARIA COM BLOCOS DE CONCRETO, DIMENSÕES INTERNAS: 1,6 X 5,6 X H=1,67 M, VOLUME ÚTIL: 10752 L (PARA 103 CONTRIBUINTES). AF_12/2020","SERV","UNID.",null,null,0,{"$f":"IF( $G383 <> \"\",\nTRUNC( $H383 * $I383, 2 ),\nSUMIFS( $K384:$K$520,\n          $B384:$B$520, $B383 & \".*\",\n          $B384:$B$520, \"<>\" & $B383 & \".*.*\"\n) )","v":0},{"$f":"IF( $G383 <> \"\",\n     TRUNC( $H383 * $J383, 2 ),\n     SUMIFS( $L384:$L$520,\n              $B384:$B$520, $B383 & \".*\",\n              $B384:$B$520, \"<>\" & $B383 & \".*.*\"\n     ) )","v":0}]
[null,"7.2.48",null,null,"SUMIDOURO RETANGULAR, EM ALVENARIA COM BLOCOS DE CONCRETO, DIMENSÕES INTERNAS: 1,6 X 5,8 X H=3,0 M, ÁREA DE INFILTRAÇÃO: 50 M² (PARA 20 CONTRIBUINTES). . AF_12/2020","SERV","UNID.",null,null,0,{"$f":"IF( $G384 <> \"\",\nTRUNC( $H384 * $I384, 2 ),\nSUMIFS( $K385:$K$520,\n          $B385:$B$520, $B384 & \".*\",\n          $B385:$B$520, \"<>\" & $B384 & \".*.*\"\n) )","v":0},{"$f":"IF( $G384 <> \"\",\n     TRUNC( $H384 * $J384, 2 ),\n     SUMIFS( $L385:$L$520,\n              $B385:$B$520, $B384 & \".*\",\n              $B385:$B$520, \"<>\" & $B384 & \".*.*\"\n     ) )","v":0}]
[null,"7.3",null,null,"COLETA DE ÁGUAS PLUVIAIS",{"$nulls":4},"",{"$f":"IF( $G385 <> \"\",\nTRUNC( $H385 * $I385, 2 ),\nSUMIFS( $K386:$K$520,\n          $B386:$B$520, $B385 & \".*\",\n          $B386:$B$520, \"<>\" & $B385 & \".*.*\"\n) )","v":0},{"$f":"IF( $G385 <> \"\",\n     TRUNC( $H385 * $J385, 2 ),\n     SUMIFS( $L386:$L$520,\n              $B386:$B$520, $B385 & \".*\",\n              $B386:$B$520, \"<>\" & $B385 & \".*.*\"\n     ) )","v":0}]
[null,"7.3.1",null,null,"BASE PARA POÇO DE VISITA CIRCULAR PARA DRENAGEM, EM CONCRETO PRÉ-MOLDADO, DIÂMETRO INTERNO = 0,80 M, PROFUNDIDADE = 1,35 M, EXCLUINDO TAMPÃO. AF_12/2020_PA","SERV","UNID.",null,null,0,{"$f":"IF( $G386 <> \"\",\nTRUNC( $H386 * $I386, 2 ),\nSUMIFS( $K387:$K$520,\n          $B387:$B$520, $B386 & \".*\",\n          $B387:$B$520, \"<>\" & $B386 & \".*.*\"\n) )","v":0},{"$f":"IF( $G386 <> \"\",\n     TRUNC( $H386 * $J386, 2 ),\n     SUMIFS( $L387:$L$520,\n              $B387:$B$520, $B386 & \".*\",\n              $B387:$B$520, \"<>\" & $B386 & \".*.*\"\n     ) )","v":0}]
[null,"7.3.2",null,null,"TAMPAO FOFO SIMPLES COM BASE / REQUADRO, CLASSE B125 CARGA MAX. 12,5 T, REDONDO, TAMPA 600 MM (COM INSCRICAO EM RELEVO DO TIPO DE REDE)","FORN","UNID.",null,null,0,{"$f":"IF( $G387 <> \"\",\nTRUNC( $H387 * $I387, 2 ),\nSUMIFS( $K388:$K$520,\n          $B388:$B$520, $B387 & \".*\",\n          $B388:$B$520, \"<>\" & $B387 & \".*.*\"\n) )","v":0},{"$f":"IF( $G387 <> \"\",\n     TRUNC( $H387 * $J387, 2 ),\n     SUMIFS( $L388:$L$520,\n              $B388:$B$520, $B387 & \".*\",\n              $B388:$B$520, \"<>\" & $B387 & \".*.*\"\n     ) )","v":0}]
[null,"7.3.3",null,null,"JOELHO 45 GRAUS, PVC, SERIE NORMAL, ESGOTO PREDIAL, DN 100 MM, JUNTA ELÁSTICA, FORNECIDO E INSTALADO EM RAMAL DE DESCARGA OU RAMAL DE ESGOTO SANITÁRIO. AF_08/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G388 <> \"\",\nTRUNC( $H388 * $I388, 2 ),\nSUMIFS( $K389:$K$520,\n          $B389:$B$520, $B388 & \".*\",\n          $B389:$B$520, \"<>\" & $B388 & \".*.*\"\n) )","v":0},{"$f":"IF( $G388 <> \"\",\n     TRUNC( $H388 * $J388, 2 ),\n     SUMIFS( $L389:$L$520,\n              $B389:$B$520, $B388 & \".*\",\n              $B389:$B$520, \"<>\" & $B388 & \".*.*\"\n     ) )","v":0}]
[null,"7.3.4",null,null,"JOELHO 90 GRAUS, PVC, SERIE NORMAL, ESGOTO PREDIAL, DN 100 MM, JUNTA ELÁSTICA, FORNECIDO E INSTALADO EM RAMAL DE DESCARGA OU RAMAL DE ESGOTO SANITÁRIO. AF_08/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G389 <> \"\",\nTRUNC( $H389 * $I389, 2 ),\nSUMIFS( $K390:$K$520,\n          $B390:$B$520, $B389 & \".*\",\n          $B390:$B$520, \"<>\" & $B389 & \".*.*\"\n) )","v":0},{"$f":"IF( $G389 <> \"\",\n     TRUNC( $H389 * $J389, 2 ),\n     SUMIFS( $L390:$L$520,\n              $B390:$B$520, $B389 & \".*\",\n              $B390:$B$520, \"<>\" & $B389 & \".*.*\"\n     ) )","v":0}]
[null,"7.3.5",null,null,"JOELHO 90 GRAUS, PVC, SERIE NORMAL, ESGOTO PREDIAL, DN 150 MM, JUNTA ELÁSTICA, FORNECIDO E INSTALADO EM SUBCOLETOR AÉREO DE ESGOTO SANITÁRIO. AF_08/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G390 <> \"\",\nTRUNC( $H390 * $I390, 2 ),\nSUMIFS( $K391:$K$520,\n          $B391:$B$520, $B390 & \".*\",\n          $B391:$B$520, \"<>\" & $B390 & \".*.*\"\n) )","v":0},{"$f":"IF( $G390 <> \"\",\n     TRUNC( $H390 * $J390, 2 ),\n     SUMIFS( $L391:$L$520,\n              $B391:$B$520, $B390 & \".*\",\n              $B391:$B$520, \"<>\" & $B390 & \".*.*\"\n     ) )","v":0}]
[null,"7.3.6",null,null,"JOELHO 90 GRAUS, PVC, SERIE NORMAL, ESGOTO PREDIAL, DN 75 MM, JUNTA ELÁSTICA, FORNECIDO E INSTALADO EM RAMAL DE DESCARGA OU RAMAL DE ESGOTO SANITÁRIO. AF_08/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G391 <> \"\",\nTRUNC( $H391 * $I391, 2 ),\nSUMIFS( $K392:$K$520,\n          $B392:$B$520, $B391 & \".*\",\n          $B392:$B$520, \"<>\" & $B391 & \".*.*\"\n) )","v":0},{"$f":"IF( $G391 <> \"\",\n     TRUNC( $H391 * $J391, 2 ),\n     SUMIFS( $L392:$L$520,\n              $B392:$B$520, $B391 & \".*\",\n              $B392:$B$520, \"<>\" & $B391 & \".*.*\"\n     ) )","v":0}]
[null,"7.3.7",null,null,"PLUG, PVC OCRE, JUNTA ELÁSTICA, DN 100 MM, PARA COLETOR PREDIAL DE ESGOTO. AF_06/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G392 <> \"\",\nTRUNC( $H392 * $I392, 2 ),\nSUMIFS( $K393:$K$520,\n          $B393:$B$520, $B392 & \".*\",\n          $B393:$B$520, \"<>\" & $B392 & \".*.*\"\n) )","v":0},{"$f":"IF( $G392 <> \"\",\n     TRUNC( $H392 * $J392, 2 ),\n     SUMIFS( $L393:$L$520,\n              $B393:$B$520, $B392 & \".*\",\n              $B393:$B$520, \"<>\" & $B392 & \".*.*\"\n     ) )","v":0}]
[null,"7.3.8",null,null,"TUBO PVC RIGIDO SOLDAVEL, SERIE REFORÇADA, P/ESGOTO E AGUAS PLUVIAIS, D= 100MM","SERV","M",null,null,{"$f":"IF(F393<>\"\",\nTRUNC(IF(F393=\"SERV\",I393*(1+$L$5/100),I393*(1+$L$6/100)),2),\n\"\" )","v":0},{"$f":"IF( $G393 <> \"\",\nTRUNC( $H393 * $I393, 2 ),\nSUMIFS( $K394:$K$520,\n          $B394:$B$520, $B393 & \".*\",\n          $B394:$B$520, \"<>\" & $B393 & \".*.*\"\n) )","v":0},{"$f":"IF( $G393 <> \"\",\n     TRUNC( $H393 * $J393, 2 ),\n     SUMIFS( $L394:$L$520,\n              $B394:$B$520, $B393 & \".*\",\n              $B394:$B$520, \"<>\" & $B393 & \".*.*\"\n     ) )","v":0}]
[null,"7.3.9",null,null,"TE, PVC, SÉRIE NORMAL, ESGOTO PREDIAL, DN 100 X 75 MM, JUNTA ELÁSTICA, FORNECIDO E INSTALADO EM RAMAL DE DESCARGA OU RAMAL DE ESGOTO SANITÁRIO. AF_08/2022","SERV","UNID.",null,null,0,{"$f":"IF( $G394 <> \"\",\nTRUNC( $H394 * $I394, 2 ),\nSUMIFS( $K395:$K$520,\n          $B395:$B$520, $B394 & \".*\",\n          $B395:$B$520, \"<>\" & $B394 & \".*.*\"\n) )","v":0},{"$f":"IF( $G394 <> \"\",\n     TRUNC( $H394 * $J394, 2 ),\n     SUMIFS( $L395:$L$520,\n              $B395:$B$520, $B394 & \".*\",\n              $B395:$B$520, \"<>\" & $B394 & \".*.*\"\n     ) )","v":0}]
[null,"7.4",null,null,"BANCADAS E LAVATÓRIOS",{"$nulls":4},"",{"$f":"IF( $G395 <> \"\",\nTRUNC( $H395 * $I395, 2 ),\nSUMIFS( $K396:$K$520,\n          $B396:$B$520, $B395 & \".*\",\n          $B396:$B$520, \"<>\" & $B395 & \".*.*\"\n) )","v":0},{"$f":"IF( $G395 <> \"\",\n     TRUNC( $H395 * $J395, 2 ),\n     SUMIFS( $L396:$L$520,\n              $B396:$B$520, $B395 & \".*\",\n              $B396:$B$520, \"<>\" & $B395 & \".*.*\"\n     ) )","v":0}]
[null,"7.4.1",null,null,"BANCADA GRANITO CINZA  150 X 60 CM, COM CUBA DE EMBUTIR DE AÇO, VÁLVULA AMERICANA EM METAL, SIFÃO FLEXÍVEL EM PVC, ENGATE FLEXÍVEL 30 CM, TORNEIRA CROMADA LONGA, DE PAREDE, 1/2\" OU 3/4\", P/ COZINHA, PADRÃO POPULAR - FORNEC. E INSTALAÇÃO. AF_01/2020","SERV","UNID.",null,null,0,{"$f":"IF( $G396 <> \"\",\nTRUNC( $H396 * $I396, 2 ),\nSUMIFS( $K397:$K$520,\n          $B397:$B$520, $B396 & \".*\",\n          $B397:$B$520, \"<>\" & $B396 & \".*.*\"\n) )","v":0},{"$f":"IF( $G396 <> \"\",\n     TRUNC( $H396 * $J396, 2 ),\n     SUMIFS( $L397:$L$520,\n              $B397:$B$520, $B396 & \".*\",\n              $B397:$B$520, \"<>\" & $B396 & \".*.*\"\n     ) )","v":0}]
[null,"7.4.2",null,null,"BANCADA GRANITO CINZA,  50 X 60 CM, INCL. CUBA DE EMBUTIR OVAL LOUÇA BRANCA 35 X 50 CM, VÁLVULA METAL CROMADO, SIFÃO FLEXÍVEL PVC, ENGATE 30 CM FLEXÍVEL PLÁSTICO E TORNEIRA CROMADA DE MESA, PADRÃO POPULAR - FORNEC. E INSTALAÇÃO. AF_01/2020","SERV","UNID.",null,null,0,{"$f":"IF( $G397 <> \"\",\nTRUNC( $H397 * $I397, 2 ),\nSUMIFS( $K398:$K$520,\n          $B398:$B$520, $B397 & \".*\",\n          $B398:$B$520, \"<>\" & $B397 & \".*.*\"\n) )","v":0},{"$f":"IF( $G397 <> \"\",\n     TRUNC( $H397 * $J397, 2 ),\n     SUMIFS( $L398:$L$520,\n              $B398:$B$520, $B397 & \".*\",\n              $B398:$B$520, \"<>\" & $B397 & \".*.*\"\n     ) )","v":0}]
[null,"7.4.3",null,null,"ESPELHO CRISTAL E = 4 MM","FORN","M²",null,null,0,{"$f":"IF( $G398 <> \"\",\nTRUNC( $H398 * $I398, 2 ),\nSUMIFS( $K399:$K$520,\n          $B399:$B$520, $B398 & \".*\",\n          $B399:$B$520, \"<>\" & $B398 & \".*.*\"\n) )","v":0},{"$f":"IF( $G398 <> \"\",\n     TRUNC( $H398 * $J398, 2 ),\n     SUMIFS( $L399:$L$520,\n              $B399:$B$520, $B398 & \".*\",\n              $B399:$B$520, \"<>\" & $B398 & \".*.*\"\n     ) )","v":0}]
[null,"7.5",null,null,"RESERVATÓRIO ENTERRADO",{"$nulls":4},"",{"$f":"IF( $G399 <> \"\",\nTRUNC( $H399 * $I399, 2 ),\nSUMIFS( $K400:$K$520,\n          $B400:$B$520, $B399 & \".*\",\n          $B400:$B$520, \"<>\" & $B399 & \".*.*\"\n) )","v":0},{"$f":"IF( $G399 <> \"\",\n     TRUNC( $H399 * $J399, 2 ),\n     SUMIFS( $L400:$L$520,\n              $B400:$B$520, $B399 & \".*\",\n              $B400:$B$520, \"<>\" & $B399 & \".*.*\"\n     ) )","v":0}]
[null,"7.5.1",null,null,"ESCAVAÇÃO VERTICAL PARA  EDIFICAÇÃO, COM CARGA, DESCARGA E TRANSPORTE DE SOLO DE 1ª CATEGORIA, COM ESCAVADEIRA HIDRÁULICA (CAÇAMBA: 1,2 M³ / 155 HP), FROTA DE 5 CAMINHÕES BASCULANTES DE 18 M³, DMT DE 2 KM E VELOCIDADE MÉDIA 19 KM/H. AF_05/2020","SERV","M³",null,null,0,{"$f":"IF( $G400 <> \"\",\nTRUNC( $H400 * $I400, 2 ),\nSUMIFS( $K401:$K$520,\n          $B401:$B$520, $B400 & \".*\",\n          $B401:$B$520, \"<>\" & $B400 & \".*.*\"\n) )","v":0},{"$f":"IF( $G400 <> \"\",\n     TRUNC( $H400 * $J400, 2 ),\n     SUMIFS( $L401:$L$520,\n              $B401:$B$520, $B400 & \".*\",\n              $B401:$B$520, \"<>\" & $B400 & \".*.*\"\n     ) )","v":0}]
[null,"7.5.2",null,null,"MONTAGEM E DESMONTAGEM DE FÔRMA DE LAJE MACIÇA, PÉ-DIREITO SIMPLES, EM CHAPA DE MADEIRA COMPENSADA RESINADA, 2 UTILIZAÇÕES. AF_09/2020","SERV","M²",null,null,0,{"$f":"IF( $G401 <> \"\",\nTRUNC( $H401 * $I401, 2 ),\nSUMIFS( $K402:$K$520,\n          $B402:$B$520, $B401 & \".*\",\n          $B402:$B$520, \"<>\" & $B401 & \".*.*\"\n) )","v":0},{"$f":"IF( $G401 <> \"\",\n     TRUNC( $H401 * $J401, 2 ),\n     SUMIFS( $L402:$L$520,\n              $B402:$B$520, $B401 & \".*\",\n              $B402:$B$520, \"<>\" & $B401 & \".*.*\"\n     ) )","v":0}]
[null,"7.5.3",null,null,"ARMAÇÃO DE PILAR OU VIGA DE ESTRUTURA CONVENCIONAL DE CONCRETO ARMADO UTILIZANDO AÇO CA-50 DE 6,3 MM - MONTAGEM. AF_06/2022","SERV","KG",null,null,0,{"$f":"IF( $G402 <> \"\",\nTRUNC( $H402 * $I402, 2 ),\nSUMIFS( $K403:$K$520,\n          $B403:$B$520, $B402 & \".*\",\n          $B403:$B$520, \"<>\" & $B402 & \".*.*\"\n) )","v":0},{"$f":"IF( $G402 <> \"\",\n     TRUNC( $H402 * $J402, 2 ),\n     SUMIFS( $L403:$L$520,\n              $B403:$B$520, $B402 & \".*\",\n              $B403:$B$520, \"<>\" & $B402 & \".*.*\"\n     ) )","v":0}]
[null,"7.5.4",null,null,"ARMAÇÃO DE PILAR OU VIGA DE ESTRUTURA CONVENCIONAL DE CONCRETO ARMADO UTILIZANDO AÇO CA-50 DE 8,0 MM - MONTAGEM. AF_06/2022","SERV","KG",null,null,0,{"$f":"IF( $G403 <> \"\",\nTRUNC( $H403 * $I403, 2 ),\nSUMIFS( $K404:$K$520,\n          $B404:$B$520, $B403 & \".*\",\n          $B404:$B$520, \"<>\" & $B403 & \".*.*\"\n) )","v":0},{"$f":"IF( $G403 <> \"\",\n     TRUNC( $H403 * $J403, 2 ),\n     SUMIFS( $L404:$L$520,\n              $B404:$B$520, $B403 & \".*\",\n              $B404:$B$520, \"<>\" & $B403 & \".*.*\"\n     ) )","v":0}]
[null,"7.5.5",null,null,"ARMAÇÃO DE PILAR OU VIGA DE ESTRUTURA CONVENCIONAL DE CONCRETO ARMADO UTILIZANDO AÇO CA-50 DE 10,0 MM - MONTAGEM. AF_06/2022","SERV","KG",null,null,0,{"$f":"IF( $G404 <> \"\",\nTRUNC( $H404 * $I404, 2 ),\nSUMIFS( $K405:$K$520,\n          $B405:$B$520, $B404 & \".*\",\n          $B405:$B$520, \"<>\" & $B404 & \".*.*\"\n) )","v":0},{"$f":"IF( $G404 <> \"\",\n     TRUNC( $H404 * $J404, 2 ),\n     SUMIFS( $L405:$L$520,\n              $B405:$B$520, $B404 & \".*\",\n              $B405:$B$520, \"<>\" & $B404 & \".*.*\"\n     ) )","v":0}]
[null,"7.5.6",null,null,"ARMAÇÃO DE PILAR OU VIGA DE ESTRUTURA CONVENCIONAL DE CONCRETO ARMADO UTILIZANDO AÇO CA-50 DE 12,5 MM - MONTAGEM. AF_06/2022","SERV","KG",null,null,0,{"$f":"IF( $G405 <> \"\",\nTRUNC( $H405 * $I405, 2 ),\nSUMIFS( $K406:$K$520,\n          $B406:$B$520, $B405 & \".*\",\n          $B406:$B$520, \"<>\" & $B405 & \".*.*\"\n) )","v":0},{"$f":"IF( $G405 <> \"\",\n     TRUNC( $H405 * $J405, 2 ),\n     SUMIFS( $L406:$L$520,\n              $B406:$B$520, $B405 & \".*\",\n              $B406:$B$520, \"<>\" & $B405 & \".*.*\"\n     ) )","v":0}]
[null,"7.5.7",null,null,"ARMAÇÃO DE PILAR OU VIGA DE ESTRUTURA CONVENCIONAL DE CONCRETO ARMADO UTILIZANDO AÇO CA-60 DE 5,0 MM - MONTAGEM. AF_06/2022","SERV","KG",null,null,0,{"$f":"IF( $G406 <> \"\",\nTRUNC( $H406 * $I406, 2 ),\nSUMIFS( $K407:$K$520,\n          $B407:$B$520, $B406 & \".*\",\n          $B407:$B$520, \"<>\" & $B406 & \".*.*\"\n) )","v":0},{"$f":"IF( $G406 <> \"\",\n     TRUNC( $H406 * $J406, 2 ),\n     SUMIFS( $L407:$L$520,\n              $B407:$B$520, $B406 & \".*\",\n              $B407:$B$520, \"<>\" & $B406 & \".*.*\"\n     ) )","v":0}]
[null,"7.5.8",null,null,"CONCRETAGEM DE PILARES, FCK = 30 MPA, COM USO DE BOMBA - LANÇAMENTO, ADENSAMENTO E ACABAMENTO (ADAPTADO). AF_02/2022_PS","SERV","M³",null,null,0,{"$f":"IF( $G407 <> \"\",\nTRUNC( $H407 * $I407, 2 ),\nSUMIFS( $K408:$K$520,\n          $B408:$B$520, $B407 & \".*\",\n          $B408:$B$520, \"<>\" & $B407 & \".*.*\"\n) )","v":0},{"$f":"IF( $G407 <> \"\",\n     TRUNC( $H407 * $J407, 2 ),\n     SUMIFS( $L408:$L$520,\n              $B408:$B$520, $B407 & \".*\",\n              $B408:$B$520, \"<>\" & $B407 & \".*.*\"\n     ) )","v":0}]
[null,"7.5.9",null,null,"REATERRO MANUAL DE VALAS, COM COMPACTADOR DE SOLOS DE PERCUSSÃO. AF_08/2023","SERV","M³",null,null,0,{"$f":"IF( $G408 <> \"\",\nTRUNC( $H408 * $I408, 2 ),\nSUMIFS( $K409:$K$520,\n          $B409:$B$520, $B408 & \".*\",\n          $B409:$B$520, \"<>\" & $B408 & \".*.*\"\n) )","v":0},{"$f":"IF( $G408 <> \"\",\n     TRUNC( $H408 * $J408, 2 ),\n     SUMIFS( $L409:$L$520,\n              $B409:$B$520, $B408 & \".*\",\n              $B409:$B$520, \"<>\" & $B408 & \".*.*\"\n     ) )","v":0}]
[null,"7.5.10",null,null,"CARGA, MANOBRA E DESCARGA DE SOLOS E MATERIAIS GRANULARES EM CAMINHÃO BASCULANTE 6 M³ - CARGA COM PÁ CARREGADEIRA (CAÇAMBA DE 1,7 A 2,8 M³ / 128 HP) E DESCARGA LIVRE (UNIDADE: M3). AF_07/2020","SERV","M³",null,null,0,{"$f":"IF( $G409 <> \"\",\nTRUNC( $H409 * $I409, 2 ),\nSUMIFS( $K410:$K$520,\n          $B410:$B$520, $B409 & \".*\",\n          $B410:$B$520, \"<>\" & $B409 & \".*.*\"\n) )","v":0},{"$f":"IF( $G409 <> \"\",\n     TRUNC( $H409 * $J409, 2 ),\n     SUMIFS( $L410:$L$520,\n              $B410:$B$520, $B409 & \".*\",\n              $B410:$B$520, \"<>\" & $B409 & \".*.*\"\n     ) )","v":0}]
[null,"7.5.11",null,null,"TRANSPORTE COM CAMINHÃO BASCULANTE DE 6 M³, EM VIA URBANA EM LEITO NATURAL (UNIDADE: M3XKM). AF_07/2020","SERV","M³XKM",null,null,0,{"$f":"IF( $G410 <> \"\",\nTRUNC( $H410 * $I410, 2 ),\nSUMIFS( $K411:$K$520,\n          $B411:$B$520, $B410 & \".*\",\n          $B411:$B$520, \"<>\" & $B410 & \".*.*\"\n) )","v":0},{"$f":"IF( $G410 <> \"\",\n     TRUNC( $H410 * $J410, 2 ),\n     SUMIFS( $L411:$L$520,\n              $B411:$B$520, $B410 & \".*\",\n              $B411:$B$520, \"<>\" & $B410 & \".*.*\"\n     ) )","v":0}]
[null,"7.5.12",null,null,"IMPERMEABILIZAÇÃO DE SUPERFÍCIE COM ARGAMASSA POLIMÉRICA / MEMBRANA ACRÍLICA, 4 DEMÃOS, REFORÇADA COM VÉU DE POLIÉSTER (MAV). AF_09/2023","SERV","M²",null,null,0,{"$f":"IF( $G411 <> \"\",\nTRUNC( $H411 * $I411, 2 ),\nSUMIFS( $K412:$K$520,\n          $B412:$B$520, $B411 & \".*\",\n          $B412:$B$520, \"<>\" & $B411 & \".*.*\"\n) )","v":0},{"$f":"IF( $G411 <> \"\",\n     TRUNC( $H411 * $J411, 2 ),\n     SUMIFS( $L412:$L$520,\n              $B412:$B$520, $B411 & \".*\",\n              $B412:$B$520, \"<>\" & $B411 & \".*.*\"\n     ) )","v":0}]
[null,8,null,null,"VENTILAÇÃO MECÂNICA E EXAUSTORES",{"$nulls":4},"",{"$f":"IF( $G412 <> \"\",\nTRUNC( $H412 * $I412, 2 ),\nSUMIFS( $K413:$K$520,\n          $B413:$B$520, $B412 & \".*\",\n          $B413:$B$520, \"<>\" & $B412 & \".*.*\"\n) )","v":0},{"$f":"IF( $G412 <> \"\",\n     TRUNC( $H412 * $J412, 2 ),\n     SUMIFS( $L413:$L$520,\n              $B413:$B$520, $B412 & \".*\",\n              $B413:$B$520, \"<>\" & $B412 & \".*.*\"\n     ) )","v":0}]
[null,"8.1",null,null,"EXAUSTOR PARA BANHEIRO, BIVOLT, REF.: C 80 A, DA VENTOKIT OU SIMILAR - FORNECIMENTO E INSTALAÇÃO","SERV","UNID.",null,null,0,{"$f":"IF( $G413 <> \"\",\nTRUNC( $H413 * $I413, 2 ),\nSUMIFS( $K414:$K$520,\n          $B414:$B$520, $B413 & \".*\",\n          $B414:$B$520, \"<>\" & $B413 & \".*.*\"\n) )","v":0},{"$f":"IF( $G413 <> \"\",\n     TRUNC( $H413 * $J413, 2 ),\n     SUMIFS( $L414:$L$520,\n              $B414:$B$520, $B413 & \".*\",\n              $B414:$B$520, \"<>\" & $B413 & \".*.*\"\n     ) )","v":0}]
[null,"8.2",null,null,"DUTO CORRUGADO FLEXÍVEL EM PEAD Ø = 4\", TIPO KANALEX OU SIMILAR, LANÇADO DIRETAMENTE NO SOLO, EXCLUSIVE ESCAVAÇÃO E REATERRO","SERV","M",null,null,0,{"$f":"IF( $G414 <> \"\",\nTRUNC( $H414 * $I414, 2 ),\nSUMIFS( $K415:$K$520,\n          $B415:$B$520, $B414 & \".*\",\n          $B415:$B$520, \"<>\" & $B414 & \".*.*\"\n) )","v":0},{"$f":"IF( $G414 <> \"\",\n     TRUNC( $H414 * $J414, 2 ),\n     SUMIFS( $L415:$L$520,\n              $B415:$B$520, $B414 & \".*\",\n              $B415:$B$520, \"<>\" & $B414 & \".*.*\"\n     ) )","v":0}]
[null,"8.3",null,null,"DUTO EM CHAPA GALVANIZADA Nº18 COM DIAM=300MM, PARA SISTEMA EXAUSTÃO (OBRA: MERCADO DE LAGARTO)","SERV","M",null,null,0,{"$f":"IF( $G415 <> \"\",\nTRUNC( $H415 * $I415, 2 ),\nSUMIFS( $K416:$K$520,\n          $B416:$B$520, $B415 & \".*\",\n          $B416:$B$520, \"<>\" & $B415 & \".*.*\"\n) )","v":0},{"$f":"IF( $G415 <> \"\",\n     TRUNC( $H415 * $J415, 2 ),\n     SUMIFS( $L416:$L$520,\n              $B416:$B$520, $B415 & \".*\",\n              $B416:$B$520, \"<>\" & $B415 & \".*.*\"\n     ) )","v":0}]
[null,"8.4",null,null,"CURVA 45º EM CHAPA GALVANIZADA Nº18, DIAM=300MM, P/SISTEMA EXAUSTÃO (OBRA: MERCADO DE LAGARTO)","SERV","UNID.",null,null,0,{"$f":"IF( $G416 <> \"\",\nTRUNC( $H416 * $I416, 2 ),\nSUMIFS( $K417:$K$520,\n          $B417:$B$520, $B416 & \".*\",\n          $B417:$B$520, \"<>\" & $B416 & \".*.*\"\n) )","v":0},{"$f":"IF( $G416 <> \"\",\n     TRUNC( $H416 * $J416, 2 ),\n     SUMIFS( $L417:$L$520,\n              $B417:$B$520, $B416 & \".*\",\n              $B417:$B$520, \"<>\" & $B416 & \".*.*\"\n     ) )","v":0}]
[null,"8.5",null,null,"FURO MECANIZADO EM CONCRETO, COM MARTELO DEMOLIDOR, PARA INSTALAÇÕES HIDRÁULICAS, DIÂMETROS MAIORES QUE 75 MM E MENORES OU IGUAIS A 150 MM. AF_09/2023","SERV","UNID.",null,null,0,{"$f":"IF( $G417 <> \"\",\nTRUNC( $H417 * $I417, 2 ),\nSUMIFS( $K418:$K$520,\n          $B418:$B$520, $B417 & \".*\",\n          $B418:$B$520, \"<>\" & $B417 & \".*.*\"\n) )","v":0},{"$f":"IF( $G417 <> \"\",\n     TRUNC( $H417 * $J417, 2 ),\n     SUMIFS( $L418:$L$520,\n              $B418:$B$520, $B417 & \".*\",\n              $B418:$B$520, \"<>\" & $B417 & \".*.*\"\n     ) )","v":0}]
[null,"8.6",null,null,"CHAMINÉ COM 2 METROS DE DUTOS E CHAPÉU TIPO CANHÃO COR PRETA","FORN","UNID.",null,null,0,{"$f":"IF( $G418 <> \"\",\nTRUNC( $H418 * $I418, 2 ),\nSUMIFS( $K419:$K$520,\n          $B419:$B$520, $B418 & \".*\",\n          $B419:$B$520, \"<>\" & $B418 & \".*.*\"\n) )","v":0},{"$f":"IF( $G418 <> \"\",\n     TRUNC( $H418 * $J418, 2 ),\n     SUMIFS( $L419:$L$520,\n              $B419:$B$520, $B418 & \".*\",\n              $B419:$B$520, \"<>\" & $B418 & \".*.*\"\n     ) )","v":0}]
[null,9,null,null,"PISO E PAVIMENTAÇÃO",{"$nulls":4},"",{"$f":"IF( $G419 <> \"\",\nTRUNC( $H419 * $I419, 2 ),\nSUMIFS( $K420:$K$520,\n          $B420:$B$520, $B419 & \".*\",\n          $B420:$B$520, \"<>\" & $B419 & \".*.*\"\n) )","v":0},{"$f":"IF( $G419 <> \"\",\n     TRUNC( $H419 * $J419, 2 ),\n     SUMIFS( $L420:$L$520,\n              $B420:$B$520, $B419 & \".*\",\n              $B420:$B$520, \"<>\" & $B419 & \".*.*\"\n     ) )","v":0}]
[null,"9.1",null,null,"CONTRAPISO EM ARGAMASSA PRONTA, PREPARO MECÂNICO COM MISTURADOR 300 KG, APLICADO EM ÁREAS SECAS SOBRE LAJE, ADERIDO, ACABAMENTO NÃO REFORÇADO, ESPESSURA 2CM. AF_07/2021","SERV","M²",null,null,0,{"$f":"IF( $G420 <> \"\",\nTRUNC( $H420 * $I420, 2 ),\nSUMIFS( $K421:$K$520,\n          $B421:$B$520, $B420 & \".*\",\n          $B421:$B$520, \"<>\" & $B420 & \".*.*\"\n) )","v":0},{"$f":"IF( $G420 <> \"\",\n     TRUNC( $H420 * $J420, 2 ),\n     SUMIFS( $L421:$L$520,\n              $B421:$B$520, $B420 & \".*\",\n              $B421:$B$520, \"<>\" & $B420 & \".*.*\"\n     ) )","v":0}]
[null,"9.2",null,null,"REVESTIMENTO CERÂMICO PARA PISO COM PLACAS TIPO PORCELANATO DE DIMENSÕES 60X60 CM APLICADA EM AMBIENTES DE ÁREA MAIOR QUE 10 M². AF_02/2023_PE","SERV","M²",null,null,0,{"$f":"IF( $G421 <> \"\",\nTRUNC( $H421 * $I421, 2 ),\nSUMIFS( $K422:$K$520,\n          $B422:$B$520, $B421 & \".*\",\n          $B422:$B$520, \"<>\" & $B421 & \".*.*\"\n) )","v":0},{"$f":"IF( $G421 <> \"\",\n     TRUNC( $H421 * $J421, 2 ),\n     SUMIFS( $L422:$L$520,\n              $B422:$B$520, $B421 & \".*\",\n              $B422:$B$520, \"<>\" & $B421 & \".*.*\"\n     ) )","v":0}]
[null,"9.3",null,null,"SOLEIRA EM GRANITO, LARGURA 15 CM, ESPESSURA 2,0 CM. AF_09/2020","SERV","M",null,null,0,{"$f":"IF( $G422 <> \"\",\nTRUNC( $H422 * $I422, 2 ),\nSUMIFS( $K423:$K$520,\n          $B423:$B$520, $B422 & \".*\",\n          $B423:$B$520, \"<>\" & $B422 & \".*.*\"\n) )","v":0},{"$f":"IF( $G422 <> \"\",\n     TRUNC( $H422 * $J422, 2 ),\n     SUMIFS( $L423:$L$520,\n              $B423:$B$520, $B422 & \".*\",\n              $B423:$B$520, \"<>\" & $B422 & \".*.*\"\n     ) )","v":0}]
[null,"9.4",null,null,"RODAPÉ CERÂMICO 10 X 50,0 CM, PORCELANATO, ELIZABETH OU SIMILAR, APLICADO COMARGAMASSA INDUSTRIALIZADA AC-III, REJUNTADO","SERV","M",null,null,0,{"$f":"IF( $G423 <> \"\",\nTRUNC( $H423 * $I423, 2 ),\nSUMIFS( $K424:$K$520,\n          $B424:$B$520, $B423 & \".*\",\n          $B424:$B$520, \"<>\" & $B423 & \".*.*\"\n) )","v":0},{"$f":"IF( $G423 <> \"\",\n     TRUNC( $H423 * $J423, 2 ),\n     SUMIFS( $L424:$L$520,\n              $B424:$B$520, $B423 & \".*\",\n              $B424:$B$520, \"<>\" & $B423 & \".*.*\"\n     ) )","v":0}]
[null,"9.5",null,null,"REGULARIZAÇÃO MANUAL E COMPACTAÇÃO COM PLACA VIBRATÓRIA","SERV","M²",null,null,0,{"$f":"IF( $G424 <> \"\",\nTRUNC( $H424 * $I424, 2 ),\nSUMIFS( $K425:$K$520,\n          $B425:$B$520, $B424 & \".*\",\n          $B425:$B$520, \"<>\" & $B424 & \".*.*\"\n) )","v":0},{"$f":"IF( $G424 <> \"\",\n     TRUNC( $H424 * $J424, 2 ),\n     SUMIFS( $L425:$L$520,\n              $B425:$B$520, $B424 & \".*\",\n              $B425:$B$520, \"<>\" & $B424 & \".*.*\"\n     ) )","v":0}]
[null,"9.6",null,null,"PISO PODOTÁTIL DE ALERTA OU DIRECIONAL, DE BORRACHA, ASSENTADO SOBRE ARGAMASSA. AF_05/2020","SERV","M",null,null,0,{"$f":"IF( $G425 <> \"\",\nTRUNC( $H425 * $I425, 2 ),\nSUMIFS( $K426:$K$520,\n          $B426:$B$520, $B425 & \".*\",\n          $B426:$B$520, \"<>\" & $B425 & \".*.*\"\n) )","v":0},{"$f":"IF( $G425 <> \"\",\n     TRUNC( $H425 * $J425, 2 ),\n     SUMIFS( $L426:$L$520,\n              $B426:$B$520, $B425 & \".*\",\n              $B426:$B$520, \"<>\" & $B425 & \".*.*\"\n     ) )","v":0}]
[null,"9.7",null,null,"EXECUÇÃO DE PAVIMENTO EM PISO INTERTRAVADO, COM BLOCO RETANGULAR COR NATURAL DE 20 X 10 CM, ESPESSURA 8 CM. AF_10/2022","SERV","M²",null,null,0,{"$f":"IF( $G426 <> \"\",\nTRUNC( $H426 * $I426, 2 ),\nSUMIFS( $K427:$K$520,\n          $B427:$B$520, $B426 & \".*\",\n          $B427:$B$520, \"<>\" & $B426 & \".*.*\"\n) )","v":0},{"$f":"IF( $G426 <> \"\",\n     TRUNC( $H426 * $J426, 2 ),\n     SUMIFS( $L427:$L$520,\n              $B427:$B$520, $B426 & \".*\",\n              $B427:$B$520, \"<>\" & $B426 & \".*.*\"\n     ) )","v":0}]
[null,"9.8",null,null,"RAMPA DE ACESSIBILIDADE EM CONCRETO MOLDADO IN LOCO, EM CALÇADA NOVA COM LARGURA MAIOR OU IGUAL À 3,00 M, FCK 25MPA, COM PISO PODOTÁTIL. AF_03/2024","SERV","UNID.",null,null,0,{"$f":"IF( $G427 <> \"\",\nTRUNC( $H427 * $I427, 2 ),\nSUMIFS( $K428:$K$520,\n          $B428:$B$520, $B427 & \".*\",\n          $B428:$B$520, \"<>\" & $B427 & \".*.*\"\n) )","v":0},{"$f":"IF( $G427 <> \"\",\n     TRUNC( $H427 * $J427, 2 ),\n     SUMIFS( $L428:$L$520,\n              $B428:$B$520, $B427 & \".*\",\n              $B428:$B$520, \"<>\" & $B427 & \".*.*\"\n     ) )","v":0}]
[null,"9.9",null,null,"ASSENTAMENTO DE GUIA (MEIO-FIO) EM TRECHO RETO, CONFECCIONADA EM CONCRETO PRÉ-FABRICADO, DIMENSÕES 100X15X13X30 CM (COMPRIMENTO X BASE INFERIOR X BASE SUPERIOR X ALTURA). AF_01/2024","SERV","M",null,null,0,{"$f":"IF( $G428 <> \"\",\nTRUNC( $H428 * $I428, 2 ),\nSUMIFS( $K429:$K$520,\n          $B429:$B$520, $B428 & \".*\",\n          $B429:$B$520, \"<>\" & $B428 & \".*.*\"\n) )","v":0},{"$f":"IF( $G428 <> \"\",\n     TRUNC( $H428 * $J428, 2 ),\n     SUMIFS( $L429:$L$520,\n              $B429:$B$520, $B428 & \".*\",\n              $B429:$B$520, \"<>\" & $B428 & \".*.*\"\n     ) )","v":0}]
[null,"9.10",null,null,"PLANTIO DE ÁRVORE ORNAMENTAL COM ALTURA DE MUDA MAIOR QUE 2,00 M E MENOR OU IGUAL A 4,00 M . AF_07/2024","SERV","UNID.",null,null,0,{"$f":"IF( $G429 <> \"\",\nTRUNC( $H429 * $I429, 2 ),\nSUMIFS( $K430:$K$520,\n          $B430:$B$520, $B429 & \".*\",\n          $B430:$B$520, \"<>\" & $B429 & \".*.*\"\n) )","v":0},{"$f":"IF( $G429 <> \"\",\n     TRUNC( $H429 * $J429, 2 ),\n     SUMIFS( $L430:$L$520,\n              $B430:$B$520, $B429 & \".*\",\n              $B430:$B$520, \"<>\" & $B429 & \".*.*\"\n     ) )","v":0}]
[null,10,null,null,"REVESTIMENTOS",{"$nulls":4},"",{"$f":"IF( $G430 <> \"\",\nTRUNC( $H430 * $I430, 2 ),\nSUMIFS( $K431:$K$520,\n          $B431:$B$520, $B430 & \".*\",\n          $B431:$B$520, \"<>\" & $B430 & \".*.*\"\n) )","v":0},{"$f":"IF( $G430 <> \"\",\n     TRUNC( $H430 * $J430, 2 ),\n     SUMIFS( $L431:$L$520,\n              $B431:$B$520, $B430 & \".*\",\n              $B431:$B$520, \"<>\" & $B430 & \".*.*\"\n     ) )","v":0}]
[null,"10.1",null,null,"FORNECIMENTO E INSTALAÇÃO DE PAINEL DE FACHADA EM PLACA CIMENTÍCIA, INCLUSIVE ESTRUTURA METÁLICA DE FIXAÇÃO, APLICAÇÃO DE MASSA ACRÍLICA E PINTURA.","SERV","M²",null,null,0,{"$f":"IF( $G431 <> \"\",\nTRUNC( $H431 * $I431, 2 ),\nSUMIFS( $K432:$K$520,\n          $B432:$B$520, $B431 & \".*\",\n          $B432:$B$520, \"<>\" & $B431 & \".*.*\"\n) )","v":0},{"$f":"IF( $G431 <> \"\",\n     TRUNC( $H431 * $J431, 2 ),\n     SUMIFS( $L432:$L$520,\n              $B432:$B$520, $B431 & \".*\",\n              $B432:$B$520, \"<>\" & $B431 & \".*.*\"\n     ) )","v":0}]
[null,"10.2",null,null,"REVESTIMENTO CERÂMICO PARA PAREDES INTERNAS COM PLACAS TIPO ESMALTADA DE DIMENSÕES 20X20 CM APLICADAS A MEIA ALTURA DAS PAREDES. AF_02/2023_PE","SERV","M²",null,null,0,{"$f":"IF( $G432 <> \"\",\nTRUNC( $H432 * $I432, 2 ),\nSUMIFS( $K433:$K$520,\n          $B433:$B$520, $B432 & \".*\",\n          $B433:$B$520, \"<>\" & $B432 & \".*.*\"\n) )","v":0},{"$f":"IF( $G432 <> \"\",\n     TRUNC( $H432 * $J432, 2 ),\n     SUMIFS( $L433:$L$520,\n              $B433:$B$520, $B432 & \".*\",\n              $B433:$B$520, \"<>\" & $B432 & \".*.*\"\n     ) )","v":0}]
[null,"10.3",null,null,"CHAPISCO APLICADO EM ALVENARIAS E ESTRUTURAS DE CONCRETO INTERNAS, COM COLHER DE PEDREIRO.  ARGAMASSA TRAÇO 1:3 COM PREPARO MANUAL. AF_10/2022","SERV","M²",null,null,0,{"$f":"IF( $G433 <> \"\",\nTRUNC( $H433 * $I433, 2 ),\nSUMIFS( $K434:$K$520,\n          $B434:$B$520, $B433 & \".*\",\n          $B434:$B$520, \"<>\" & $B433 & \".*.*\"\n) )","v":0},{"$f":"IF( $G433 <> \"\",\n     TRUNC( $H433 * $J433, 2 ),\n     SUMIFS( $L434:$L$520,\n              $B434:$B$520, $B433 & \".*\",\n              $B434:$B$520, \"<>\" & $B433 & \".*.*\"\n     ) )","v":0}]
[null,"10.4",null,null,"MASSA ÚNICA, EM ARGAMASSA TRAÇO 1:2:8, PREPARO MECÂNICO, APLICADA MANUALMENTE EM PAREDES INTERNAS DE AMBIENTES COM ÁREA ENTRE 5M² E 10M², E = 17,5MM, COM TALISCAS. AF_03/2024","SERV","M²",null,null,0,{"$f":"IF( $G434 <> \"\",\nTRUNC( $H434 * $I434, 2 ),\nSUMIFS( $K435:$K$520,\n          $B435:$B$520, $B434 & \".*\",\n          $B435:$B$520, \"<>\" & $B434 & \".*.*\"\n) )","v":0},{"$f":"IF( $G434 <> \"\",\n     TRUNC( $H434 * $J434, 2 ),\n     SUMIFS( $L435:$L$520,\n              $B435:$B$520, $B434 & \".*\",\n              $B435:$B$520, \"<>\" & $B434 & \".*.*\"\n     ) )","v":0}]
[null,"10.5",null,null,"REVESTIMENTO CERÂMICO PARA PISO COM PLACAS TIPO PORCELANATO DE DIMENSÕES 60X60 CM APLICADA EM AMBIENTES DE ÁREA MAIOR QUE 10 M². AF_02/2023_PE","SERV","M²",null,null,0,{"$f":"IF( $G435 <> \"\",\nTRUNC( $H435 * $I435, 2 ),\nSUMIFS( $K436:$K$520,\n          $B436:$B$520, $B435 & \".*\",\n          $B436:$B$520, \"<>\" & $B435 & \".*.*\"\n) )","v":0},{"$f":"IF( $G435 <> \"\",\n     TRUNC( $H435 * $J435, 2 ),\n     SUMIFS( $L436:$L$520,\n              $B436:$B$520, $B435 & \".*\",\n              $B436:$B$520, \"<>\" & $B435 & \".*.*\"\n     ) )","v":0}]
[null,"10.6",null,null,"TELHAMENTO COM TELHA EM AÇO GALVALUME, DUPLA, TRAPEZOIDAL, COM PREENCHIMENTO PIR 50MM, PRÉ-PINTADA, TP40 - 2 X 0,43MM, KINGSPAN- ISOESTE OU SIMILAR","SERV","M²",null,null,0,{"$f":"IF( $G436 <> \"\",\nTRUNC( $H436 * $I436, 2 ),\nSUMIFS( $K437:$K$520,\n          $B437:$B$520, $B436 & \".*\",\n          $B437:$B$520, \"<>\" & $B436 & \".*.*\"\n) )","v":0},{"$f":"IF( $G436 <> \"\",\n     TRUNC( $H436 * $J436, 2 ),\n     SUMIFS( $L437:$L$520,\n              $B437:$B$520, $B436 & \".*\",\n              $B437:$B$520, \"<>\" & $B436 & \".*.*\"\n     ) )","v":0}]
[null,"10.7",null,null,"TELHA TERMOISOLANTE REVESTIDA EM ACO GALVANIZADO, FACES SUPERIOR E INFERIOR EM TELHA TRAPEZOIDAL (SEM ACESSORIOS DE FIXACAO), REVESTIMENTO COM ESPESSURA DE 0,50 MM COM PRE-PINTURA NAS DUAS FACES, NUCLEO EM POLIESTIRENO (EPS) DE 50 MM","FORN","M²",null,null,0,{"$f":"IF( $G437 <> \"\",\nTRUNC( $H437 * $I437, 2 ),\nSUMIFS( $K438:$K$520,\n          $B438:$B$520, $B437 & \".*\",\n          $B438:$B$520, \"<>\" & $B437 & \".*.*\"\n) )","v":0},{"$f":"IF( $G437 <> \"\",\n     TRUNC( $H437 * $J437, 2 ),\n     SUMIFS( $L438:$L$520,\n              $B438:$B$520, $B437 & \".*\",\n              $B438:$B$520, \"<>\" & $B437 & \".*.*\"\n     ) )","v":0}]
[null,"10.8",null,null,"PEDRA GRANITICA OU BASALTO, CACO, RETALHO, CAVACO, TIPO MIRACEMA, MADEIRA, PADUANA, RACHINHA, SANTA ISABEL OU OUTRAS SIMILARES, E= *1,0 A *2,0 CM","FORN","M²",null,null,0,{"$f":"IF( $G438 <> \"\",\nTRUNC( $H438 * $I438, 2 ),\nSUMIFS( $K439:$K$520,\n          $B439:$B$520, $B438 & \".*\",\n          $B439:$B$520, \"<>\" & $B438 & \".*.*\"\n) )","v":0},{"$f":"IF( $G438 <> \"\",\n     TRUNC( $H438 * $J438, 2 ),\n     SUMIFS( $L439:$L$520,\n              $B439:$B$520, $B438 & \".*\",\n              $B439:$B$520, \"<>\" & $B438 & \".*.*\"\n     ) )","v":0}]
[null,11,null,null,"PINTURA",{"$nulls":4},"",{"$f":"IF( $G439 <> \"\",\nTRUNC( $H439 * $I439, 2 ),\nSUMIFS( $K440:$K$520,\n          $B440:$B$520, $B439 & \".*\",\n          $B440:$B$520, \"<>\" & $B439 & \".*.*\"\n) )","v":0},{"$f":"IF( $G439 <> \"\",\n     TRUNC( $H439 * $J439, 2 ),\n     SUMIFS( $L440:$L$520,\n              $B440:$B$520, $B439 & \".*\",\n              $B440:$B$520, \"<>\" & $B439 & \".*.*\"\n     ) )","v":0}]
[null,"11.1",null,null,"PINTURA TINTA DE ACABAMENTO (PIGMENTADA) ESMALTE SINTÉTICO ACETINADO EM MADEIRA, 2 DEMÃOS. AF_01/2021","SERV","M²",null,null,0,{"$f":"IF( $G440 <> \"\",\nTRUNC( $H440 * $I440, 2 ),\nSUMIFS( $K441:$K$520,\n          $B441:$B$520, $B440 & \".*\",\n          $B441:$B$520, \"<>\" & $B440 & \".*.*\"\n) )","v":0},{"$f":"IF( $G440 <> \"\",\n     TRUNC( $H440 * $J440, 2 ),\n     SUMIFS( $L441:$L$520,\n              $B441:$B$520, $B440 & \".*\",\n              $B441:$B$520, \"<>\" & $B440 & \".*.*\"\n     ) )","v":0}]
[null,"11.2",null,null,"PINTURA COM TINTA ALQUÍDICA DE ACABAMENTO (ESMALTE SINTÉTICO BRILHANTE) PULVERIZADA SOBRE SUPERFÍCIES METÁLICAS (EXCETO PERFIL) EXECUTADO EM OBRA (02 DEMÃOS). AF_01/2020_PE","SERV","M²",null,null,0,{"$f":"IF( $G441 <> \"\",\nTRUNC( $H441 * $I441, 2 ),\nSUMIFS( $K442:$K$520,\n          $B442:$B$520, $B441 & \".*\",\n          $B442:$B$520, \"<>\" & $B441 & \".*.*\"\n) )","v":0},{"$f":"IF( $G441 <> \"\",\n     TRUNC( $H441 * $J441, 2 ),\n     SUMIFS( $L442:$L$520,\n              $B442:$B$520, $B441 & \".*\",\n              $B442:$B$520, \"<>\" & $B441 & \".*.*\"\n     ) )","v":0}]
[null,"11.3",null,null,"EMASSAMENTO COM MASSA LÁTEX, APLICAÇÃO EM PAREDE, DUAS DEMÃOS, LIXAMENTO MANUAL. AF_04/2023","SERV","M²",null,null,0,{"$f":"IF( $G442 <> \"\",\nTRUNC( $H442 * $I442, 2 ),\nSUMIFS( $K443:$K$520,\n          $B443:$B$520, $B442 & \".*\",\n          $B443:$B$520, \"<>\" & $B442 & \".*.*\"\n) )","v":0},{"$f":"IF( $G442 <> \"\",\n     TRUNC( $H442 * $J442, 2 ),\n     SUMIFS( $L443:$L$520,\n              $B443:$B$520, $B442 & \".*\",\n              $B443:$B$520, \"<>\" & $B442 & \".*.*\"\n     ) )","v":0}]
[null,"11.4",null,null,"APLICAÇÃO MANUAL DE MASSA ACRÍLICA EM PAREDES EXTERNAS DE CASAS, DUAS DEMÃOS. AF_03/2024","SERV","M²",null,null,0,{"$f":"IF( $G443 <> \"\",\nTRUNC( $H443 * $I443, 2 ),\nSUMIFS( $K444:$K$520,\n          $B444:$B$520, $B443 & \".*\",\n          $B444:$B$520, \"<>\" & $B443 & \".*.*\"\n) )","v":0},{"$f":"IF( $G443 <> \"\",\n     TRUNC( $H443 * $J443, 2 ),\n     SUMIFS( $L444:$L$520,\n              $B444:$B$520, $B443 & \".*\",\n              $B444:$B$520, \"<>\" & $B443 & \".*.*\"\n     ) )","v":0}]
[null,"11.5",null,null,"PINTURA LÁTEX ACRÍLICA PREMIUM, APLICAÇÃO MANUAL EM PAREDES, DUAS DEMÃOS. AF_04/2023","SERV","M²",null,null,0,{"$f":"IF( $G444 <> \"\",\nTRUNC( $H444 * $I444, 2 ),\nSUMIFS( $K445:$K$520,\n          $B445:$B$520, $B444 & \".*\",\n          $B445:$B$520, \"<>\" & $B444 & \".*.*\"\n) )","v":0},{"$f":"IF( $G444 <> \"\",\n     TRUNC( $H444 * $J444, 2 ),\n     SUMIFS( $L445:$L$520,\n              $B445:$B$520, $B444 & \".*\",\n              $B445:$B$520, \"<>\" & $B444 & \".*.*\"\n     ) )","v":0}]
[null,"11.6",null,null,"PINTURA COM TINTA ALQUÍDICA DE ACABAMENTO (ESMALTE SINTÉTICO BRILHANTE) PULVERIZADA SOBRE SUPERFÍCIES METÁLICAS (EXCETO PERFIL) EXECUTADO EM OBRA (02 DEMÃOS). AF_01/2020_PE","SERV","M²",null,null,0,{"$f":"IF( $G445 <> \"\",\nTRUNC( $H445 * $I445, 2 ),\nSUMIFS( $K446:$K$520,\n          $B446:$B$520, $B445 & \".*\",\n          $B446:$B$520, \"<>\" & $B445 & \".*.*\"\n) )","v":0},{"$f":"IF( $G445 <> \"\",\n     TRUNC( $H445 * $J445, 2 ),\n     SUMIFS( $L446:$L$520,\n              $B446:$B$520, $B445 & \".*\",\n              $B446:$B$520, \"<>\" & $B445 & \".*.*\"\n     ) )","v":0}]
[null,"11.7",null,null,"EMASSAMENTO COM MASSA LÁTEX, APLICAÇÃO EM TETO, UMA DEMÃO, LIXAMENTO MANUAL. AF_04/2023","SERV","M²",null,null,0,{"$f":"IF( $G446 <> \"\",\nTRUNC( $H446 * $I446, 2 ),\nSUMIFS( $K447:$K$520,\n          $B447:$B$520, $B446 & \".*\",\n          $B447:$B$520, \"<>\" & $B446 & \".*.*\"\n) )","v":0},{"$f":"IF( $G446 <> \"\",\n     TRUNC( $H446 * $J446, 2 ),\n     SUMIFS( $L447:$L$520,\n              $B447:$B$520, $B446 & \".*\",\n              $B447:$B$520, \"<>\" & $B446 & \".*.*\"\n     ) )","v":0}]
[null,"11.8",null,null,"PINTURA LÁTEX ACRÍLICA STANDARD, APLICAÇÃO MANUAL EM TETO, DUAS DEMÃOS. AF_04/2023","SERV","M²",null,null,0,{"$f":"IF( $G447 <> \"\",\nTRUNC( $H447 * $I447, 2 ),\nSUMIFS( $K448:$K$520,\n          $B448:$B$520, $B447 & \".*\",\n          $B448:$B$520, \"<>\" & $B447 & \".*.*\"\n) )","v":0},{"$f":"IF( $G447 <> \"\",\n     TRUNC( $H447 * $J447, 2 ),\n     SUMIFS( $L448:$L$520,\n              $B448:$B$520, $B447 & \".*\",\n              $B448:$B$520, \"<>\" & $B447 & \".*.*\"\n     ) )","v":0}]
[null,"11.9",null,null,"FUNDO SELADOR ACRÍLICO, APLICAÇÃO MANUAL EM PAREDE, UMA DEMÃO. AF_04/2023","SERV","M²",null,null,0,{"$f":"IF( $G448 <> \"\",\nTRUNC( $H448 * $I448, 2 ),\nSUMIFS( $K449:$K$520,\n          $B449:$B$520, $B448 & \".*\",\n          $B449:$B$520, \"<>\" & $B448 & \".*.*\"\n) )","v":0},{"$f":"IF( $G448 <> \"\",\n     TRUNC( $H448 * $J448, 2 ),\n     SUMIFS( $L449:$L$520,\n              $B449:$B$520, $B448 & \".*\",\n              $B449:$B$520, \"<>\" & $B448 & \".*.*\"\n     ) )","v":0}]
[null,"11.10",null,null,"FUNDO SELADOR ACRÍLICO, APLICAÇÃO MANUAL EM TETO, UMA DEMÃO. AF_04/2023","SERV","M²",null,null,0,{"$f":"IF( $G449 <> \"\",\nTRUNC( $H449 * $I449, 2 ),\nSUMIFS( $K450:$K$520,\n          $B450:$B$520, $B449 & \".*\",\n          $B450:$B$520, \"<>\" & $B449 & \".*.*\"\n) )","v":0},{"$f":"IF( $G449 <> \"\",\n     TRUNC( $H449 * $J449, 2 ),\n     SUMIFS( $L450:$L$520,\n              $B450:$B$520, $B449 & \".*\",\n              $B450:$B$520, \"<>\" & $B449 & \".*.*\"\n     ) )","v":0}]
[null,12,null,null,"PROJETO PREVENTIVO CONTRA INCÊNDIO",{"$nulls":4},"",{"$f":"IF( $G450 <> \"\",\nTRUNC( $H450 * $I450, 2 ),\nSUMIFS( $K451:$K$520,\n          $B451:$B$520, $B450 & \".*\",\n          $B451:$B$520, \"<>\" & $B450 & \".*.*\"\n) )","v":0},{"$f":"IF( $G450 <> \"\",\n     TRUNC( $H450 * $J450, 2 ),\n     SUMIFS( $L451:$L$520,\n              $B451:$B$520, $B450 & \".*\",\n              $B451:$B$520, \"<>\" & $B450 & \".*.*\"\n     ) )","v":0}]
[null,"12.1",null,null,"PLACA DE SINALIZACAO, FOTOLUMINESCENTE, 38X19 CM, EM PVC , COM SETA INDICATIVA DE SENTIDO (ESQUERDA OU DIREITA) DE SAÍDA DE EMERGÊNCIA- PLACA S2","SERV","UNID.",null,null,0,{"$f":"IF( $G451 <> \"\",\nTRUNC( $H451 * $I451, 2 ),\nSUMIFS( $K452:$K$520,\n          $B452:$B$520, $B451 & \".*\",\n          $B452:$B$520, \"<>\" & $B451 & \".*.*\"\n) )","v":0},{"$f":"IF( $G451 <> \"\",\n     TRUNC( $H451 * $J451, 2 ),\n     SUMIFS( $L452:$L$520,\n              $B452:$B$520, $B451 & \".*\",\n              $B452:$B$520, \"<>\" & $B451 & \".*.*\"\n     ) )","v":0}]
[null,"12.2",null,null,"FORNECIMENTO E INSTALAÇÃO DE CRUZETAL EM PVC, PARA ELETROCALHA, 300X100MM","SERV","UNID.",null,null,0,{"$f":"IF( $G452 <> \"\",\nTRUNC( $H452 * $I452, 2 ),\nSUMIFS( $K453:$K$520,\n          $B453:$B$520, $B452 & \".*\",\n          $B453:$B$520, \"<>\" & $B452 & \".*.*\"\n) )","v":0},{"$f":"IF( $G452 <> \"\",\n     TRUNC( $H452 * $J452, 2 ),\n     SUMIFS( $L453:$L$520,\n              $B453:$B$520, $B452 & \".*\",\n              $B453:$B$520, \"<>\" & $B452 & \".*.*\"\n     ) )","v":0}]
[null,"12.3",null,null,"PLACA DE SINALIZACAO DE SEGURANCA CONTRA INCENDIO, FOTOLUMINESCENTE, QUADRADA, *20 X 20* CM, EM PVC *2* MM ANTI-CHAMAS (SIMBOLOS, CORES E PICTOGRAMAS CONFORME NBR 13434)","SERV","UNID.",null,null,0,{"$f":"IF( $G453 <> \"\",\nTRUNC( $H453 * $I453, 2 ),\nSUMIFS( $K454:$K$520,\n          $B454:$B$520, $B453 & \".*\",\n          $B454:$B$520, \"<>\" & $B453 & \".*.*\"\n) )","v":0},{"$f":"IF( $G453 <> \"\",\n     TRUNC( $H453 * $J453, 2 ),\n     SUMIFS( $L454:$L$520,\n              $B454:$B$520, $B453 & \".*\",\n              $B454:$B$520, \"<>\" & $B453 & \".*.*\"\n     ) )","v":0}]
[null,"12.4",null,null,"LUMINÁRIA DE EMERGÊNCIA C/ DOIS PROJETORS LED ALIMENTAÇÃO 127/220 DE 12V/55 AUTONOMIA DE 3HORAS","FORN","UNID.",null,null,0,{"$f":"IF( $G454 <> \"\",\nTRUNC( $H454 * $I454, 2 ),\nSUMIFS( $K455:$K$520,\n          $B455:$B$520, $B454 & \".*\",\n          $B455:$B$520, \"<>\" & $B454 & \".*.*\"\n) )","v":0},{"$f":"IF( $G454 <> \"\",\n     TRUNC( $H454 * $J454, 2 ),\n     SUMIFS( $L455:$L$520,\n              $B455:$B$520, $B454 & \".*\",\n              $B455:$B$520, \"<>\" & $B454 & \".*.*\"\n     ) )","v":0}]
[null,"12.5",null,null,"PLACA DE SINALIZACAO, FOTOLUMINESCENTE, 30X30 CM, EM PVC , COM LOGOTIPO \"ABRIGO DE MANGUEIRA E HIDRANTE\"- PLACA E7","SERV","UNID.",null,null,0,{"$f":"IF( $G455 <> \"\",\nTRUNC( $H455 * $I455, 2 ),\nSUMIFS( $K456:$K$520,\n          $B456:$B$520, $B455 & \".*\",\n          $B456:$B$520, \"<>\" & $B455 & \".*.*\"\n) )","v":0},{"$f":"IF( $G455 <> \"\",\n     TRUNC( $H455 * $J455, 2 ),\n     SUMIFS( $L456:$L$520,\n              $B456:$B$520, $B455 & \".*\",\n              $B456:$B$520, \"<>\" & $B455 & \".*.*\"\n     ) )","v":0}]
[null,"12.6",null,null,"PLACA DE SINALIZACAO, FOTOLUMINESCENTE, 38X19 CM, EM PVC , COM LOGOTIPO \"COMANDO MANUAL DE ALARME DE INCÊNDIO\"- PLACA E2","SERV","UNID.",null,null,0,{"$f":"IF( $G456 <> \"\",\nTRUNC( $H456 * $I456, 2 ),\nSUMIFS( $K457:$K$520,\n          $B457:$B$520, $B456 & \".*\",\n          $B457:$B$520, \"<>\" & $B456 & \".*.*\"\n) )","v":0},{"$f":"IF( $G456 <> \"\",\n     TRUNC( $H456 * $J456, 2 ),\n     SUMIFS( $L457:$L$520,\n              $B457:$B$520, $B456 & \".*\",\n              $B457:$B$520, \"<>\" & $B456 & \".*.*\"\n     ) )","v":0}]
[null,"12.7",null,null,"PLACA DE SINALIZACAO, FOTOLUMINESCENTE, 30X30 CM, EM PVC , COM LOGOTIPO \"ALARME SONORO\"- PLACA E1","FORN","UNID.",null,null,{"$f":"IF(F457<>\"\",\nTRUNC(IF(F457=\"SERV\",I457*(1+$L$5/100),I457*(1+$L$6/100)),2),\n\"\" )","v":0},{"$f":"IF( $G457 <> \"\",\nTRUNC( $H457 * $I457, 2 ),\nSUMIFS( $K458:$K$520,\n          $B458:$B$520, $B457 & \".*\",\n          $B458:$B$520, \"<>\" & $B457 & \".*.*\"\n) )","v":0},{"$f":"IF( $G457 <> \"\",\n     TRUNC( $H457 * $J457, 2 ),\n     SUMIFS( $L458:$L$520,\n              $B458:$B$520, $B457 & \".*\",\n              $B458:$B$520, \"<>\" & $B457 & \".*.*\"\n     ) )","v":0}]
[null,"12.8",null,null,"EXTINTOR DE PÓ QUÍMICO ABC, CAPACIDADE 6 KG, ALCANCE MÉDIO DO JATO 5M , TEMPODE DESCARGA 12S, NBR9443, 9444, 10721","SERV","UNID.",null,null,0,{"$f":"IF( $G458 <> \"\",\nTRUNC( $H458 * $I458, 2 ),\nSUMIFS( $K459:$K$520,\n          $B459:$B$520, $B458 & \".*\",\n          $B459:$B$520, \"<>\" & $B458 & \".*.*\"\n) )","v":0},{"$f":"IF( $G458 <> \"\",\n     TRUNC( $H458 * $J458, 2 ),\n     SUMIFS( $L459:$L$520,\n              $B459:$B$520, $B458 & \".*\",\n              $B459:$B$520, \"<>\" & $B458 & \".*.*\"\n     ) )","v":0}]
[null,"12.9",null,null,"PINTURA DE SÍMBOLOS E TEXTOS COM TINTA ACRÍLICA, DEMARCAÇÃO COM FITA ADESIVA E APLICAÇÃO COM ROLO. AF_05/2021","SERV","M²",null,null,0,{"$f":"IF( $G459 <> \"\",\nTRUNC( $H459 * $I459, 2 ),\nSUMIFS( $K460:$K$520,\n          $B460:$B$520, $B459 & \".*\",\n          $B460:$B$520, \"<>\" & $B459 & \".*.*\"\n) )","v":0},{"$f":"IF( $G459 <> \"\",\n     TRUNC( $H459 * $J459, 2 ),\n     SUMIFS( $L460:$L$520,\n              $B460:$B$520, $B459 & \".*\",\n              $B460:$B$520, \"<>\" & $B459 & \".*.*\"\n     ) )","v":0}]
[null,"12.10",null,null,"EXTINTOR DE INCÊNDIO PORTÁTIL COM CARGA DE PQS DE 6 KG, CLASSE BC - FORNECIMENTO E INSTALAÇÃO. AF_10/2020_PE","SERV","UNID.",null,null,0,{"$f":"IF( $G460 <> \"\",\nTRUNC( $H460 * $I460, 2 ),\nSUMIFS( $K461:$K$520,\n          $B461:$B$520, $B460 & \".*\",\n          $B461:$B$520, \"<>\" & $B460 & \".*.*\"\n) )","v":0},{"$f":"IF( $G460 <> \"\",\n     TRUNC( $H460 * $J460, 2 ),\n     SUMIFS( $L461:$L$520,\n              $B461:$B$520, $B460 & \".*\",\n              $B461:$B$520, \"<>\" & $B460 & \".*.*\"\n     ) )","v":0}]
[null,"12.11",null,null,"ABRIGO PARA HIDRANTE INTERNO, INCLUSIVE CAIXA EMBUTIR CHAPA FERRO N.º 14, DIMENSÕES 0.90 X 0.60 X 0.17 M, REGISTRO TIPO GLOBO 2 1/2\", COM 02 MANGUEIRAS (15M E 30M) COM ESGUICHO E CONEXÕES - REV. 01","SERV","UNID.",null,null,0,{"$f":"IF( $G461 <> \"\",\nTRUNC( $H461 * $I461, 2 ),\nSUMIFS( $K462:$K$520,\n          $B462:$B$520, $B461 & \".*\",\n          $B462:$B$520, \"<>\" & $B461 & \".*.*\"\n) )","v":0},{"$f":"IF( $G461 <> \"\",\n     TRUNC( $H461 * $J461, 2 ),\n     SUMIFS( $L462:$L$520,\n              $B462:$B$520, $B461 & \".*\",\n              $B462:$B$520, \"<>\" & $B461 & \".*.*\"\n     ) )","v":0}]
[null,"12.12",null,null,"ACIONADOR MANUAL (BOTOEIRA) TIPO QUEBRA-VIDRO, P/INSTAL. INCENDIO","SERV","UNID.",null,null,0,{"$f":"IF( $G462 <> \"\",\nTRUNC( $H462 * $I462, 2 ),\nSUMIFS( $K463:$K$520,\n          $B463:$B$520, $B462 & \".*\",\n          $B463:$B$520, \"<>\" & $B462 & \".*.*\"\n) )","v":0},{"$f":"IF( $G462 <> \"\",\n     TRUNC( $H462 * $J462, 2 ),\n     SUMIFS( $L463:$L$520,\n              $B463:$B$520, $B462 & \".*\",\n              $B463:$B$520, \"<>\" & $B462 & \".*.*\"\n     ) )","v":0}]
[null,"12.13",null,null,"CENTRAL DE ALARME ENDEREÇÁVEL DE INCENDIO COM SISTEMA P/ ATÉ 250 DISPOSITIVOS, MARCAL VERIN OU SIMILAR, MODELO VRE-250 C/ BATERIA DE 12V E 7AMPERES","SERV","UNID.",null,null,0,{"$f":"IF( $G463 <> \"\",\nTRUNC( $H463 * $I463, 2 ),\nSUMIFS( $K464:$K$520,\n          $B464:$B$520, $B463 & \".*\",\n          $B464:$B$520, \"<>\" & $B463 & \".*.*\"\n) )","v":0},{"$f":"IF( $G463 <> \"\",\n     TRUNC( $H463 * $J463, 2 ),\n     SUMIFS( $L464:$L$520,\n              $B464:$B$520, $B463 & \".*\",\n              $B464:$B$520, \"<>\" & $B463 & \".*.*\"\n     ) )","v":0}]
[null,"12.14",null,null,"SIRENE AÚDIOVISUAL ENDEREÇAVEL, 120DB, PARA ALARME DE INCÊNDIO","SERV","UNID.",null,null,0,{"$f":"IF( $G464 <> \"\",\nTRUNC( $H464 * $I464, 2 ),\nSUMIFS( $K465:$K$520,\n          $B465:$B$520, $B464 & \".*\",\n          $B465:$B$520, \"<>\" & $B464 & \".*.*\"\n) )","v":0},{"$f":"IF( $G464 <> \"\",\n     TRUNC( $H464 * $J464, 2 ),\n     SUMIFS( $L465:$L$520,\n              $B465:$B$520, $B464 & \".*\",\n              $B465:$B$520, \"<>\" & $B464 & \".*.*\"\n     ) )","v":0}]
[null,"12.15",null,null,"BOMBA CENTRÍFUGA, TRIFÁSICA, 1 CV OU 0,99 HP, HM 14 A 40 M, Q 0,6 A 8,4 M3/H - FORNECIMENTO E INSTALAÇÃO. AF_12/2020","SERV","UNID.",null,null,0,{"$f":"IF( $G465 <> \"\",\nTRUNC( $H465 * $I465, 2 ),\nSUMIFS( $K466:$K$520,\n          $B466:$B$520, $B465 & \".*\",\n          $B466:$B$520, \"<>\" & $B465 & \".*.*\"\n) )","v":0},{"$f":"IF( $G465 <> \"\",\n     TRUNC( $H465 * $J465, 2 ),\n     SUMIFS( $L466:$L$520,\n              $B466:$B$520, $B465 & \".*\",\n              $B466:$B$520, \"<>\" & $B465 & \".*.*\"\n     ) )","v":0}]
[null,"12.16",null,null,"CHAVE DE BOIA AUTOMÁTICA SUPERIOR/INFERIOR 15A/250V - FORNECIMENTO E INSTALAÇÃO. AF_12/2020","SERV","UNID.",null,null,0,{"$f":"IF( $G466 <> \"\",\nTRUNC( $H466 * $I466, 2 ),\nSUMIFS( $K467:$K$520,\n          $B467:$B$520, $B466 & \".*\",\n          $B467:$B$520, \"<>\" & $B466 & \".*.*\"\n) )","v":0},{"$f":"IF( $G466 <> \"\",\n     TRUNC( $H466 * $J466, 2 ),\n     SUMIFS( $L467:$L$520,\n              $B467:$B$520, $B466 & \".*\",\n              $B467:$B$520, \"<>\" & $B466 & \".*.*\"\n     ) )","v":0}]
[null,"12.17",null,null,"ASSENTAMENTO DE TUBOS EM FERRO FUNDIDO, JUNTA ELÁSTICA, PONTA / BOLSA, DIAM.=   600 MM","SERV","M",null,null,0,{"$f":"IF( $G467 <> \"\",\nTRUNC( $H467 * $I467, 2 ),\nSUMIFS( $K468:$K$520,\n          $B468:$B$520, $B467 & \".*\",\n          $B468:$B$520, \"<>\" & $B467 & \".*.*\"\n) )","v":0},{"$f":"IF( $G467 <> \"\",\n     TRUNC( $H467 * $J467, 2 ),\n     SUMIFS( $L468:$L$520,\n              $B468:$B$520, $B467 & \".*\",\n              $B468:$B$520, \"<>\" & $B467 & \".*.*\"\n     ) )","v":0}]
[null,"12.18",null,null,"TUBO DE AÇO GALVANIZADO LEVE C/ COSTURA C/ ROSCA BSP Ø = 60,30MM ( 2\" ), E = 2,65MM, L = 6000MM NBR 5580","FORN","M",null,null,0,{"$f":"IF( $G468 <> \"\",\nTRUNC( $H468 * $I468, 2 ),\nSUMIFS( $K469:$K$520,\n          $B469:$B$520, $B468 & \".*\",\n          $B469:$B$520, \"<>\" & $B468 & \".*.*\"\n) )","v":0},{"$f":"IF( $G468 <> \"\",\n     TRUNC( $H468 * $J468, 2 ),\n     SUMIFS( $L469:$L$520,\n              $B469:$B$520, $B468 & \".*\",\n              $B469:$B$520, \"<>\" & $B468 & \".*.*\"\n     ) )","v":0}]
[null,13,null,null,"FORROS",{"$nulls":4},"",{"$f":"IF( $G469 <> \"\",\nTRUNC( $H469 * $I469, 2 ),\nSUMIFS( $K470:$K$520,\n          $B470:$B$520, $B469 & \".*\",\n          $B470:$B$520, \"<>\" & $B469 & \".*.*\"\n) )","v":0},{"$f":"IF( $G469 <> \"\",\n     TRUNC( $H469 * $J469, 2 ),\n     SUMIFS( $L470:$L$520,\n              $B470:$B$520, $B469 & \".*\",\n              $B470:$B$520, \"<>\" & $B469 & \".*.*\"\n     ) )","v":0}]
[null,"13.1",null,null,"BRISE METÁLICO HUNTER DOUGLAS REF. MINIWARE # 103 COR PRATA OU SIMILAR, COM ESTRUTURA E MONTAGEM, EXCLUSIVE ANDAIMES OU PLATAFORMA","SERV","M²",null,null,0,{"$f":"IF( $G470 <> \"\",\nTRUNC( $H470 * $I470, 2 ),\nSUMIFS( $K471:$K$520,\n          $B471:$B$520, $B470 & \".*\",\n          $B471:$B$520, \"<>\" & $B470 & \".*.*\"\n) )","v":0},{"$f":"IF( $G470 <> \"\",\n     TRUNC( $H470 * $J470, 2 ),\n     SUMIFS( $L471:$L$520,\n              $B471:$B$520, $B470 & \".*\",\n              $B471:$B$520, \"<>\" & $B470 & \".*.*\"\n     ) )","v":0}]
[null,"13.2",null,null,"FORRO EM DRYWALL, PARA AMBIENTES COMERCIAIS, INCLUSIVE ESTRUTURA BIRECIONAL DE FIXAÇÃO. AF_08/2023_PS","SERV","M²",null,null,0,{"$f":"IF( $G471 <> \"\",\nTRUNC( $H471 * $I471, 2 ),\nSUMIFS( $K472:$K$520,\n          $B472:$B$520, $B471 & \".*\",\n          $B472:$B$520, \"<>\" & $B471 & \".*.*\"\n) )","v":0},{"$f":"IF( $G471 <> \"\",\n     TRUNC( $H471 * $J471, 2 ),\n     SUMIFS( $L472:$L$520,\n              $B472:$B$520, $B471 & \".*\",\n              $B472:$B$520, \"<>\" & $B471 & \".*.*\"\n     ) )","v":0}]
[null,"13.3",null,null,"FORRO EM MADEIRA PINUS, PARA AMBIENTES RESIDENCIAIS E COMERCIAIS, INCLUSIVE ESTRUTURA BIDIRECIONAL DE FIXAÇÃO. AF_08/2023","SERV","M²",null,null,0,{"$f":"IF( $G472 <> \"\",\nTRUNC( $H472 * $I472, 2 ),\nSUMIFS( $K473:$K$520,\n          $B473:$B$520, $B472 & \".*\",\n          $B473:$B$520, \"<>\" & $B472 & \".*.*\"\n) )","v":0},{"$f":"IF( $G472 <> \"\",\n     TRUNC( $H472 * $J472, 2 ),\n     SUMIFS( $L473:$L$520,\n              $B473:$B$520, $B472 & \".*\",\n              $B473:$B$520, \"<>\" & $B472 & \".*.*\"\n     ) )","v":0}]
[null,14,null,null,"ELEVADOR",{"$nulls":4},"",{"$f":"IF( $G473 <> \"\",\nTRUNC( $H473 * $I473, 2 ),\nSUMIFS( $K474:$K$520,\n          $B474:$B$520, $B473 & \".*\",\n          $B474:$B$520, \"<>\" & $B473 & \".*.*\"\n) )","v":0},{"$f":"IF( $G473 <> \"\",\n     TRUNC( $H473 * $J473, 2 ),\n     SUMIFS( $L474:$L$520,\n              $B474:$B$520, $B473 & \".*\",\n              $B474:$B$520, \"<>\" & $B473 & \".*.*\"\n     ) )","v":0}]
[null,"14.1",null,null,"PLATAFORMA ELEVATÓRIA PARA PNE, SEMI CABINADA, MODELO (UN140/1 ENTRADA)/ADJACENTE (ADJ140/2 ENTRADA) DIM. CABINE 1100X1400X1100MM, AÇO INOX, FECHAMENTO ALUMINIO COMP.(ACM) E VIDRO, 02 PARADAS PERC.3M CX. ALVENARIA, DA APTUS OU SIMILAR","SERV","UNID.",null,null,0,{"$f":"IF( $G474 <> \"\",\nTRUNC( $H474 * $I474, 2 ),\nSUMIFS( $K475:$K$520,\n          $B475:$B$520, $B474 & \".*\",\n          $B475:$B$520, \"<>\" & $B474 & \".*.*\"\n) )","v":0},{"$f":"IF( $G474 <> \"\",\n     TRUNC( $H474 * $J474, 2 ),\n     SUMIFS( $L475:$L$520,\n              $B475:$B$520, $B474 & \".*\",\n              $B475:$B$520, \"<>\" & $B474 & \".*.*\"\n     ) )","v":0}]
[null,15,null,null,"ESTACIONAMENTO",{"$nulls":4},"",{"$f":"IF( $G475 <> \"\",\nTRUNC( $H475 * $I475, 2 ),\nSUMIFS( $K476:$K$520,\n          $B476:$B$520, $B475 & \".*\",\n          $B476:$B$520, \"<>\" & $B475 & \".*.*\"\n) )","v":0},{"$f":"IF( $G475 <> \"\",\n     TRUNC( $H475 * $J475, 2 ),\n     SUMIFS( $L476:$L$520,\n              $B476:$B$520, $B475 & \".*\",\n              $B476:$B$520, \"<>\" & $B475 & \".*.*\"\n     ) )","v":0}]
[null,"15.1",null,null,"PISOS",{"$nulls":4},"",{"$f":"IF( $G476 <> \"\",\nTRUNC( $H476 * $I476, 2 ),\nSUMIFS( $K477:$K$520,\n          $B477:$B$520, $B476 & \".*\",\n          $B477:$B$520, \"<>\" & $B476 & \".*.*\"\n) )","v":0},{"$f":"IF( $G476 <> \"\",\n     TRUNC( $H476 * $J476, 2 ),\n     SUMIFS( $L477:$L$520,\n              $B477:$B$520, $B476 & \".*\",\n              $B477:$B$520, \"<>\" & $B476 & \".*.*\"\n     ) )","v":0}]
[null,"15.1.1",null,null,"LEVANTAMENTO TOPOGRÁFICO PLANIMÉTRICO CADASTRAL","SERV","M²",null,null,0,{"$f":"IF( $G477 <> \"\",\nTRUNC( $H477 * $I477, 2 ),\nSUMIFS( $K478:$K$520,\n          $B478:$B$520, $B477 & \".*\",\n          $B478:$B$520, \"<>\" & $B477 & \".*.*\"\n) )","v":0},{"$f":"IF( $G477 <> \"\",\n     TRUNC( $H477 * $J477, 2 ),\n     SUMIFS( $L478:$L$520,\n              $B478:$B$520, $B477 & \".*\",\n              $B478:$B$520, \"<>\" & $B477 & \".*.*\"\n     ) )","v":0}]
[null,"15.1.2",null,null,"LIMPEZA MECANIZADA DE CAMADA VEGETAL, VEGETAÇÃO E PEQUENAS ÁRVORES (DIÂMETRO DE TRONCO MENOR QUE 0,20 M), COM TRATOR DE ESTEIRAS. AF_03/2024","SERV","M²",null,null,0,{"$f":"IF( $G478 <> \"\",\nTRUNC( $H478 * $I478, 2 ),\nSUMIFS( $K479:$K$520,\n          $B479:$B$520, $B478 & \".*\",\n          $B479:$B$520, \"<>\" & $B478 & \".*.*\"\n) )","v":0},{"$f":"IF( $G478 <> \"\",\n     TRUNC( $H478 * $J478, 2 ),\n     SUMIFS( $L479:$L$520,\n              $B479:$B$520, $B478 & \".*\",\n              $B479:$B$520, \"<>\" & $B478 & \".*.*\"\n     ) )","v":0}]
[null,"15.1.3",null,null,"CARGA, MANOBRA E DESCARGA DE SOLOS E MATERIAIS GRANULARES EM CAMINHÃO BASCULANTE 10 M³ - CARGA COM PÁ CARREGADEIRA (CAÇAMBA DE 1,7 A 2,8 M³ / 128 HP) E DESCARGA LIVRE (UNIDADE: M3). AF_07/2020","SERV","M³",null,null,0,{"$f":"IF( $G479 <> \"\",\nTRUNC( $H479 * $I479, 2 ),\nSUMIFS( $K480:$K$520,\n          $B480:$B$520, $B479 & \".*\",\n          $B480:$B$520, \"<>\" & $B479 & \".*.*\"\n) )","v":0},{"$f":"IF( $G479 <> \"\",\n     TRUNC( $H479 * $J479, 2 ),\n     SUMIFS( $L480:$L$520,\n              $B480:$B$520, $B479 & \".*\",\n              $B480:$B$520, \"<>\" & $B479 & \".*.*\"\n     ) )","v":0}]
[null,"15.1.4",null,null,"TRANSPORTE COM CAMINHÃO BASCULANTE DE 10 M³, EM VIA URBANA PAVIMENTADA, ADICIONAL PARA DMT EXCEDENTE A 30 KM (UNIDADE: M3XKM). AF_07/2020","SERV","M³XKM",null,null,0,{"$f":"IF( $G480 <> \"\",\nTRUNC( $H480 * $I480, 2 ),\nSUMIFS( $K481:$K$520,\n          $B481:$B$520, $B480 & \".*\",\n          $B481:$B$520, \"<>\" & $B480 & \".*.*\"\n) )","v":0},{"$f":"IF( $G480 <> \"\",\n     TRUNC( $H480 * $J480, 2 ),\n     SUMIFS( $L481:$L$520,\n              $B481:$B$520, $B480 & \".*\",\n              $B481:$B$520, \"<>\" & $B480 & \".*.*\"\n     ) )","v":0}]
[null,"15.1.5",null,null,"REGULARIZAÇÃO E COMPACTAÇÃO DE SUBLEITO DE SOLO PREDOMINANTEMENTE ARGILOSO, PARA OBRAS DE CONSTRUÇÃO DE PAVIMENTOS. AF_09/2024","SERV","M²",null,null,0,{"$f":"IF( $G481 <> \"\",\nTRUNC( $H481 * $I481, 2 ),\nSUMIFS( $K482:$K$520,\n          $B482:$B$520, $B481 & \".*\",\n          $B482:$B$520, \"<>\" & $B481 & \".*.*\"\n) )","v":0},{"$f":"IF( $G481 <> \"\",\n     TRUNC( $H481 * $J481, 2 ),\n     SUMIFS( $L482:$L$520,\n              $B482:$B$520, $B481 & \".*\",\n              $B482:$B$520, \"<>\" & $B481 & \".*.*\"\n     ) )","v":0}]
[null,"15.1.6",null,null,"CONSTRUÇÃO DE BASE E SUB-BASE PARA PAVIMENTAÇÃO DE SOLO ESTABILIZADO GRANULOMETRICAMENTE COM MISTURA DE SOLOS EM PISTA - EXCLUSIVE SOLO, ESCAVAÇÃO, CARGA E TRANSPORTE. AF_09/2024","SERV","M³",null,null,0,{"$f":"IF( $G482 <> \"\",\nTRUNC( $H482 * $I482, 2 ),\nSUMIFS( $K483:$K$520,\n          $B483:$B$520, $B482 & \".*\",\n          $B483:$B$520, \"<>\" & $B482 & \".*.*\"\n) )","v":0},{"$f":"IF( $G482 <> \"\",\n     TRUNC( $H482 * $J482, 2 ),\n     SUMIFS( $L483:$L$520,\n              $B483:$B$520, $B482 & \".*\",\n              $B483:$B$520, \"<>\" & $B482 & \".*.*\"\n     ) )","v":0}]
[null,"15.1.7",null,null,"ESCAVAÇÃO MANUAL DE VALA. AF_09/2024","SERV","M³",null,null,0,{"$f":"IF( $G483 <> \"\",\nTRUNC( $H483 * $I483, 2 ),\nSUMIFS( $K484:$K$520,\n          $B484:$B$520, $B483 & \".*\",\n          $B484:$B$520, \"<>\" & $B483 & \".*.*\"\n) )","v":0},{"$f":"IF( $G483 <> \"\",\n     TRUNC( $H483 * $J483, 2 ),\n     SUMIFS( $L484:$L$520,\n              $B484:$B$520, $B483 & \".*\",\n              $B484:$B$520, \"<>\" & $B483 & \".*.*\"\n     ) )","v":0}]
[null,"15.1.8",null,null,"ASSENTAMENTO DE GUIA (MEIO-FIO) EM TRECHO RETO, CONFECCIONADA EM CONCRETO PRÉ-FABRICADO, DIMENSÕES 100X15X13X30 CM (COMPRIMENTO X BASE INFERIOR X BASE SUPERIOR X ALTURA). AF_01/2024","SERV","M",null,null,0,{"$f":"IF( $G484 <> \"\",\nTRUNC( $H484 * $I484, 2 ),\nSUMIFS( $K485:$K$520,\n          $B485:$B$520, $B484 & \".*\",\n          $B485:$B$520, \"<>\" & $B484 & \".*.*\"\n) )","v":0},{"$f":"IF( $G484 <> \"\",\n     TRUNC( $H484 * $J484, 2 ),\n     SUMIFS( $L485:$L$520,\n              $B485:$B$520, $B484 & \".*\",\n              $B485:$B$520, \"<>\" & $B484 & \".*.*\"\n     ) )","v":0}]
[null,"15.1.9",null,null,"ASSENTAMENTO DE GUIA (MEIO-FIO) EM TRECHO CURVO, CONFECCIONADA EM CONCRETO PRÉ-FABRICADO, DIMENSÕES 100X15X13X30 CM (COMPRIMENTO X BASE INFERIOR X BASE SUPERIOR X ALTURA). AF_01/2024","SERV","M",null,null,0,{"$f":"IF( $G485 <> \"\",\nTRUNC( $H485 * $I485, 2 ),\nSUMIFS( $K486:$K$520,\n          $B486:$B$520, $B485 & \".*\",\n          $B486:$B$520, \"<>\" & $B485 & \".*.*\"\n) )","v":0},{"$f":"IF( $G485 <> \"\",\n     TRUNC( $H485 * $J485, 2 ),\n     SUMIFS( $L486:$L$520,\n              $B486:$B$520, $B485 & \".*\",\n              $B486:$B$520, \"<>\" & $B485 & \".*.*\"\n     ) )","v":0}]
[null,"15.1.10",null,null,"EXECUÇÃO DE PAVIMENTO EM PISO INTERTRAVADO, COM BLOCO RETANGULAR COR NATURAL DE 20 X 10 CM, ESPESSURA 8 CM. AF_10/2022","SERV","M²",null,null,0,{"$f":"IF( $G486 <> \"\",\nTRUNC( $H486 * $I486, 2 ),\nSUMIFS( $K487:$K$520,\n          $B487:$B$520, $B486 & \".*\",\n          $B487:$B$520, \"<>\" & $B486 & \".*.*\"\n) )","v":0},{"$f":"IF( $G486 <> \"\",\n     TRUNC( $H486 * $J486, 2 ),\n     SUMIFS( $L487:$L$520,\n              $B487:$B$520, $B486 & \".*\",\n              $B487:$B$520, \"<>\" & $B486 & \".*.*\"\n     ) )","v":0}]
[null,"15.2",null,null,"DRENAGEM",{"$nulls":4},"",{"$f":"IF( $G487 <> \"\",\nTRUNC( $H487 * $I487, 2 ),\nSUMIFS( $K488:$K$520,\n          $B488:$B$520, $B487 & \".*\",\n          $B488:$B$520, \"<>\" & $B487 & \".*.*\"\n) )","v":0},{"$f":"IF( $G487 <> \"\",\n     TRUNC( $H487 * $J487, 2 ),\n     SUMIFS( $L488:$L$520,\n              $B488:$B$520, $B487 & \".*\",\n              $B488:$B$520, \"<>\" & $B487 & \".*.*\"\n     ) )","v":0}]
[null,"15.2.1",null,null,"ESCAVAÇÃO MECANIZADA DE VALA COM PROFUNDIDADE MAIOR QUE 1,5 M ATÉ 3,0 M (MÉDIA MONTANTE E JUSANTE/UMA COMPOSIÇÃO POR TRECHO), RETROESCAV (0,26 M3), LARGURA DE 0,8 M A 1,5 M, EM SOLO DE 1A CATEGORIA, LOCAIS COM BAIXO NÍVEL DE INTERFERÊNCIA. AF_09/2024","SERV","M³",null,null,0,{"$f":"IF( $G488 <> \"\",\nTRUNC( $H488 * $I488, 2 ),\nSUMIFS( $K489:$K$520,\n          $B489:$B$520, $B488 & \".*\",\n          $B489:$B$520, \"<>\" & $B488 & \".*.*\"\n) )","v":0},{"$f":"IF( $G488 <> \"\",\n     TRUNC( $H488 * $J488, 2 ),\n     SUMIFS( $L489:$L$520,\n              $B489:$B$520, $B488 & \".*\",\n              $B489:$B$520, \"<>\" & $B488 & \".*.*\"\n     ) )","v":0}]
[null,"15.2.2",null,null,"PREPARO DE FUNDO DE VALA COM LARGURA MENOR QUE 1,5 M, COM CAMADA DE AREIA, LANÇAMENTO MECANIZADO. AF_08/2020","SERV","M³",null,null,0,{"$f":"IF( $G489 <> \"\",\nTRUNC( $H489 * $I489, 2 ),\nSUMIFS( $K490:$K$520,\n          $B490:$B$520, $B489 & \".*\",\n          $B490:$B$520, \"<>\" & $B489 & \".*.*\"\n) )","v":0},{"$f":"IF( $G489 <> \"\",\n     TRUNC( $H489 * $J489, 2 ),\n     SUMIFS( $L490:$L$520,\n              $B490:$B$520, $B489 & \".*\",\n              $B490:$B$520, \"<>\" & $B489 & \".*.*\"\n     ) )","v":0}]
[null,"15.2.3",null,null,"TRANSPORTE COM CAMINHÃO BASCULANTE DE 10 M³, EM VIA URBANA PAVIMENTADA, ADICIONAL PARA DMT EXCEDENTE A 30 KM (UNIDADE: M3XKM). AF_07/2020","SERV","M³XKM",null,null,0,{"$f":"IF( $G490 <> \"\",\nTRUNC( $H490 * $I490, 2 ),\nSUMIFS( $K491:$K$520,\n          $B491:$B$520, $B490 & \".*\",\n          $B491:$B$520, \"<>\" & $B490 & \".*.*\"\n) )","v":0},{"$f":"IF( $G490 <> \"\",\n     TRUNC( $H490 * $J490, 2 ),\n     SUMIFS( $L491:$L$520,\n              $B491:$B$520, $B490 & \".*\",\n              $B491:$B$520, \"<>\" & $B490 & \".*.*\"\n     ) )","v":0}]
[null,"15.2.4",null,null,"TUBO DE CONCRETO PARA REDES COLETORAS DE ÁGUAS PLUVIAIS, DIÂMETRO DE 400 MM, JUNTA RÍGIDA, INSTALADO EM LOCAL COM ALTO NÍVEL DE INTERFERÊNCIAS - FORNECIMENTO E ASSENTAMENTO. AF_03/2024","SERV","M",null,null,0,{"$f":"IF( $G491 <> \"\",\nTRUNC( $H491 * $I491, 2 ),\nSUMIFS( $K492:$K$520,\n          $B492:$B$520, $B491 & \".*\",\n          $B492:$B$520, \"<>\" & $B491 & \".*.*\"\n) )","v":0},{"$f":"IF( $G491 <> \"\",\n     TRUNC( $H491 * $J491, 2 ),\n     SUMIFS( $L492:$L$520,\n              $B492:$B$520, $B491 & \".*\",\n              $B492:$B$520, \"<>\" & $B491 & \".*.*\"\n     ) )","v":0}]
[null,"15.2.5",null,null,"TAMPAO FOFO SIMPLES COM BASE / REQUADRO, CLASSE D400 CARGA MAX. 40 T, REDONDO, TAMPA 600 MM (COM INSCRICAO EM RELEVO DO TIPO DE REDE)","FORN","UNID.",null,null,0,{"$f":"IF( $G492 <> \"\",\nTRUNC( $H492 * $I492, 2 ),\nSUMIFS( $K493:$K$520,\n          $B493:$B$520, $B492 & \".*\",\n          $B493:$B$520, \"<>\" & $B492 & \".*.*\"\n) )","v":0},{"$f":"IF( $G492 <> \"\",\n     TRUNC( $H492 * $J492, 2 ),\n     SUMIFS( $L493:$L$520,\n              $B493:$B$520, $B492 & \".*\",\n              $B493:$B$520, \"<>\" & $B492 & \".*.*\"\n     ) )","v":0}]
[null,"15.2.6",null,null,"TUBO DE CONCRETO PARA REDES COLETORAS DE ÁGUAS PLUVIAIS, DIÂMETRO DE 600 MM, JUNTA RÍGIDA, INSTALADO EM LOCAL COM ALTO NÍVEL DE INTERFERÊNCIAS - FORNECIMENTO E ASSENTAMENTO. AF_03/2024","SERV","M",null,null,0,{"$f":"IF( $G493 <> \"\",\nTRUNC( $H493 * $I493, 2 ),\nSUMIFS( $K494:$K$520,\n          $B494:$B$520, $B493 & \".*\",\n          $B494:$B$520, \"<>\" & $B493 & \".*.*\"\n) )","v":0},{"$f":"IF( $G493 <> \"\",\n     TRUNC( $H493 * $J493, 2 ),\n     SUMIFS( $L494:$L$520,\n              $B494:$B$520, $B493 & \".*\",\n              $B494:$B$520, \"<>\" & $B493 & \".*.*\"\n     ) )","v":0}]
[null,"15.2.7",null,null,"REATERRO MECANIZADO DE VALA COM RETROESCAVADEIRA (CAPACIDADE DA CAÇAMBA   DA RETRO: 0,26 M³/POTÊNCIA: 88 HP), LARGURA 0,8 A 1,5 M, PROFUNDIDADE ATÉ 1,5 M, COM SOLO (SEM SUBSTITUIÇÃO) DE 1ª CATEGORIA, COM COMPACTADOR DE SOLOS DE PERCUSSÃO AF_08/2023","SERV","M³",null,null,0,{"$f":"IF( $G494 <> \"\",\nTRUNC( $H494 * $I494, 2 ),\nSUMIFS( $K495:$K$520,\n          $B495:$B$520, $B494 & \".*\",\n          $B495:$B$520, \"<>\" & $B494 & \".*.*\"\n) )","v":0},{"$f":"IF( $G494 <> \"\",\n     TRUNC( $H494 * $J494, 2 ),\n     SUMIFS( $L495:$L$520,\n              $B495:$B$520, $B494 & \".*\",\n              $B495:$B$520, \"<>\" & $B494 & \".*.*\"\n     ) )","v":0}]
[null,"15.2.8",null,null,"BASE PARA POÇO DE VISITA RETANGULAR PARA DRENAGEM, EM ALVENARIA COM BLOCOS DE CONCRETO, DIMENSÕES INTERNAS = 2X2 M, PROFUNDIDADE = 1,40 M, EXCLUINDO TAMPÃO. AF_12/2020_PA","SERV","UNID.",null,null,0,{"$f":"IF( $G495 <> \"\",\nTRUNC( $H495 * $I495, 2 ),\nSUMIFS( $K496:$K$520,\n          $B496:$B$520, $B495 & \".*\",\n          $B496:$B$520, \"<>\" & $B495 & \".*.*\"\n) )","v":0},{"$f":"IF( $G495 <> \"\",\n     TRUNC( $H495 * $J495, 2 ),\n     SUMIFS( $L496:$L$520,\n              $B496:$B$520, $B495 & \".*\",\n              $B496:$B$520, \"<>\" & $B495 & \".*.*\"\n     ) )","v":0}]
[null,"15.2.9",null,null,"CAIXA PARA BOCA DE LOBO COMBINADA COM GRELHA RETANGULAR, EM ALVENARIA COM BLOCOS DE CONCRETO, DIMENSÕES INTERNAS: 1,3X1X1,2 M. AF_12/2020","SERV","UNID.",null,null,0,{"$f":"IF( $G496 <> \"\",\nTRUNC( $H496 * $I496, 2 ),\nSUMIFS( $K497:$K$520,\n          $B497:$B$520, $B496 & \".*\",\n          $B497:$B$520, \"<>\" & $B496 & \".*.*\"\n) )","v":0},{"$f":"IF( $G496 <> \"\",\n     TRUNC( $H496 * $J496, 2 ),\n     SUMIFS( $L497:$L$520,\n              $B497:$B$520, $B496 & \".*\",\n              $B497:$B$520, \"<>\" & $B496 & \".*.*\"\n     ) )","v":0}]
[null,"15.3",null,null,"ILUMINAÇÃO",{"$nulls":4},"",{"$f":"IF( $G497 <> \"\",\nTRUNC( $H497 * $I497, 2 ),\nSUMIFS( $K498:$K$520,\n          $B498:$B$520, $B497 & \".*\",\n          $B498:$B$520, \"<>\" & $B497 & \".*.*\"\n) )","v":0},{"$f":"IF( $G497 <> \"\",\n     TRUNC( $H497 * $J497, 2 ),\n     SUMIFS( $L498:$L$520,\n              $B498:$B$520, $B497 & \".*\",\n              $B498:$B$520, \"<>\" & $B497 & \".*.*\"\n     ) )","v":0}]
[null,"15.3.1",null,null,"ELETRODUTO RÍGIDO ROSCÁVEL, PVC, DN 50 MM (1 1/2\"), PARA REDE ENTERRADA DE DISTRIBUIÇÃO DE ENERGIA ELÉTRICA - FORNECIMENTO E INSTALAÇÃO. AF_12/2021","SERV","M",null,null,0,{"$f":"IF( $G498 <> \"\",\nTRUNC( $H498 * $I498, 2 ),\nSUMIFS( $K499:$K$520,\n          $B499:$B$520, $B498 & \".*\",\n          $B499:$B$520, \"<>\" & $B498 & \".*.*\"\n) )","v":0},{"$f":"IF( $G498 <> \"\",\n     TRUNC( $H498 * $J498, 2 ),\n     SUMIFS( $L499:$L$520,\n              $B499:$B$520, $B498 & \".*\",\n              $B499:$B$520, \"<>\" & $B498 & \".*.*\"\n     ) )","v":0}]
[null,"15.3.2",null,null,"CABO DE COBRE FLEXÍVEL ISOLADO, 2,5 MM², ANTI-CHAMA 0,6/1,0 KV, PARA CIRCUITOS TERMINAIS - FORNECIMENTO E INSTALAÇÃO. AF_03/2023","SERV","M",null,null,0,{"$f":"IF( $G499 <> \"\",\nTRUNC( $H499 * $I499, 2 ),\nSUMIFS( $K500:$K$520,\n          $B500:$B$520, $B499 & \".*\",\n          $B500:$B$520, \"<>\" & $B499 & \".*.*\"\n) )","v":0},{"$f":"IF( $G499 <> \"\",\n     TRUNC( $H499 * $J499, 2 ),\n     SUMIFS( $L500:$L$520,\n              $B500:$B$520, $B499 & \".*\",\n              $B500:$B$520, \"<>\" & $B499 & \".*.*\"\n     ) )","v":0}]
[null,"15.3.3",null,null,"CAIXA ENTERRADA ELÉTRICA RETANGULAR, EM ALVENARIA COM BLOCOS DE CONCRETO, FUNDO COM BRITA, DIMENSÕES INTERNAS: 0,4X0,4X0,4 M. AF_12/2020","SERV","UNID.",null,null,0,{"$f":"IF( $G500 <> \"\",\nTRUNC( $H500 * $I500, 2 ),\nSUMIFS( $K501:$K$520,\n          $B501:$B$520, $B500 & \".*\",\n          $B501:$B$520, \"<>\" & $B500 & \".*.*\"\n) )","v":0},{"$f":"IF( $G500 <> \"\",\n     TRUNC( $H500 * $J500, 2 ),\n     SUMIFS( $L501:$L$520,\n              $B501:$B$520, $B500 & \".*\",\n              $B501:$B$520, \"<>\" & $B500 & \".*.*\"\n     ) )","v":0}]
[null,"15.3.4",null,null,"POSTE DECORATIVO 2 PÉTALAS, EM AÇO GALVANIZADO COM DIFUSOR EM VIDRO TRANSPARENTE TEMPERADO, COM 3M/4M, INCLUSIVE LÂMPADA DE LED 50W","SERV","UNID.",null,null,0,{"$f":"IF( $G501 <> \"\",\nTRUNC( $H501 * $I501, 2 ),\nSUMIFS( $K502:$K$520,\n          $B502:$B$520, $B501 & \".*\",\n          $B502:$B$520, \"<>\" & $B501 & \".*.*\"\n) )","v":0},{"$f":"IF( $G501 <> \"\",\n     TRUNC( $H501 * $J501, 2 ),\n     SUMIFS( $L502:$L$520,\n              $B502:$B$520, $B501 & \".*\",\n              $B502:$B$520, \"<>\" & $B501 & \".*.*\"\n     ) )","v":0}]
[null,"15.3.5",null,null,"POSTE DECORATIVO 1 PÉTALAS, EM AÇO GALVANIZADO COM DIFUSOR EM VIDRO TRANSPARENTE TEMPERADO, COM 3M/4M, INCLUSIVE LÂMPADA DE LED 50W","SERV","UNID.",null,null,0,{"$f":"IF( $G502 <> \"\",\nTRUNC( $H502 * $I502, 2 ),\nSUMIFS( $K503:$K$520,\n          $B503:$B$520, $B502 & \".*\",\n          $B503:$B$520, \"<>\" & $B502 & \".*.*\"\n) )","v":0},{"$f":"IF( $G502 <> \"\",\n     TRUNC( $H502 * $J502, 2 ),\n     SUMIFS( $L503:$L$520,\n              $B503:$B$520, $B502 & \".*\",\n              $B503:$B$520, \"<>\" & $B502 & \".*.*\"\n     ) )","v":0}]
[null,"15.3.6",null,null,"SENSOR DE PRESENÇA SEM FOTOCÉLULA, FIXAÇÃO EM PAREDE - FORNECIMENTO E INSTALAÇÃO. AF_09/2024","SERV","UNID.",null,null,0,{"$f":"IF( $G503 <> \"\",\nTRUNC( $H503 * $I503, 2 ),\nSUMIFS( $K504:$K$520,\n          $B504:$B$520, $B503 & \".*\",\n          $B504:$B$520, \"<>\" & $B503 & \".*.*\"\n) )","v":0},{"$f":"IF( $G503 <> \"\",\n     TRUNC( $H503 * $J503, 2 ),\n     SUMIFS( $L504:$L$520,\n              $B504:$B$520, $B503 & \".*\",\n              $B504:$B$520, \"<>\" & $B503 & \".*.*\"\n     ) )","v":0}]
[null,"15.4",null,null,"PAISAGISMO",{"$nulls":4},"",{"$f":"IF( $G504 <> \"\",\nTRUNC( $H504 * $I504, 2 ),\nSUMIFS( $K505:$K$520,\n          $B505:$B$520, $B504 & \".*\",\n          $B505:$B$520, \"<>\" & $B504 & \".*.*\"\n) )","v":0},{"$f":"IF( $G504 <> \"\",\n     TRUNC( $H504 * $J504, 2 ),\n     SUMIFS( $L505:$L$520,\n              $B505:$B$520, $B504 & \".*\",\n              $B505:$B$520, \"<>\" & $B504 & \".*.*\"\n     ) )","v":0}]
[null,"15.4.1",null,null,"PLANTIO DE GRAMA ESMERALDA OU SÃO CARLOS OU CURITIBANA, EM PLACAS. AF_07/2024","SERV","M²",null,null,0,{"$f":"IF( $G505 <> \"\",\nTRUNC( $H505 * $I505, 2 ),\nSUMIFS( $K506:$K$520,\n          $B506:$B$520, $B505 & \".*\",\n          $B506:$B$520, \"<>\" & $B505 & \".*.*\"\n) )","v":0},{"$f":"IF( $G505 <> \"\",\n     TRUNC( $H505 * $J505, 2 ),\n     SUMIFS( $L506:$L$520,\n              $B506:$B$520, $B505 & \".*\",\n              $B506:$B$520, \"<>\" & $B505 & \".*.*\"\n     ) )","v":0}]
[null,"15.4.2",null,null,"PLANTIO DE ÁRVORE ORNAMENTAL COM ALTURA DE MUDA MAIOR QUE 2,00 M E MENOR OU IGUAL A 4,00 M . AF_07/2024","SERV","UNID.",null,null,0,{"$f":"IF( $G506 <> \"\",\nTRUNC( $H506 * $I506, 2 ),\nSUMIFS( $K507:$K$520,\n          $B507:$B$520, $B506 & \".*\",\n          $B507:$B$520, \"<>\" & $B506 & \".*.*\"\n) )","v":0},{"$f":"IF( $G506 <> \"\",\n     TRUNC( $H506 * $J506, 2 ),\n     SUMIFS( $L507:$L$520,\n              $B507:$B$520, $B506 & \".*\",\n              $B507:$B$520, \"<>\" & $B506 & \".*.*\"\n     ) )","v":0}]
[null,"15.4.3",null,null,"PLANTA - SIBIPIRUNA (CAESALPINIA PELTOPHOROIDES), FORNECIMENTO E PLANTIO","SERV","UNID.",null,null,0,{"$f":"IF( $G507 <> \"\",\nTRUNC( $H507 * $I507, 2 ),\nSUMIFS( $K508:$K$520,\n          $B508:$B$520, $B507 & \".*\",\n          $B508:$B$520, \"<>\" & $B507 & \".*.*\"\n) )","v":0},{"$f":"IF( $G507 <> \"\",\n     TRUNC( $H507 * $J507, 2 ),\n     SUMIFS( $L508:$L$520,\n              $B508:$B$520, $B507 & \".*\",\n              $B508:$B$520, \"<>\" & $B507 & \".*.*\"\n     ) )","v":0}]
[null,"15.4.4",null,null,"LIXEIRA DUPLA, COM CAPACIDADE VOLUMETRICA DE 60L*, FABRICADA EM TUBO DE ACO CARBONO, CESTOS EM CHAPA DE ACO E PINTURA NO PROCESSO ELETROSTATICO - PARA ACADEMIA AO AR LIVRE / ACADEMIA DA TERCEIRA IDADE - ATI","FORN","UNID.",null,null,0,{"$f":"IF( $G508 <> \"\",\nTRUNC( $H508 * $I508, 2 ),\nSUMIFS( $K509:$K$520,\n          $B509:$B$520, $B508 & \".*\",\n          $B509:$B$520, \"<>\" & $B508 & \".*.*\"\n) )","v":0},{"$f":"IF( $G508 <> \"\",\n     TRUNC( $H508 * $J508, 2 ),\n     SUMIFS( $L509:$L$520,\n              $B509:$B$520, $B508 & \".*\",\n              $B509:$B$520, \"<>\" & $B508 & \".*.*\"\n     ) )","v":0}]
[null,"15.5",null,null,"SINALIZAÇÃO",{"$nulls":4},"",{"$f":"IF( $G509 <> \"\",\nTRUNC( $H509 * $I509, 2 ),\nSUMIFS( $K510:$K$520,\n          $B510:$B$520, $B509 & \".*\",\n          $B510:$B$520, \"<>\" & $B509 & \".*.*\"\n) )","v":0},{"$f":"IF( $G509 <> \"\",\n     TRUNC( $H509 * $J509, 2 ),\n     SUMIFS( $L510:$L$520,\n              $B510:$B$520, $B509 & \".*\",\n              $B510:$B$520, \"<>\" & $B509 & \".*.*\"\n     ) )","v":0}]
[null,"15.5.1",null,null,"PINTURA DE FAIXA DE PEDESTRE OU ZEBRADA TINTA RETRORREFLETIVA A BASE DE RESINA ACRÍLICA COM MICROESFERAS DE VIDRO, E = 30 CM, APLICAÇÃO MANUAL. AF_05/2021","SERV","M²",null,null,0,{"$f":"IF( $G510 <> \"\",\nTRUNC( $H510 * $I510, 2 ),\nSUMIFS( $K511:$K$520,\n          $B511:$B$520, $B510 & \".*\",\n          $B511:$B$520, \"<>\" & $B510 & \".*.*\"\n) )","v":0},{"$f":"IF( $G510 <> \"\",\n     TRUNC( $H510 * $J510, 2 ),\n     SUMIFS( $L511:$L$520,\n              $B511:$B$520, $B510 & \".*\",\n              $B511:$B$520, \"<>\" & $B510 & \".*.*\"\n     ) )","v":0}]
[null,"15.5.2",null,null,"PINTURA DE DEMARCAÇÃO DE VAGA COM TINTA EPÓXI, E = 10 CM, APLICAÇÃO MANUAL. AF_05/2021","SERV","M",null,null,0,{"$f":"IF( $G511 <> \"\",\nTRUNC( $H511 * $I511, 2 ),\nSUMIFS( $K512:$K$520,\n          $B512:$B$520, $B511 & \".*\",\n          $B512:$B$520, \"<>\" & $B511 & \".*.*\"\n) )","v":0},{"$f":"IF( $G511 <> \"\",\n     TRUNC( $H511 * $J511, 2 ),\n     SUMIFS( $L512:$L$520,\n              $B512:$B$520, $B511 & \".*\",\n              $B512:$B$520, \"<>\" & $B511 & \".*.*\"\n     ) )","v":0}]
[null,"15.5.3",null,null,"PINTURA DE SÍMBOLOS E TEXTOS COM TINTA ACRÍLICA, DEMARCAÇÃO COM FITA ADESIVA E APLICAÇÃO COM ROLO. AF_05/2021","SERV","M²",null,null,0,{"$f":"IF( $G512 <> \"\",\nTRUNC( $H512 * $I512, 2 ),\nSUMIFS( $K513:$K$520,\n          $B513:$B$520, $B512 & \".*\",\n          $B513:$B$520, \"<>\" & $B512 & \".*.*\"\n) )","v":0},{"$f":"IF( $G512 <> \"\",\n     TRUNC( $H512 * $J512, 2 ),\n     SUMIFS( $L513:$L$520,\n              $B513:$B$520, $B512 & \".*\",\n              $B513:$B$520, \"<>\" & $B512 & \".*.*\"\n     ) )","v":0}]
[null,"15.5.4",null,null,"PINTURA DE MEIO-FIO COM TINTA BRANCA A BASE DE CAL (CAIAÇÃO). AF_05/2021","SERV","M",null,null,0,{"$f":"IF( $G513 <> \"\",\nTRUNC( $H513 * $I513, 2 ),\nSUMIFS( $K514:$K$520,\n          $B514:$B$520, $B513 & \".*\",\n          $B514:$B$520, \"<>\" & $B513 & \".*.*\"\n) )","v":0},{"$f":"IF( $G513 <> \"\",\n     TRUNC( $H513 * $J513, 2 ),\n     SUMIFS( $L514:$L$520,\n              $B514:$B$520, $B513 & \".*\",\n              $B514:$B$520, \"<>\" & $B513 & \".*.*\"\n     ) )","v":0}]
[null,"15.5.5",null,null,"PLACA DE SINALIZAÇÃO, DIM.: 60 X 80 CM,  - \"ESTACIONAMENTO RESERVADO - DEFICIENTE/IDOSOS\", INCLUSO BARROTE PARA FIXAÇÃO - FORNECIMENTO E INSTALAÇÃO","SERV","UNID.",null,null,0,{"$f":"IF( $G514 <> \"\",\nTRUNC( $H514 * $I514, 2 ),\nSUMIFS( $K515:$K$520,\n          $B515:$B$520, $B514 & \".*\",\n          $B515:$B$520, \"<>\" & $B514 & \".*.*\"\n) )","v":0},{"$f":"IF( $G514 <> \"\",\n     TRUNC( $H514 * $J514, 2 ),\n     SUMIFS( $L515:$L$520,\n              $B515:$B$520, $B514 & \".*\",\n              $B515:$B$520, \"<>\" & $B514 & \".*.*\"\n     ) )","v":0}]
[null,"15.5.6",null,null,"SINALIZAÇÃO PERMANENTE, VERTICAL,  COM PLACA DE AÇO (50X80CM) COM POSTE DE MADEIRA 3,50M FIXADO COM BASE DE CONCRETO 40X40X50, INCLUSIVE MÃO DE OBRA - REV01/2023","SERV","UNID.",null,null,0,{"$f":"IF( $G515 <> \"\",\nTRUNC( $H515 * $I515, 2 ),\nSUMIFS( $K516:$K$520,\n          $B516:$B$520, $B515 & \".*\",\n          $B516:$B$520, \"<>\" & $B515 & \".*.*\"\n) )","v":0},{"$f":"IF( $G515 <> \"\",\n     TRUNC( $H515 * $J515, 2 ),\n     SUMIFS( $L516:$L$520,\n              $B516:$B$520, $B515 & \".*\",\n              $B516:$B$520, \"<>\" & $B515 & \".*.*\"\n     ) )","v":0}]
[null,16,null,null,"SERVIÇOS FINAIS",{"$nulls":4},"",{"$f":"IF( $G516 <> \"\",\nTRUNC( $H516 * $I516, 2 ),\nSUMIFS( $K517:$K$520,\n          $B517:$B$520, $B516 & \".*\",\n          $B517:$B$520, \"<>\" & $B516 & \".*.*\"\n) )","v":0},{"$f":"IF( $G516 <> \"\",\n     TRUNC( $H516 * $J516, 2 ),\n     SUMIFS( $L517:$L$520,\n              $B517:$B$520, $B516 & \".*\",\n              $B517:$B$520, \"<>\" & $B516 & \".*.*\"\n     ) )","v":0}]
[null,"16.1",null,null,"LIMPEZA GERAL","SERV","M²",null,null,0,{"$f":"IF( $G517 <> \"\",\nTRUNC( $H517 * $I517, 2 ),\nSUMIFS( $K518:$K$520,\n          $B518:$B$520, $B517 & \".*\",\n          $B518:$B$520, \"<>\" & $B517 & \".*.*\"\n) )","v":0},{"$f":"IF( $G517 <> \"\",\n     TRUNC( $H517 * $J517, 2 ),\n     SUMIFS( $L518:$L$520,\n              $B518:$B$520, $B517 & \".*\",\n              $B518:$B$520, \"<>\" & $B517 & \".*.*\"\n     ) )","v":0}]
[null,"16.2",null,null,"PLACA DE INAUGURAÇÃO DE OBRA EM ALUMÍNIO 0,50 X 0,70 M","SERV","UNID.",null,null,0,{"$f":"IF( $G518 <> \"\",\nTRUNC( $H518 * $I518, 2 ),\nSUMIFS( $K519:$K$520,\n          $B519:$B$520, $B518 & \".*\",\n          $B519:$B$520, \"<>\" & $B518 & \".*.*\"\n) )","v":0},{"$f":"IF( $G518 <> \"\",\n     TRUNC( $H518 * $J518, 2 ),\n     SUMIFS( $L519:$L$520,\n              $B519:$B$520, $B518 & \".*\",\n              $B519:$B$520, \"<>\" & $B518 & \".*.*\"\n     ) )","v":0}]
[null,"16.3",null,null,"LETRA EM AÇO INOX ESCOVADO/POLIDO 25 X 25CM - INSTALADO","SERV","UNID.",null,null,0,{"$f":"IF( $G519 <> \"\",\nTRUNC( $H519 * $I519, 2 ),\nSUMIFS( $K520:$K$520,\n          $B520:$B$520, $B519 & \".*\",\n          $B520:$B$520, \"<>\" & $B519 & \".*.*\"\n) )","v":0},{"$f":"IF( $G519 <> \"\",\n     TRUNC( $H519 * $J519, 2 ),\n     SUMIFS( $L520:$L$520,\n              $B520:$B$520, $B519 & \".*\",\n              $B520:$B$520, \"<>\" & $B519 & \".*.*\"\n     ) )","v":0}]
[{"$nulls":4},"TOTAL GERAL",{"$nulls":4},"",{"$f":"SUMIF( $B$9:$B$519, \"<>*.*\", $K$9:$K$519 )","v":0},{"$f":"SUMIF( $B$9:$B$519, \"<>*.*\", $L$9:$L$519 )","v":0}]

{"sheet":"Planilha1","index":1,"n_rows":111,"n_cols":5,"rows_kept":111,"cut":false,"hidden":false,"merged":[]}
["TIPO","ID","descrição","UNIDADES","obra"]
["SERV",10,"hectare","HA","sim"]
["FORN",11,"hora","HORA","sim"]
[null,13,"quilograma","KG","sim"]
[null,14,"quilômetro","KM","sim"]
[null,15,"quilômetro quadrado","KM²","sim"]
[null,18,"metro","M","sim"]
[null,19,"metro quadrado","M²","sim"]
[null,20,"metro cúbico","M³","sim"]
[null,29,"tonelada","TON","sim"]
[null,30,"unidade","UNID.","sim"]
[null,35,"litro","L","sim"]
[null,83,"Centímetro","CM","sim"]
[null,84,"Centímetro Quadrado","CM²","sim"]
[null,86,"Decímetro","DM","sim"]
[null,95,"Galão","GAL","sim"]
[null,98,"Grama","G","sim"]
[null,104,"Libra","LB","sim"]
[null,127,"Tonelada","T","sim"]
[null,128,"Decímetro Cúbico","DM³","sim"]
[null,129,"Metro Cúbico por Quilômetro","M³XKM","sim"]
[null,130,"Tonelada por Quilômetro","TXKM","sim"]
[null,131,"Mês","MÊS","sim"]
[null,1,"%","%","sim"]
[null,2,"alevino","ALEVINO"]
[null,3,"centro","CENTRO"]
[null,4,"colônia","COLÔNIA"]
[null,5,"conjunto","CONJUNTO"]
[null,6,"criança","CRIANÇA"]
[null,7,"cultivo","CULTIVO"]
[null,8,"empresa","EMPRESA"]
[null,9,"evento","EVENTO"]
[null,12,"jovem","JOVEM"]
[null,16,"quilowatt hora","KWH"]
[null,17,"lote","LOTE"]
[null,21,"pessoa","PESSOA"]
[null,22,"pólos","PÓLOS"]
[null,23,"produtor","PRODUTOR"]
[null,24,"projeto","PROJETO"]
[null,25,"R$","R$"]
[null,26,"região","REGIÃO"]
[null,27,"servidor","SERVIDOR"]
[null,28,"técnico","TÉCNICO"]
[null,31,"tonelada/hectare","TON/HA"]
[null,32,"milhão","MILHÃO"]
[null,33,"-","-"]
[null,34,"pescador","PESCADOR"]
[null,36,"técnico-dia","TD"]
[null,37,"homem-dia","HD"]
[null,38,"hora-máquina","HM"]
[null,39,"caixa","CX."]
[null,40,"pacote","PCT"]
[null,41,"quilograma/hectare","KG/HA"]
[null,42,"litro/hectare","L/HA"]
[null,43,"saco","SC"]
[null,44,"1000 metros cúbicos","1000M³"]
[null,45,"módulo implantado","MÓDULO"]
[null,69,"Ampére","A"]
[null,70,"Ampola","AMP."]
[null,71,"Balde","BAL."]
[null,72,"Barra","BARRA"]
[null,73,"Barril","BRL."]
[null,74,"Bisnaga","BISN."]
[null,75,"Bloco","BL."]
[null,76,"Bobina","BOB."]
[null,77,"Botijão","BOT."]
[null,78,"Caderno","CAD."]
[null,79,"Candela","CD"]
[null,80,"Cartela","CTL."]
[null,81,"Cavalo-Vapor","CV"]
[null,82,"Centena","CT"]
[null,85,"Coleção","CL"]
[null,87,"Decímetro Quadrado","D²"]
[null,88,"Dezena","DEZ."]
[null,89,"Diária Homem","DH"]
[null,90,"Dúzia","DZ"]
[null,91,"Estojo","EJ"]
[null,92,"Fardo","FD"]
[null,93,"Folha","FL."]
[null,94,"Frasco","FR"]
[null,96,"Garrafa","GARR."]
[null,97,"Gigahertz","GHZ"]
[null,99,"GROSSA","GR"]
[null,100,"Hertz","HZ"]
[null,101,"Jogo","JG"]
[null,102,"Kelvin","K"]
[null,103,"Lata","LT"]
[null,105,"Maço","MÇ"]
[null,106,"Milheiro","MIL"]
[null,107,"Miligrama","MG"]
[null,108,"Mililitro","ML"]
[null,109,"Milímetro","MM"]
[null,110,"Milímetro Quadrado","MM2"]
[null,111,"Par","PR"]
[null,112,"Peça","PÇ"]
[null,113,"Polegada","POL"]
[null,114,"Quilograma-força","KGF"]
[null,115,"Quilonewton","KN"]
[null,116,"Resma","RESMA"]
[null,117,"Rolo","RL"]
[null,118,"Tablete","TBL."]
[null,119,"Tubo","TB"]
[null,120,"Gigabytes","GB"]
[null,121,"usuário","USUÁRIO"]
[null,122,"lauda","LAUDA"]
[null,123,"Ponto de Função","PF"]
[null,124,"Unidade de Serviços Técnicos","UST"]
[null,125,"Litros por segundo","L/S"]
[null,126,"Ponto de Função Sustentado","PFS"]
[null,132,"Horsepower-hour","HPXH"]
[null,133,"Global","GL"]